SECTION 15410

PLUMBING FIXTURES

PART 1 GENERAL

1.1	SUMMARY

A.	Includes But Not Limited To

1.	Furnish and install plumbing fixtures as described in Contract Documents.

B.	Related Sections

1.	Section 15051 - General Mechanical Requirements

2.	Section 15141 - Potable Water Piping

PART 2 PRODUCTS

2.1	GENERAL

A.	Interior exposed pipe, valves, and fixture trim, including trim behind custom casework doors, shall be chrome plated.

B.	Do not use flexible water piping.

C.	Flow Control Fittings - Vandal proof type and fit faucet spout of fixture used. Flow shall be controlled as required by local codes.

2.2	MANUFACTURED UNITS

A.	Water Closets

1.	Standard Fixture -

a.	Maximum water usage of 1.6 gallons per flush.

b.	Approved Manufacturers And Models -

1)	American Standard - AFWALL 2257-103.

2)	Briggs

3)	Crane

4)	Eljer

5)	Kohler

2.	Handicap Accessible Fixture -

a.	18 inch maximum rim height.

b.	Maximum water usage of 1.6 gallons per flush.

c.	Approved Manufacturers And Models -

1)	American Standard - AFWALL 2257-103

2)	Briggs

3)	Crane

4)	Eljer

5)	Kohler

3.	Seats -

a.	Provide split front type with check hinge.

b.	Approved Manufacturers And Models for Standard And Handicap Accessible Fixtures -

1)	Bemis - 1655-C

2)	Beneke Corporation - Series 527 - CH

3)	Church - No. 9500-C

4)	Kohler - K-4666-C

5)	Olsonite - 95CC

6)	Spertzel - 50EWCH

4.	Flush Valve -

a.	Flow flow 1.6 gallon per flush maximum

b.	Proximity sensor type

c.	Approved Manufacturers -

1)	Coyne

2)	Sloan - 81111-LH

3)	Zurn

B.	Urinals

1.	Standard Fixture -

a.	Approved Manufacturers And Models -

1)	American Standard - Trimbrook 6561.017

2)	Crane - Embassy 7-150

3)	Eljer - Savon 161-1090

4)	Kohler - Freshman K-4985-T

2.	Handicap Fixture -

a.	Approved Manufacturers And Models -

1)	American Standard - Trimbrook 6561.017

2)	Crane - Embassy 7-150

3)	Eljer - Savon 161-1090

4)	Kohler - Freshman K-4989-T

3.	Carrier / Support -

a.	Approved Manufacturers -

1)	Josam

2)	Smith

3)	Wade

4)	Zurn

4.	Flush Valve -

a.	Low flow, 1.0 gal per flush maximum

b.	Proximity sensor type

c.	Approved Manufacturers And Models -

1)	Coyne - I 1452

2)	Sloan - 8186-LH

3)	Zurn - ZR-6003-XL

C.	Standard Lavatories

1.	Counter Top Fixture -

a.	Size 20 by 17 inches (maximum)

b.	Approved Manufacturers And Models -

1)	American Standard - Aqualyn 0476.028

2)	Crane - Sonnet 1-283-V

3)	Eljer - Laura 051-0124

4)	Kohler - Pennington K-2195

2.	Fittings -

a.	Faucet and Drain -

1)	Provide flow control fitting on each spout in place of aerator.

2)	Approved Manufacturers And Models -

a)	American Standard - 5402.102H

b)	Cambridge Brass - 21T341CB with metal HDL

c)	Chicago - 1802A with 327A

d)	Crane - C-1042 Citadel Dial-ese and C-1065-G drain

e)	Delta - 2502 RHP

f)	Eljer - 552-1680 with 803-0552 drain

g)	Kohler - K-7404-T with K-7715 strainer

h)	Sanitary Dash - R7304

I)	Speakman - SC-3073 complete with drain

j)	T S Brass - B-2971 with B-899 Drain

b.	Supply pipes with stops -

1.	Provide stuffing box and chrome plating.

2.	Approved Manufacturers And Models -

a)	Brass Craft - TCR 1912 A-CP

b)	Eastman - C 5M12-SBT-CP

c.	Trap -

1.	17 ga tube 'P' trap, chrome plated

2.	Approved Manufacturers -

a)	Dearborn

b)	Keeney Manufacturing

c)	Sanitary Dash

D.	Handicap Accessible Lavatories

1.	Self Supporting Fixture -

a.	Size - 20 by 18 inches

b.	Approved Manufacturers -

a)	American Standard - New Lucern 0355.012

b)	Crane - Norwich 1-412V

c)	Eljer - Delwyn 051-2644

d)	Kohler - Greenwich K-2032

2.	Fittings -

a.	Faucet And Drain -

1)	Approved Manufacturers And Models -

a)	American Standard - 5402.172H

b)	Cambridge Brass - 21T344

c)	Chicago - 1802A-E3-317

d)	Delta - 2523 HDF

e)	Eljer - 559-2200 with 803-0530 drain.

f)	Kohler - K-7404-5-A with K-13885 drain.

g)	Sanitary Dash - R7308

h)	Speakman SC-3075-ADA

I)	T & S Brass - B-890

b.	Supply pipes with stops -

1)	Provide stuffing box and chrome plating.

2)	Approved Manufacturers And Models -

a)	Brass Craft - TCR 1912 A-CP

b)	Eastman - C 5M12-SBT-CP

c.	Traps -

1)	17 ga tube 'P' trap, chrome plated

2)	Approved Manufacturers -

a)	Dearborn

b)	Keeney Manufacturing

c)	Sanitary Dash

3.	Safety Covers -

a.	Provide protection on hot water supply pipe and on trap.

b.	Approved Manufacturers And Models -

1)	Trapwrap by Brocar Products Inc

2)	Pro Wrap by McGuire Products

3)	Handy-Shield by Plumberex Specialty Products

4)	Handi Lav-Guard by TrueBro

E.	Service Sink

1.	Fixture -

a.	Floor Type, 28 by 28 inches with Stainless Steel rim guard.

b.	Approved Manufacturers And Models -

1)	American Standard - Florwell 7741.000

2)	Eljer - Custodial 242-0050

3)	Fiat - TSBC-1610

4)	Graning - 466-3

5)	Kohler - Whitby K-6710

6)	Stern-Williams - Cornaro SBC-1502

2.	Fittings -

a.	Supply -

1)	Mounting height of 42 inches

2)	Provide 48 inch hose and clamp unless spout is threaded.

3)	Approved Manufacturers And Models -

a)	American Standard - 8344.111 with threaded spout.

b)	Cambridge Brass - 28T2383CB

c)	Chicago - 897

d)	Crane - CH-8556

e)	Eljer - 749-1450

f)	Fiat - No. 830AA

g)	Grohe - 31512

h)	Kohler - K-8928

I)	Speakman - SC-5811 RCP-5H

j)	T & S Brass - B-665-BSTR

b.	Drain and Strainer -

1)	Approved Manufacturers And Models -

a)	American Standard - 7721.038

b)	Eljer - 803-0630

c)	Kohler - K-9146, 3 inch IPS.

c.	Trap - Cast iron

d.	Waste -

1)	Approved Manufacturers And Models -

a)	Crane - 8-5241

b)	Eljer - 803-0580

c)	Elkay - LK-99

d)	Just - JB-99

e)	Kohler - K-8801

f)	Sanitary Dash - SS250W

e.	Supply pipes with stops -

1)	Provide stuffing box and chrome plating.

2)	Approved Manufacturers And Models -

a)	Brass Craft - TCR 1912 A-CP

b)	Eastman - C5M12-SBT-CP

f.	Trap -

1)	17 gauge tube 'P' trap, chrome plated

2)	Approved Manufacturers -

a)	Dearborn

b)	Keeney Manufacturing

c)	Sanitary Dash

F.	Break Room Sink

1.	Fixture -

a.	Self-rimming, 18 gauge SS with satin finish.

b.	Size - 33 by 19 inches

c.	Approved Manufacturers And Models -	Approved Products

1)	Elkay - LR-3319

2)	Just - DL-1933-AGR

2.	Fittings -

a.	Supply -

1)	Provide flow control fitting on spout in place of aerator.

2)	Approved Manufacturers And Models -	Approved Products

a)	Cambridge Brass - W6600-8 less serrated spout

b)	Chicago - 350

c)	Eljer - 559-2851

d)	Kohler - K-7895

e)	Speakman - SC-7051-A less serrated spout

f)	T & S Brass - B-0305 with B-0199-02

b.	Supply with Stops -

1)	Provide stuffing box and chrome plating.

2)	Approved Manufacturers And Models -	Approved Products

a)	Brass Craft - TCR 1912 A-CP

b)	Eastman - C5M12-SBT-CP

c.	Waste -

1)	Approved Manufacturers And Models -	Approved Products

a)	Eljer - 803-0570

b)	Elkay - LK-18 C P

c)	Just - J-35-FS

d)	Kohler - K-8807

d.	Trap -

1)	17 gauge tube 'P' trap, chrome plated

2)	Approved Manufacturers -	Approved Products

a)	Dearborn

b)	Keeney Manufacturing

c)	Sanitary Dash

Disposers should not be installed in buildings served by a septic tank system. Disposer are generally authorized only for stake centers, if necessary.

e.	Disposer

1)	Heavy duty residential continuous feed type with adaptor assembly for direct sink mounting.

2)	Stainless steel grinding chamber.

3)	Motor - ½ HP, single phase, 115 volts, totally enclosed, fan cooled.

4)	Approved Models And Manufacturers -	Approved Products

a)	77 by In-Sink-Erator

b)	SS-5000 by Waste King

A work room sink is normally required on on CES Projects.

G.	Work Room Sink

1.	Fixture -

a.	Self-rimming, 18 gauge SS with satin finish.

b.	Size - 22 by 19 inches

c.	Approved Manufacturers And Models -	Approved Products

1)	Elkay - LR-2219

2)	Just - SL-1921-AGR

2.	Fittings -

a.	Supply -

1)	Provide flow control fitting on spout in place of aerator.

2)	Approved Manufacturers And Models -	Approved Products

a)	American Standard - 4146.130

b)	Cambridge Brass - 27T2443CB with 11 inch spout

c)	Chicago - 1888

d)	Crane - C-5011B

e)	Delta - 2100 HDF modified with 4381 handles

f)	Eljer - 718-1000

g)	Kohler - K-7761-T

h)	Sanitary Dash - R450W

i)	Speakman - SC-5763

j)	T S Brass - B-855/180F/B-199-1

b.	Supply with Stops -

1)	Provide stuffing box and chrome plating.

2)	Approved Manufacturers And Models -	Approved Products

a)	Brass Craft - TCR 1912 A-CP

b)	Eastman - C5M12-SBT-CP

c.	Waste -

1)	Approved Manufacturers And Models -	Approved Products

a)	Eljer - 803-0570

b)	Elkay - LK-18 C P

c)	Just - J-35-FS

d)	Kohler - K-8807

d.	Trap -

1)	17 gauge tube 'P' trap, chrome plated

2)	Approved Manufacturers -	Approved Products

a)	Dearborn

b)	Keeney Manufacturing

c)	Sanitary Dash

It is required that at least one sink in all new or remodelled Serving Areas be a three compartment sink. Additional one or two compartment sinks may be included if required by local code or the size of the Serving Area.

H.	Vegetable Preparation Sink

1.	Fixtures - See Section 11400

2.	Fittings -

a.	Provide flow control fittings on spouts in place of aerator.

b.	Supply -

1)	Three compartment sinks -

a)	Approved Manufacturers And Models -

(1)	American Standard - Two 6530.140

(2)	Cambridge Brass - Two 27T2443CB with 11 inch spout

(3)	Chicago - 1888

(4)	Crane - Two C-5011B

(5)	Delta - Two 2100 HDF modified with 4381 handles

(6)	Eljer - Two 718-1000

(7)	Kohler - Two K-7761-T

(8)	Speakman - SC-5763

(9)	T & S Brass - B-855 with 180F and B-199-1

3.	Disposer - See Section 11400

I.	Hand Lavatory - Vegetable Preparation Area

1.	Fixture - See Section 11400

2.	Fittings -

a.	Faucet And Drain -

1)	Approved Manufacturers And Models -

a)	American Standard - 5402.172H

b)	Cambridge Brass - 21T344

c)	Chicago - 1802A-E3-317

d)	Delta - 2523 HDF

e)	Eljer - 559-2200 with 803-0530 drain.

f)	Kohler - K-7404-5-A with K-13885 drain.

g)	Sanitary Dash - R7308

h)	Speakman SC-3075-ADA

I)	T & S Brass - B-890

b.	Supply pipes with stops -

1)	Provide stuffing box and chrome plating.

2)	Approved Manufacturers And Models -

a)	Brass Craft - TCR 1912 A-CP

b)	Eastman - C 5M12-SBT-CP

c.	Traps -

1)	17 ga tube 'P' trap, chrome plated

2)	Approved Manufacturers -

a)	Dearborn

b)	Keeney Manufacturing

c)	Sanitary Dash

3.	Safety Covers -

a.	Provide protection on hot water supply pipe and on trap.

b.	Approved Manufacturers And Models -

1)	Trapwrap by Brocar Products Inc

2)	Pro Wrap by McGuire Products

3)	Handy-Shield by Plumberex Specialty Products

4)	Handi Lav-Guard by TrueBro

J.	Handicap Accessible Bi-Level Fountain

1.	Include accessory fountain. Vandal proof operating bar on front and both sides. 7.8 GPH minimum of 50 deg F water with 90 deg F room temperature, 1/5 horsepower motor, 120 V, 60 Hz, single phase. Flexi-guard or chrome plated brass bubbler.

2.	Approved Manufacturers And Models -

a.	Elkay - Model EBFATL-8

b.	Halsey Taylor - HAC8BL-Q

c.	Haws - HWBFA8L

d.	Oasis - Model PLF8WMQSL

e.	Sunroc - NWCA-8-BL

K.	Wash Fountain

1.	All exposed materials are Type 304 stainless steel polished to a #4 finish, with hand control and pressure mixing valve

2.	Approved Manufacturer -

a.	Bradley - 2003/B, standard height/LSD/PBV.

L.	Emergency Eyewash

1.	Bradley S190210BF safety yellow, stainless steel eye/face washbowl with dual heads, cover, and push bar operation.

M.	Hydrants

1.	Provide with integral anti-siphon device.

2.	Approved Manufacturers And Models -

a.	Ancon - HY-420

b.	Josam - 71050

c.	Smith - 5609-QT

d.	Wade - W-8600

e.	Zurn - Z-1310

N.	Floor Drains

1.	FD-1 -

a.	Approved types with deep seal trap and chrome plated strainer.

b.	Approved Manufacturers And Models -

1)	Ancon - FD-100-C-A with MS-950-H trap

2)	Josam - 30000Z-5A with 88152 trap

3)	Smith - 2010-A with 7222 trap

4)	Wade - 1100 with 2450-T trap

5)	Zurn - 415 with Z 1000 trap

2.	FD-2 -

a.	Stainless steel drain, 10" top with removable perforated basket and drain cover, trap primer connection.

b.	Approved Manufacturers -	Approved Products

1)	Scherping Systems SF15850 (Winsted MN, 320-485-4401). No substitues.

O.	Cleanouts

1.	Furnish wall cleanouts with chrome wall cover and screw.

2.	Finish Floors -

a.	Approved Manufacturers And Models -

1)	Ancon - CO-200-R

2)	Josam - 56010

3)	J. R. Smith - 4023

4)	Wade - W-6000

5)	Zurn - Z-1402

3.	Resilient Flooring -

a.	Approved Manufacturers And Models -

1)	Ancon - CO-200-T

2)	Josam - 56010-12

3)	J. R. Smith - 4140

4)	Wade - W-6000-T

5)	Zurn - Z-1400-6

4.	Finished Wall -

a.	Approved Manufacturers And Models -

1)	Ancon - CO-460-RD

2)	Josam - 58790

3)	J. R. Smith - 4530

4)	Wade - W8460R

5)	Zurn - Z-1446

5.	Exposed Drain Lines -

a.	Approved Manufacturers And Models -

1)	Ancon - CO-460

2)	Josam - 58510

3)	J. R. Smith - 4510

4)	Wade - W8560A

5)	Zurn - Z-1440-4

6.	General Purpose -

a.	Approved Manufacturers And Models -

1)	Ancon - CO-450

2)	Josam - 58500

3)	J. R. Smith - 4400

4)	Wade - W8550A

5)	Zurn - Z-1440-4

PART 3 EXECUTION

3.1	INSTALLATION

A.	Install fixtures including traps and accessories with accessible stop or control valve in each hot and cold water branch supply line.

B.	Mounting

1.	Urinals -

a.	Standard - 20 inches from floor to bottom lip.

b.	Handicap Accessible - 17 inches from floor to bottom lip.

c.	Install urinals using carriers.

2.	Self Supporting Lavatories - Install using carriers.

3.	Drinking Fountains -

a.	Coordinate location of fountain with location and height of electrical outlet to ensure concealment of outlet by fountain.

b.	Handicap Accessible Bi-Level Fountain -

1)	Anchor bottom of fountain to wall.

2)	Top surfaces to be 40 and 32 inches above floor unless required otherwise by local code.

3)	Install 3/8 inch IPS union connection and Chicago No. 376 stop to building supply line.

4)	Install 1-1/4 inch IPS slip cast brass 'P' trap. Install trap so it is concealed.

C.	Make fixture floor connections with approved brand of cast iron floor flange, soldered or calked securely to waste pipe. Make joints between fixtures and floor flanges tight with approved fixture setting compound or gaskets. Calk between fixtures and wall and floor with white butyl rubber non-absorbent sealant. Point edges.

3.2	CLEANING

A.	Polish chrome finish at completion of Project.

END OF SECTION