SECTION 15440

CENTRAL VACUUM SYSTEM

PART 1 GENERAL

1.1	SUMMARY

A.	Includes But Not Limited To

1.	Furnish and install central vacuum system complete with necessary valves, connections, and accessories as described in Contract Documents.

PART 2 PRODUCTS

2.1	SYSTEM COMPONENTS

A.	Pipe:

1.	Schedule 10 tubing.

B.	Fittings:

1.	Schedule 10

C.	Connections

1.	Soldered

D.	Hose Outlets:

1.	2" mail thread-a VLV-90087 with recessed flange mount at 8" AFF. Equal to Spencer Turbine Company (Craig Van Hoover, 407-260-1030).

E.	Elbows:

1.	Schedule 10 long radius.

F.	The installer shall provide a shop drawing indicating piping routing, hanger location, valve outlets, etc. prior to fabrication.

H.	Central vacuum equal to Electrolux UL Listed two-stage bypass blower system, 12 amp, 120, single phase, 6" reusable foam filter, 115 cfm, 6 gallon tank capacity. Sales representative is Barbara Carroll 407-895-0355. No substitutions.

END OF SECTION