10558 Baton Rouge HVAC ProjectProject 10558 Baton Rouge HVAC Calculations
Mon May 15 18:56:29 CDT 2006 
There is no calculation for North & Shaded Glass 
There is no calculation for NorthEast and NorthWest Glass 
There is no calculation for East and West Glass 
The Btuh Gain for 200 SqFt of SouthEast and SouthWest Double Pane Glass = 20000 
There is no calculation for South Glass 
There is no calculation for SkyLights 
There is no calculation for Windows in Doors 

The Btuh Gain for 700 SqFt of Mason Above Grade R-5 Wall Number 1 = 2170 
The Btuh Gain for 216 SqFt of Mason Above Grade R-5 Wall Number 2 = 669.6 
There is no calculation for Wall Number 3 
There is no calculation for Wall Number 4 
The Btuh Gain for 1599 SqFt of Roof Only No Insulation; Ceiling Number 1 = 68757 


There is no calculation for Ceiling Number 2 
There is no calculation for Floor Number 1 
There is no calculation for Floor Number 2 
The Btuh Gain for 25 People = 250 
There is no calculation for Motor HP 
There is no calculation for Ducts Out of Conditioned Spaces 
The Btuh Gain for 1599 SqFt of Area Lighting in a Retail Store = 6396 
There is no calculation for Coffee Machines 
There is no calculation for Electric Food Warmers 
There is no calculation for Gas Food Warmers 
There is no calculation for Electric Fry Kettle 
There is no calculation for Gas Fry Kettle 
There is no calculation for Electric Griddle 
There is no calculation for Gas Griddle 
There is no calculation for Hair Dryer Helmets 
There is no calculation for 4-Slice Toaster 
There is no calculation for other appliances of known wattages 
There is no calculation for Outside Fresh Air #1 
There is no calculation for Outside Fresh Air #2 
There is no calculation for Outside Fresh Air #3 
The Cafeteria or Fast Food Outside Fresh Air #4 = 360 cfm 
The Btuh Gain for Outside Fresh Air #4 = 10800 
The Kitchen Outside Fresh Air #5 = 105 cfm
The Btuh Gain for Outside Fresh Air #5 = 3150 
There is no calculation for Outside Fresh Air #6

The Total Outside Fresh Air CFM = 465 
This is in accordance with International Mechanical Code 2003 
The Total BTUh Gain = 112192.6 
The Total Tons of HVAC needed = 9.34938333333333 