SECTION 08360

OVERHEAD DOORS

PART 1  GENERAL
1.01	SECTION INCLUDES
A.	Residential type overhead garage door at maintenance building.
1.02	RELATED SECTIONS
A.	Section 08710 - Finish Hardware:  Padlocks and Lock cylinders.
1.03	SUBMITTALS
A.	See Section 01300 - Administrative Requirements, for submittal procedures.
B.	Product Date: Provide manufacturer's standard details and catalog data. Provide installation instructions.
1.04	DELIVER, STORAGE, AND HANDLING
A.	Store products indoor and protect from moisture, construction traffic, and damage.
PART 2  PRODUCTS
2.01	MANUFACTURERS
A.	Raynor Garage Doors, P.O. Box 448, 1101 East River Road, Dixon, IL 61021-0448. Tel: (800) 472-9667
B.	Substitutions:  See Section 01600 - Product Requirements.
2.02	OVERHEAD GARAGE DOOR
A.	Product: 'Charleston'
1.	Size: 8'-0"W x 7'-0"H
2.	Panel Style:  Colonial
3.	Color: White
4.	Material: Heavy duty, hot dipped galvanized steel sections with an epoxy primer and baked on polyester finish.
5.	Guiding Mechanism: Galvanized steel track, steel wheels with ball bearing rollers.
6.	Weather protection: Roll formed tongue and groove meeting rails continuous bottom weather seal.
7.	Operation: Manual
8.	Hood: None
9.	Locking: Locking bracket mounted on guide angle.

PART 3  EXECUTION
3.01	EXAMINATION
A.	Verify that dimensions are correct and project conditions are suitable for installation. Do not proceed with installation until unsatisfactory conditions have been corrected.
3.02	INSTALLATION 
A.	Install door unit assembly in accordance with manufacturer's instructions.
B.	Ensure that units are installed plumb and true, free of warp or twist, and within tolerances specified by manufacturer for smooth operation.
3.03	ADJUSTING
A.	Clean units in accordance with manufacturer's instructions.
B.	Restore slight blemishes in finishes in accordance with manufacturer's instructions to match original finish. Remove and provide new units where repairs are not acceptable to the Architect.

END OF SECTION