Information and Instructions about this download file

=======================
File Description: Intel(r) Chipset Software Installation Utility
Version: 6.0.1.1002
Operating Systems: Microsoft(r) Windows(r) XP
Part Number: D00144-001-002
Date: 08/17/2004
=======================


Table of Contents
=======================
Overview
Identification
Installation
Removal 		
Troubleshooting
Reason for Update
Applicable Part Numbers
=======================


Overview

This document describes the steps necessary to install the Intel chipset driver for the computer models listed in the Applicable Part Numbers section below.


Identification

To confirm that this is the correct chipset driver for your desktop computer, follow these steps:

If the computer is turned off:

1.  Turn on the computer.  On your keyboard, repeatedly press the F1 key to enter the BIOS Setup Utility.

2.  In the BIOS Setup Utility, on the Main tab, look for the BIOS version line.  The version needs to be 
SE91510J.xxx.xxxx.xxxx.xxxx.xxxx or AG91510J.xxx.xxxx.xxxx.xxxx.xxxx or SR84510A.xxx.xxxx.xxxx.xxxx.xxxx or BF86510A.xxx.xxxx.xxxx.xxxx.xxxx or Pxx.865G (where x = variable characters, identifying the version of BIOS currently loaded).  The BIOS prefix SE91510J (Luxemburg, South Lake, and South Lake 2) or AG91510J (Augsburg) or SR84510A (Seabreeze) or BF86510A (Midway, Midway 2, Midway 2 Plus, Hazelton) or Pxx.865G (Profile 5.5) is constant and specifically identifies the correct motherboard.

3.  If the BIOS prefix is SE91510J or AG91510J or SR84510A or BF86510A or Pxx.865G, this is the correct driver for your computer.  Press the F10 key to exit the BIOS Setup Utility.

If the computer is turned on and in Windows:

1.  From the Start menu, click Shut Down.  In the Shut Down Windows dialog box, select Restart, and then click Yes.

2.  As soon as the computer restarts, on your keyboard, repeatedly press the F1 key to enter the BIOS Setup Utility.

3.  In the BIOS Setup Utility, on the Main tab, look for the BIOS version line.  The version needs to list SE91510J.xxx.xxxx.xxxx.xxxx.xxxx or AG91510J.xxx.xxxx.xxxx.xxxx.xxxx or SR84510A.xxx.xxxx.xxxx.xxxx.xxxx or BF86510A.xxx.xxxx.xxxx.xxxx.xxxx or Pxx.865G (where x = variable characters, identifying the version of BIOS currently loaded).  The BIOS prefix SE91510J (Luxemburg, South Lake, and South Lake 2) or AG91510J (Augsburg) or SR84510A (Seabreeze) or BF86510A (Midway, Midway 2, Midway 2 Plus, Hazelton) or Pxx.865G (Profile 5.5) is constant and specifically identifies the correct motherboard.

4.  If the BIOS prefix is SE91510J or AG91510J or SR84510A or BF86510A or Pxx.865G, this is the correct driver for your motherboard.  Press the F10 key to exit the BIOS Setup Utility.

Note:  The version of the chipset software currently installed can be identified by examining the following registry location:

Key name: \\HKEY_LOCAL_MACHINE\Software\Intel\InfInst
Value name: Version


Installation

1.  Download the file to the desktop.

2.  On the desktop, double-click the D00144-001-002.exe file.  The needed files are expanded to the C:\Cabs\D00144-001-002 folder.

3.  From the Start menu, click Run.

4.  In the Run dialog box, type: C:\Cabs\D00144-001-002\Setup.exe.  Click OK.

5.  In the Welcome dialog box, click Next.

6.  In the License Agreement dialog box, click Yes to agree to the license agreement.

7.  In the Readme Information dialog box, click Next.

8.  In the InstallShield Wizard Complete dialog box, click Yes, I want to restart my computer now, and then click Finish.


Removal

The Intel chipset driver provides proper functionality of multiple system devices, therefore removal instructions for the Intel chipset driver and related files are not provided. 


Troubleshooting

If you have difficulties installing this update, download the file again, and then verify that all instructions in this document are followed.


Reason for Update

This is the initial release of the driver.


Applicable Part Numbers

eMachines Systems:  

5398 - eMachines H5010
5025 - eMachines H3990

5016 - eMachines T3990
5291 - eMachines T3995
5275 - eMachines T3998
5017 - eMachines T4010
5452 - eMachines T3406
5644 - eMachines T3408
5393 - eMachines T5010
5474 - eMachines T5016
5475 - eMachines T5020
5570 - eMachines T5022
4655 - eMachines T3882
4656 - eMachines T3985
4371 - eMachines T5026