SECTION 08111

STANDARD STEEL DOORS

PART 1 GENERAL

SECTION INCLUDES

[Non-rated] [fire rated] [thermally insulated] [and] [acoustic] steel doors [and panels].

[Louvers.]

RELATED SECTIONS

Section [_____-_________]: Masonry mortar fill of metal frames.

Section 08112 - Standard Steel Frames.

Section 08211 - Flush Wood Doors.

Section 08212 - Stile and Rail Wood Doors.

Section 08712 - Door Hardware.

Section 08800 - Glazing: Glass for doors.

[Section [______-____________]: Louvers.]

Section 09900 - Painting: Field painting of doors.

REFERENCES

ANSI A117.1 - Specifications for Making Buildings and Facilities Accessible to and Usable by Physically Handicapped People.

ANSI/SDI-100 - Standard Steel Doors and Frames.

ASTM A525 - Steel Sheet, Zinc-Coated (Galvanized) by the Hot-Dip Process.

ASTM C236 - Test Method for Steady-State Thermal Performance of Building Assemblies by Means of a Guarded Hot-Box.

ASTM E152 - Methods of Fire Tests of Door Assemblies.

ASTM E413 - Classification for Determination of Sound Transmission Class.

Door Hardware Institute (DHI) - The Installation of Commercial Steel Doors and Steel Frames, Insulated Steel Doors in Wood Frames and Builder's Hardware.

NFPA 80 - Fire Doors and Windows.

NFPA 252 - Fire Tests for Door Assemblies.

UL 10B - Fire Tests of Door Assemblies.

SUBMITTALS

Submit under provisions of Section [01300.] [________.]

Shop Drawings: Indicate door elevations, internal reinforcement, closure method, and cut-outs for [glazing,] [louvers,] and finish.

Product Data: Indicate door configurations, location of cut-outs for hardware reinforcement.

Samples:	Submit [two] [_______] samples of door face metal, [____x____] inch ([____x____] mm) in size illustrating pre-finished door colors and surface texture.

Manufacturer's Installation Instructions: Indicate special installation instructions.

Manufacturer's Certificate: Certify that [Products] [________] meet or exceed [specified requirements] [________].

QUALITY ASSURANCE

Conform to requirements of ANSI/SDI-100 and ANSI A117.1.

Maintain [one copy] [[____] copies] of [each] document on site.

QUALIFICATIONS

Manufacturer: Company specializing in manufacturing the Products specified in this section with minimum [three] [_______] years [documented] experience.

REGULATORY REQUIREMENTS

Fire Rated Door [and Panel] Construction: Conform to [ASTM E152] [NFPA 252] [UL 10B].

Fire Rated Door Construction: Rate of rise of [250] [450] [650] F degrees ([138] [250] [361] C degrees) across door thickness.

Installed Door [and Panel] Assembly:	Conform to [NFPA 80] [_________] for fire rated class [as scheduled.] [as indicated.]

DELIVERY, STORAGE, AND HANDLING

Deliver, store, protect, and handle products to site under provisions of Section [01600.] [________.]

Protect doors with resilient packaging [sealed with heat shrunk plastic].

****** [OR] ******

Accept doors on site in manufacturer's packaging. Inspect for damage.

Break seal on-site to permit ventilation.

FIELD MEASUREMENTS

Verify that field measurements are as [indicated [on shop drawings].] [instructed by the manufacturer.]

COORDINATION

Coordinate work under provisions of Section [01039.] [________.]

Coordinate the work with door opening construction, door frame and door hardware installation.

PART 2 PRODUCTS

DOOR MANUFACTURERS

[__________________________________] Product [_________].

[__________________________________] Product [_________].

[__________________________________] Product [_________].

Substitutions: Under provisions of Section [01600.] [________.]

DOORS [AND PANELS]

Exterior Doors (Non-thermally Broken): SDI-100 Grade [I] [II] [III] Model [1] [2] [3] [4] [5].

Exterior Doors (Thermally Broken): SDI-100 Grade [I] [II] [III] Model [1] [2] [3] [4] [5].

Interior Doors (Non-rated): SDI-100 Grade [I] [II] [III] Model [1] [2] [3] [4] [5].

Interior Doors (Fire Rated):	SDI-100 Grade [I] [II] [III] Model [1] [2] [3] [4] [5].

Interior Doors (Acoustic): SDI-100 Grade [I] [II] [III] Model [1] [2] [3] [4] [5].

DOOR CONSTRUCTION

Face: Steel sheet in accordance with ANSI/SDI-100.

Core: [Cardboard honeycomb] [polyurethane] [polystyrene foam] [mineral fiberboard] [steel channel grid] [vertical steel stiffeners] [________].

Thermal Insulated Door: Total insulation R value of [____] (RSI value of [____]), measured in accordance with ASTM C236.

Sound Rated Door: STC of [____], measured in accordance with ASTM E413.

ACCESSORIES

Louvers: [________] manufactured by [____________].

Material and Finish:	[Roll formed [steel] [aluminum]] [Extruded aluminum]; [pre-painted finish to [_________] color [as selected].] [wipe coat of zinc.]

Louver Blade: Inverted [V] [Y] [slat] blade, [sight proof] [light proof]; [fire rated to [____] hours with fusible link design to [UL] [FM] requirements].

Louver Free Area: [____] percent.

Frame: [________] style with [surface] [tamper proof] fasteners.

****** [OR] ******

Louvers: Specified in Section [________].

Removeable Stops: Rolled [steel] [aluminum] [channel] [________] shape, [butted] [mitered] corners; prepared for countersink style [tamper proof] screws.

Primer: [Zinc chromate] [_________] type.

FABRICATION

Astragals for Double Doors: [Steel] [Aluminum], [Z] [T] shaped, specifically for double doors.

Fabricate doors with hardware reinforcement welded in place.

[Attach fire rated label to each door unit.]

Close top [and bottom] edge of exterior doors with [inverted steel channel] [flush end] closure. Seal joints watertight.

[Configure exterior doors with special profile to receive recessed weatherstripping.]

FINISH

Steel Sheet: Galvanized to ASTM A525 [G60.] [A60.]

Primer: [Air dried.] [Baked.]

[Factory Finish:	[Baked enamel] [Thermosetting epoxy] [_________] of [_________] color [as selected].]

PART 3 EXECUTION

EXAMINATION

Verify substrate conditions under provisions of Section [01039.] [________.]

Verify that opening sizes and tolerances are acceptable.

INSTALLATION

Install doors in accordance with ANSI/SDI-100 and DHI.

Coordinate installation of glass and glazing.

Install door louvers, plumb and level.

Coordinate installation of doors with installation of frames specified in Section [08112] [________] and hardware specified in Section [08710.] [________.]

[Touch-up factory finished doors.]

ERECTION TOLERANCES

Maximum Diagonal Distortion:	[1/16] [1/8] [____] inch ([1.5] [3] [____] mm) measured with straight edge, corner to corner.

ADJUSTING

Adjust work under provisions of Section [01700.] [________.]

Adjust door for smooth and balanced door movement.

SCHEDULE

Door Types A, B, and C: SDI Grade I Model 4, primed ready for site finish.

Door Types D and E: SDI Grade II Model 3, baked enamel finish.

END OF SECTION