SECTION 10800

TOILET AND BATH ACCESSORIES

PART	GENERAL

SECTION INCLUDES

Toilet, [bath,] [shower,] [and] [washroom] accessories.

Grab bars.

Attachment hardware.

PRODUCTS INSTALLED BUT NOT FURNISHED UNDER THIS SECTION

Section [______-____________]: Placement of concealed anchor devices.

Section [______-____________]: Placement of [backing plate reinforcement] [________].

RELATED SECTIONS

Section [____-___________]: [In wall framing and plates] [Above ceiling framing] for support of accessories.

Section 08800 - Glazing: Wall mirrors.

Section 09307 - Wall Tile: Ceramic accessories.

Section 10160 - Metal Toilet Compartments.

Section 10165 - Plastic Laminate Toilet Compartments.

Section 10171 - Solid Phenollc Toilet Compartments.

REFERENCES

ANSI A117.1 - Safety Standards for the Handicapped.

ASTM A123 - Zinc (Hot-Dip Galvanized) Coatings on Iron and Steel Products.

ASTM A167 - Stainless and Heat-Resisting Chromium-Nickel Steel Plate, Sheet, and Strip.

ASTM A269 - Seamless and Welded Austenitic Stainless Steel Tubing for General Service.

ASTM A366 - Steel, Carbon, Cold-Rolled Sheet, Commercial Quality.

ASTM B456 - Electrodeposited Coatings of Copper Plus Nickel Plus Chromium and Nickel Plus Chromium.

NEMA LD-3 - High Pressure Decorative Laminates.

SUBMITTALS

Submit under provisions of Section [01300.] [________.]

Product Data: Provide data on accessories describing size, finish, details of function, attachment methods.

Samples: Submit [two] [_______] samples of each component, illustrating color and finish.

Manufacturer's Installation Instructions: Indicate special procedures, perimeter conditions requiring special attention, and [________].

REGULATORY REQUIREMENTS

Conform to [ANSI A117.1] [___________] code for access for the handicapped.

FIELD MEASUREMENTS

Verify that field measurements are as [indicated [on product data].] [instructed by the manufacturer.]

COORDINATION

Coordinate work under provisions of Section [01039.] [________.]

Coordinate the work with the placement of [internal wall reinforcement] [and] [reinforcement of toilet partitions] to receive anchor attachments.

PART	PRODUCTS

MANUFACTURERS

[__________________________________] Product [_________].

Other acceptable manufacturers offering equivalent products.

[______________________________] Product [_________].

[______________________________] Product [_________].

[______________________________] Product [_________].

Substitutions: Under provisions of Section [01600.] [________.]

MATERIALS

Sheet Steel: [ASTM A366.] [________.]

Stainless Steel Sheet: ASTM A167, Type 304.

Tubing: ASTM [A269, stainless steel.] [________.]

Plastic Laminate: [NEMA LD-3,] [General Purpose] [Special Purpose] [Fire Rated] Type; [0.125] [____] inch ([3.2] [____] mm) thick, [________] finish, [________] color, [________] pattern.

Adhesive: [Two component epoxy type] [Contact type], waterproof.

Fasteners, Screws, and Bolts: Hot dip galvanized, [tamper-proof,] [and] [security type].

Expansion Shields: Fiber, lead, or rubber as recommended by accessory manufacturer for component and substrate.

Primer: [________].

FABRICATION

Weld and grind joints of fabricated components, smooth.

Form exposed surfaces from single sheet of stock, free of joints. Form surfaces flat without distortion. Maintain surfaces without scratches or dents.

Fabricate grab bars of tubing, free of visible joints, return to wall with end attachment flanges. Form bar with [____] inches ([____] mm) clear of wall surface. [Knurl grip surfaces.]

Shop assemble components and package complete with anchors and fittings.

Provide steel anchor plates, adapters, and anchor components for installation.

KEYING

Supply [________] keys for each accessory to Owner.

[Master key] [Key] all accessories.

FINISHES

Galvanizing: ASTM A123 to [1.25] [____] oz/sq yd ([380] [____]g/sq m). Galvanize ferrous metal and fastening devices.

Shop Primed Ferrous Metals: Pretreat and clean, spray apply one coat primer and bake.

Enamel: Pretreat to clean condition, apply one coat primer and minimum two coats [epoxy] [electrostatic] baked enamel.

Chrome/Nickel Plating: ASTM B456, Type [SC 2] [____] [satin] [polished] finish.

Stainless Steel: [No. 4 satin luster] [Polished] [________] finish.

Back paint components where contact is made with building finishes to prevent electrolysis.

PART	EXECUTION

EXAMINATION

Verify site conditions under provisions of Section [01039.] [________.]

Verify that site conditions are ready to receive work and dimensions are as [indicated on shop drawings.] [instructed by the manufacturer.]

Verify exact location of accessories for installation.

PREPARATION

Deliver inserts and rough-in frames to site for timely installation.

Provide templates and rough-in measurements as required.

INSTALLATION

Install accessories in accordance with manufacturers' instructions [and ANSI A117.1].

Install plumb and level, securely and rigidly anchored to substrate.

SCHEDULE

ITEM	MODEL #	FINISH

Toilet Tissue Dispenser	1234	White enamel

Paper Towel Dispenser	4321	White enamel

Paper Towel Disposal	5678	Stainless Steel

Napkin Dispenser	8765	Polished Chrome

Napkin Disposal	1299	Stainless Steel

Soap Dispenser	9912	Satin Chrome

Grab Bars	1111	Satin Chrome

END OF SECTION