SECTION 12692

FLOOR MATS

PART 1 GENERAL

SECTION INCLUDES

[Nylon pile carpet] [Link] [Cocoa] [Chenille] mats[.] [with custom design inlay.]

[Surface] [Recess] positioned.

PRODUCTS FURNISHED BUT NOT INSTALLED UNDER THIS SECTION

Section [_____ - __________:] Installation of mat frame for recessing in floor.

RELATED SECTIONS

Section [_____ - __________:] Floor depression formed without frame.

Section [_____ - __________:] Floor finish terminating edge to form floor depression.

Section [_____ - __________:] Aluminum grid floor grilles, recessed.

SUBMITTALS

Submit shop drawings under provisions of Section [01300.] [01340.]

Submit shop drawings indicating dimensions][,][.] [special crest inlay design][,][.] [and] [_____________________.]

Submit product data under provisions of Section [01300.] [01340.]

Submit product data indicating mat characteristics, component dimensions[,][.] [recessed frame and details,] [and] [_______________.]

Submit samples under provisions of Section [01300.] [01340.]

Submit [two] [_____] samples [_____ x _____] inches ([_____ x _____] mm) in size illustrating pattern, color, finish, edging [and] [_______________________.]

OPERATION AND MAINTENANCE DATA

Submit maintenance data under provisions of Section [01700.] [01730.]

Include cleaning instructions, stain removal procedures, [and] [_________________________.]

PART 2 PRODUCTS

MANUFACTURERS

[___________________________] Product [__________.]

[___________________________] Product [__________.]

[___________________________] Product [__________.]

Substitutions: Under provisions of Section [01600.] [01630.]

MATERIALS

Carpet Mat: Cut nylon pile permanently bonded to [vinyl] [rubber] backing; [_____] inch ([_____] mm) wide x [_____] inch ([_____] mm) long with one inch (25 mm) [black] [_______________] matching [vinyl] [rubber] border on all edges; [_______________] color[.] [as selected.]

Link Mats: Extruded [vinyl] [rubber] links fastened with 11 gage (2.90 mm) galvanized spring steel wire; overall size [_____] inch ([_____] mm) wide x [_____] inch ([_____] mm) long, 1/2 inch (13 mm) thick; [square] [bevelled] nosing; [black] [_______________] color[.] [with pattern.] [as selected.]

Rubber Mat: [1/4] [3/8] [1/2] [_____] inch ([6] [10] [13] [_____] mm) thick; [_____] inch ([_____] mm) wide x [_____] inch ([_____] mm) long; [corrugated] [pyramid] [__________] surface [texture;] [pattern;] [square] [bevelled] edges; [_______________] color[.] [as selected.]

Cocoa Mat: Woven jute backing with [vegetable] [__________] hair strand pile, interlocking woven edging, [_____ x _____] inch ([_____ x _____] mm) size x [_____] inch ([_____] mm) thick; [_______________] color[.] [as selected.]

Chenille Mat: Recycled rubber mat with woven [__________] surface fiber, [_______________] color[.] [as selected.]

PART 3 EXECUTION

EXAMINATION

Verify that floor openings are ready to receive work.

Verify field measurements are as [shown on [shop drawings.]

[Drawings.]] [instructed by the manufacturer.]

Beginning of installation means acceptance of existing conditions.

PREPARATION

Verify size of floor recess before [cutting] [fabricating] mats.

[Vacuum clean floor recess.]

INSTALLATION

Install mats [in floor recess flush with finish floor] after final cleaning of finish flooring.

TOLERANCES

Maximum Gap Allowed Between Recessed Frame and Mat: [1/4] [_____] inch ([6] [_____] mm).

SCHEDULE

Location	Mat_Type	Inches_(mm)	Color

Main Entry	Link	60 x 84 (1525 x 2130)	Pink

Rear Entry	Carpet	48 x 48 (1200 x 1200)	Brown

Receiving	Cocoa	36 x 36 (900 x 900)	Tan

END OF SECTION