| UNIT 3: INSTALLATION - LESSON 1: BASIC INSTALLATION ELEMENTS Before attempting to install the KX-TAW848 Advanced Hybrid Wired/Wireless System, be sure to read the important safety instructions located in the Installation Manual on pages 4-7 and 10-12. Installation methods and techniques can vary based upon several factors, including but not limited to, installation location, wiring availability, installer's preferences, local electrical ordinances, etc. The basic elements of any installation include the Central Office lines, backboard or Main Distribution Frame (MDF), AC power and protection, grounding, and station cabling. Recommended tools for a typical installation include: #1 Flathead screwdriver #2 Flathead screwdriver #1 Phillips head screwdriver #2 Phillips head screwdriver 66 Type Terminal Impact Tool Modular Crimping-Tool Cutting Pliers Wire Striping Tool Telephone Test Set Electric Drill with Bit Set A personal computer that meets the following requirements will be required to install the KX-TAW848 Maintenance Console Software. Operating System • Microsoft ® Windows ® 98 SE, Windows Me, Windows 2000, or Windows XP. Windows is a registered trademark of Microsoft Corporation. Hardware • CPU: Intel ® Pentium ® 133 MHz or better microprocessor • RAM: at least 64 megabytes (MB) of free RAM (128 MB recommended) • HDD: at least 100 MB of hard disc space Pentium is a registered trademark of Intel. Read Section 2 of the KX-TAW848 Installation Manual