| UNIT 4: PROGRAMMING - LESSON 3: SYSTEM PROGRAMMING BY PC Installing the KX-TAW848 Maintenance Console Software Read pages 101 through 113 of the KX-TAW848 Installation Manual Before the KX-TAW848 Maintenance Console Software (provided with each Main Unit) can be used, it must be installed on a personal computer with the following minimum requirements: Compatible PC Operating System Microsoft ® Windows ® 98 SE Windows Me Windows 2000 (must be grouped either an “Administrator” or “Power User”). Windows XP (must be grouped either an “Administrator” or “Power User”). Windows is a registered trademark of Microsoft Corporation PC Hardware minimum CPU – Pentium 133 MHZ or better microprocessor RAM – 64MB of free RAM (128 Recommended) HDD – at least 100MB of hard disc Available USB or serial port Pentium is a registered trademark of Intel. Use the procedure below to install the KX-TAW848 Maintenance Console onto the personal computer you will use to program the system: Copy the KX-TDA Maintenance Console setup file from the provided media to your PC. Double click the setup file icon on your PC to execute the installation. Follow the instructions of the wizard. (Use default selections of wizard when possible.) When the installation wizard is run for the first time, you will be asked if you want to install the USB Driver and USB Device for the KX-TAW848. You must choose yes to install this driver on PC’s that will use the USB port to connect to the Main Unit. The drivers are installed to the PC Desktop by default. After the USB Device is installed on your PC, the USB Drivers on your PC Desktop are no longer used and may be deleted.