| UNIT 6: MULTI-CELL WIRELESS - LESSON 3: INSTALLATION & PROGRAMMING Cell Stations Now that you have completed the Site Survey, it is time to install the KX-TAW848 and the Cell Stations. Refer back to the Unit 3 for basic installation instructions. Cell Stations are installed in the same way that the proprietary telephones are installed. But Cell Stations must be connected to Hybrid Line Card (HLC4) ports of the KX-TAW848. A Hybrid Line Card is pre-installed in the Main Unit. Cell Stations can be connected to any unused HLC4 ports. An expansion HLC4 card can also be installed in a Type A Free Slot and Cell Stations can be connected to these ports as well. Remember that the KX-TAW848 can support up to 4 Cell Stations. Cell Stations should be installed on the wall and should be at least 2 meters or 6.6 feet above the floor with antennas in the upright position. Once the Cell Stations have been installed, the KX-TAW848 will automatically recognize that the device connected to the HLC4 is a Cell Station. Notice in the 1. Configuration-5.Extension Port programming screen shows the Telephone Type for port 04 is a CS. Additional information about the status of the Cell Stations can be viewed by going to Utility CS Information screen. Click here to see an example of how to use the Maintenance Console to view the Utility CS Information Screen