| UNIT 2: HARDWARE & CONFIGURATION - LESSON 1: OPTIONAL SERVICE CARDS Remote Slot
MODEL # | DESCRIPTION | MAX # PER SYSTEM | SLOT TYPE
KX-TAW84896 | Remote Card (RMT) | 1 | Remote
| Modem card for remote maintenance and programming. V90 support. A maximum of 1 card can be installed per system.
Daughterboard
MODEL # | DESCRIPTION | MAX # PER SYSTEM | SLOT TYPE
KX-TAW84893 | 4-Port Caller ID Card (CID4) | 2 | Mounts on KX-TAW84880
| Allows Caller ID information to appear on the proprietary display telephones, and can be printed as part of the Station Message Detail Report. Supports Caller ID signal type FSK/FSK (with Call Waiting Caller ID)/DTMF. Mounts directly on a KX-TAW84880 central office line card. A maximum of 2 cards can be installed per system.