| UNIT 4: PROGRAMMING - LESSON 3: SYSTEM PROGRAMMING BY PC Starting the KX-TAW848 Maintenance Console Software Now that the software has been installed, it is time to connect to the KX-TAW848 Main Unit. The KX-TAW848 Maintenance Console Software can connect to the Main Unit using either a serial or USB cable. If a serial cable is used, it must have a DB9 female connector on one end, and the other end must be the correct size and gender for the serial port on your computer. In addition to the serial cable, a null modem adapter is required. Null modem adapters configure the serial cable to provide communication between the Main Unit and the computer. Click here for more information KX-TAW848 PC with 9-pin RS232 KX-TAW848 PC with 25-pin RS232 In this lesson we will be using a USB cable to connect the PC with the Main Unit since this is the fastest method of programming available. Begin by connecting the USB cable between the USB port of the KX-TAW848 and the USB port of the computer. When the installation wizard was run, it placed an icon for the KX-TAW848 Maintenance Console Software on the desktop. Follow the procedure in the following demonstration to startup the Maintenance Console Software. View the Maintenance Console software demonstration