| UNIT 3: INSTALLATION - LESSON 2: INSTALLING OPTIONAL SERVICE CARDS Installing a KX-TAW84896 The final card that we will install is the KX-TAW84896 Remote Card. This card allows the Main Unit to be programmed from a remote location using the KX-TAW848 Maintenance Console Software and an analog modem. Locate the Remote Card Slot on the upper left of the main PCB. Holding the KX-TAW84896 by the edge of the card, carefully place the card into the remote card slot. Make sure to insert the card between the guide rails and push until it locks into the slot. This completes the Installing Optional Service Cards Lesson. If any additional cards needed to be installed in the Type A, Type B or Option Slots, they would be installed in the same way described in this lesson. After all the optional service cards have been installed, the front cover must be closed and secured. Holding the cover on both sides, carefully swing the cover closed and secure it with the 3 screws.