| UNIT 1: OVERVIEW - LESSON 2: GENERAL DESCRIPTION The KX-TAW848 is an Advanced Hybrid Wired/Wireless System that has an initial configuration of four loop start Central Office (CO) lines, and four hybrid station ports. The system has the ability to expand to a maximum configuration of eight CO lines and forty-eight extensions. The forty-eight extensions can be comprised of up to twenty-four KX-T7700 series proprietary telephones and twenty-four wireless handset extensions. The maximum number of wired extensions will be affected by the number KX-T0141 Cell Stations that are installed since each Cell Station requires a Hybrid Line Card (HLC) port. The system also supports single line telephones and four doorphone/openers. System expansion is accomplished by installing optional expansion cards into the Main Unit. Other optional peripherals such as external paging speakers, a music on hold source, and a Station Message Detail Recording (SMDR) device can also be connected.
Proprietary Devices Supported |
Display Telephones KX-T7736 & KX-T7736-B (B indicates black model) • Backlit 3-Line Display Speakerphone • Lighted Keypad for dialing • 12 Flexible CO buttons • 12 Programmable Feature (PF) buttons |
KX-T7731 & KX-T7731-B • Backlit 1-Line Display Speakerphone • Lighted Keypad for dialing • 12 Flexible CO buttons • 12 Programmable Feature (PF) buttons |
Non-Display Telephones KX-T7720 & KX-T7720-B • Standard Speakerphone • 12 Flexible CO buttons • 12 Programmable Feature (PF) buttons |
KX-T7750 & KX-T7750-B • Basic Monitor Telephone • 12 Flexible CO buttons • 12 Programmable Feature (PF) buttons |
Consoles KX-T7740 & KX-T7740-B • Direct Station Selector (DSS) and Busy Lamp Field (BLF) • 32 DSS/BLF buttons • 16 PF buttons |