SECTION 07710

MANUFACTURED ROOF SPECIALTIES

PART 1 GENERAL

SECTION INCLUDES

[Copings] [Facias] [Gravel stops] [Vents.]

Roof [control] [expansion] joint covers.

Roof membrane vents.

PRODUCTS FURNISHED BUT NOT INSTALLED UNDER THIS SECTION

Section [______-____________]: Placement of [anchors] [frames] [________].

RELATED SECTIONS

Section [______-____________]:	Concrete roof deck.

Section [______-____________]: Metal deck perimeter stops.

Section [______-____________]: Wood deck [and wood curbs].

Section [______-____________]: Roof system and base flashings.

Section [07620 - Sheet Metal Flashing and Trim] [______-____________]: Metal flashings.

Section 07631 - Gutters and Downspouts.

REFERENCES

ASTM D2822 - Asphalt Roof Cement.

NRCA (National Roofing Contractors Association) - Roofing and Waterproofing Manual.

SMACNA - Architectural Sheet Metal Manual.

SUBMITTALS

Submit under provisions of Section [01300.] [________.]

Shop Drawings: Indicate configuration and dimension of components, adjacent construction, required clearances and tolerances, and other affected work.

Product Data: Provide data on shape of components, materials and finishes, anchor types and locations.

Samples:	Submit [two] [_______] samples, [____x____] inch ([____x____] mm) in size illustrating component shape, finish, and color.

Manufacturer's Installation Instructions: Indicate special procedures and perimeter conditions requiring special attention.

QUALITY ASSURANCE

Perform Work in accordance with [SMACNA] [NRCA] details.

Maintain [one copy] [[____] copies] of [each] document on site.

PART 2 PRODUCTS

MANUFACTURERS

[__________________________________] Product [_________].

[__________________________________] Product [_________].

[__________________________________] Product [_________].

Substitutions: Under provisions of Section [01600.] [________.]

COMPONENTS

[Copings] [and] [Gravel Stops]: [Extruded] [Formed] aluminum, [____] inch ([____] mm) thick, shaped [as indicated] [________], including special supports spaced at [____] inches ([____] mm) oc. Include cover plates to conceal and weather seal joints and attachment flanges.

[Control] [and] [Expansion] Joint Covers: Composite construction of [____] inch ([____] mm) wide flexible [butyl] [neoprene] [________] flashing [with closed cell [urethane] [________] foam backing,] each edge seamed to [aluminum] [copper] [pre-coated steel] [________] sheet metal flanges, designed for nominal joint width of [1] [2] [____] inch ([25] [50] [____] mm). Include special formed corners, tees, intersections, [and wall flashings,] each sealed watertight.

Roof Vents: [Formed [aluminum] [copper] [________] sheet metal] [plastic], [____] [inch] [gage] ([____] mm) thick, of watertight construction to permit construction below roof membrane to breathe; with attachment flanges [____] inch ([____] mm) wide, [________] manufactured by [____________].

Attic Vents:	[Dome] [Linear] type of [aluminum,] [[galvanized] [pre-coated] [________] sheet metal,] [____] inch ([____] mm) thick, formed to permit installation with [shingle] [________] roofing and shed water. Fabricate with [____] sq in ([____] sq mm) minimum free area of ventilation.

ACCESSORIES

Sealant:	[Same as specified in Section [07900] [________], Type [________].] [________.]

****** [OR] ******

Sealant:	[Manufacturer's standard type suitable for use with installation of system;[ [non-staining] [skinning] [non-skinning], [non-shrinking] [and] [non-sagging]; [ultra-violet and ozone resistant]; [________] color [as selected].

Roofing Cement: [Same as specified in Section [________], Type [________].] [________.]

****** [OR] ******

Roofing Cement: ASTM D2822, Type [I] [II], cutback asphalt type.

FINISHES

Aluminum: [________] finish [as selected].

****** [OR] ******

Pre-coated Steel: [________] color [as selected].

PART 3 EXECUTION

EXAMINATION

Verify that deck, curbs, roof membrane, base flashing, and other items affecting work of this Section are in place and positioned correctly.

INSTALLATION

Install components in accordance with manufacturer's instructions.

Conform to [SMACNA - Architectural Sheet Metal Manual] [NRCA - Waterproofing Manual] drawing details as noted:

[________] - [____________________________].

Coordinate installation of components of this section with installation of roofing membrane and base flashings.

Coordinate installation of sealants and roofing cement with work of this section to ensure water tightness.

Coordinate installation of flashing flanges into [reglets] [________].

SCHEDULES

Main Roof: Roof vents, Model xxx, formed pre-coated steel of "Horizon Blue"; roofing joint covers of extruded aluminum clear anodized Model www.

Penthouse Roof: Roof vents, Model yyy, formed aluminum, Stucco Embossed; control joint Model zzz, mill finish aluminum flanges, neoprene flexible flashing.

END OF SECTION