SECTION 08130

STAINLESS STEEL DOORS AND FRAMES

PART 1 GENERAL

SECTION INCLUDES

Stainless steel fabricated [non-rated] [and] [fire rated] steel frames, doors [, panels] [and] [louvers].

[Shop installed hardware.]

[Schedule at end of Section.]

PRODUCTS INSTALLED BUT NOT FURNISHED UNDER THIS SECTION

Section 08712 - Door Hardware: Hardware items provided to this Section for shop installation.

RELATED SECTIONS

Section [______-____________]: Preparation of adjacent work to receive frame anchors.

[Section [______-____________]: Mortar fill of metal frames.]

Section 08111 - Standard Steel Doors and Frames.

Section 08114 - Custom Steel Doors and Frames.

Section 08210 - Wood Doors.

Section 08213 - Plastic Faced Wood Doors.

Section 08214 - Steel Faced Wood Doors.

Section 08215 - Prefinished Wood Doors.

Section 08712 - Door Hardware: Templates for hardware items provided to this Section.

[Section 08712 - Door Hardware: Hardware and installation.]

Section 08721 - Automatic Door Equipment.

Section 08800 - Glazing.

[Section [______-____________]: Louvers.]

REFERENCES

ANSI A117.1 - Specifications for Making Buildings and Facilities Accessible to and Usable by Physically Handicapped People.

ANSI/NFPA 80 - Fire Doors and Windows.

ANSI/ASTM A167 - Stainless Quality Steel.

ASTM A480 - Flat-Rolled Stainless and Heat Resisting Steel Plate, Sheet, and Strip.

ASTM A525 - Steel Sheet, Zinc-Coated (Galvanized) by the Hot Dip Process, General Requirements.

ASTM C236 - Test Method for Steady-State Thermal Performance of Building Assemblies by Means of a Guarded Hot Box.

ASTM E152 - Methods of Fire Tests of Door Assemblies.

ASTM E413 - Classification for Determination of Sound Transmission Class.

BHMA - Builders' Hardware Manufacturers Association.

DHI - Door Hardware Institute: The Installation of Commercial Steel Doors and Steel Frames, Insulated Steel Doors in Wood Frames and Builder's Hardware.

NAAMM CHM-1-74 - Recommended Architectural Specifications for Custom Hollow Metal Doors and Frames.

NAAMM Hollow Metal Technical and Design Manual - Section 6: Installation of Doors and Frames.

NAAMM Hollow Metal Technical and Design Manual - Section 8: Fire Rated Doors and Frames.

NFPA 252 - Fire Tests of Door Assemblies.

SDI 100 - Steel Door Institute Recommended Specifications - Standard Steel Doors and Frames.

UL 10B - Fire Tests of Door Assemblies.

PERFORMANCE REQUIREMENTS

Acoustic Rating for Door and Frame Assembly:	ASTM E413, minimum STC [35] [____].

Thermal Rating for Exterior Doors: ASTM C236 to an R value of [____] (RSI value of [____]).

SUBMITTALS

Submit under provisions of Section [01300] [________].

Shop Drawings: Indicate dimensions, frame configuration, anchor spacings, door elevations [, stile and rail reinforcement] closure method [, and cut outs for [glazing] [louvers]].

Product Data: Provide general construction, connections, anchor types, location of cutouts for hardware, and hardware reinforcement.

Manufacturer's Installation Instructions: Indicate special procedures and protection to finishes required.

Manufacturer's Certificate: Certify that [products] [________] meet or exceed [specified requirements] [___________________].

QUALITY ASSURANCE

Perform Work in accordance with [SDI 100] [NAAMM CHM-1-74] and as supplemented in this Section.

Maintain [one] [____] copy of [each] document on site.

QUALIFICATIONS

Fabricator: Company specializing in performing the work of this Section with minimum [__________] years [documented] experience.

REGULATORY REQUIREMENTS

Conform to [applicable] [_________] code for fire rated [frames] [, doors] [and] [panels].

****** [OR] ******

Fire Rated [Frames] [, Doors] [and Panel] Construction: Conform to [ASTM E152] [UL 10B] [NFPA 252] [NAAMM Section 8].

Installed frame and door assembly to conform to [ANSI/NFPA 80] [NAAMM Section 6] [_________] for fire rated class indicated.

Provide certificate of compliance from [authority having jurisdiction] [________________] indicating approval of door and frame assemblies.

DELIVERY, STORAGE, AND HANDLING

Deliver, store, protect and handle products to site under provisions of Section [01600] [________].

Protect [doors] [and] [frames] with resilient packaging [sealed with heat shrunk plastic].

Puncture seal on delivery to permit ventilation.

FIELD MEASUREMENTS

Verify that field measurements are as [indicated [on shop drawings]] [instructed by the manufacturer].

COORDINATION

Coordinate work under provisions of Section [01039] [________].

Coordinate the Work with door hardware sizes, types and installation.

PART 2 PRODUCTS

FABRICATORS

[__________________________________].

[__________________________________].

[__________________________________].

Substitutions: Under provisions of Section [01600] [________].

MATERIALS

Frame, Door [and Panel] Material: [ASTM A480, Type [304] [316]] [ANSI/ASTM A167]; rollable temper stainless steel, [No. 4.] [______] finish.

Frame Reinforcement:	ASTM A525 sheet steel with [1.25] [____] oz/sq ft ([380] [____] gm/sq m) galvanized coating.

Door [and Panel] Core Construction: [[Polyurethane] [Polystyrene] insulation] [Steel channel grid]; [vertical [galvanized] [stainless] steel stiffeners].

Door [and Panel] Core Filler: [Mineral fiberboard] [Batt insulation] [________________].

Door [and Panel] Acoustic Material: [Glass fiber insulation] [_________].

FRAME AND DOOR COMPONENTS

Exterior Frames:	[Thermally broken with interior portion of frame insulated]; [with [channel] [snap-in] glazing stops]:

Thickness:	[14] [____] gage ([1.8] [____] mm).

Profile:	[____] inches ([____] mm) wide by [____] inch ([____] mm) deep.

Interior Frames:	[With [channel] [snap-in] glazing stops]:

Thickness:	[16] [____] gage ([1.5] [____] mm).

Profile:	[____] inches ([____] mm) wide by [____] inch ([____] mm) deep.

Doors:	[With [channel] [snap-in] glazing stops]:

Face Sheet Thickness:	[18] [____] gage ([1.2] [____] mm).

Total Door Thickness:	[2] [1-3/4] [____] inch ([51] [44] [____] mm).

Vertical Stiles:	[____] inch ([____] mm) wide.

Top Rail:	[____] inch ([____] mm) wide.

Bottom Rail:	[____] inch ([____] mm).

Hardware Reinforcement: Size, thickness, and location in accordance with [NAAMM CHM-1-74] [_________].

ACCESSORIES

Louvers:	Roll formed stainless steel, [inverted [V] [Y]] [slat] blade, [sight proof] [light proof] [___________] design; [85] [____] percent free area; [flush] [________] style frame with [flush] [surface] [tamperproof] fasteners.

Jamb Anchors: [T-strap] [Stirrup and strap] [Wire] [________________] type.

Silencers:	Resilient rubber.

Glazing Stops: Rolled stainless steel [channel] [bevel] [________] shape, [square] [mitered] corners; prepared for countersunk [tamperproof] screws.

Shim Space Insulation: [Loose glass fiber] [Foamed-in-place] [________] type.

FRAME COATING

Coating: [Fibered asphalt emulsion] [________________].

FABRICATION

Fabricate frames as a [shop welded with mitered corners] [knocked down for field assembly] unit. [Grind welds smooth and apply filler, sand smooth.]

Size units to allow for installation clearances, shim spacing at perimeter of installed assembly, and deflection of lintel.

Provide flush hairline [and weatherproof] joints and connections. Match components for continuity of line and design.

Mullions for Double Doors:	[Fixed] [Removable] type.

****** [OR] ******

Astragals for Double Doors: Metal [Z] [T] [flat] shaped astragals for doors.

Fabricate frames and doors with hardware reinforcement plates welded in place. Locate reinforcement in accordance with templates provided.

[Weld mortar guard boxes to frames protecting hardware reinforcement.]

[Reinforce frames wider than 48 inches (1 200 mm) with roll formed steel channels fitted tightly into frame head, flush with top.]

[Terminate door stops [6] [____] inches ([150] [____] mm) above finished floor on interior frames. Cut stop at [45] [90] degree angle and close.]

Prepare frame for silencers; three silencers for strike jamb at single doors [and on mullions of double doors]; two single silencers on frame head at each leaf for double doors [; and four silencers for strike jamb at dutch doors].

[Attach fire rated label to each rated unit.]

Close top edge of exterior door with inverted [stainless steel] [extruded vinyl] channel closure. Seal joints weather tight.

[Configure exterior frames with special profile to receive weatherstripping.]

[Fabricate frames for masonry wall coursing with [4] [____] inch ([100] [____] mm) head member.]

[Place glazing stops on [secure] [________] side of glazed frames.]

HARDWARE INSTALLATION

Install hardware in accordance with manufacturer's instructions [and requirements of [NAAMM Sections 6 and 8] [ANSI/NFPA 80] [BHMA] [DHI] [________]].

Use the templates provided by hardware item manufacturer.

Mounting heights for hardware from finished floor to center line of hardware item:

Locksets:	[____] inches ([____] mm).

Push/Pulls:	[____] inches ([____] mm).

Dead Locks:	[____] inches ([____] mm).

Panic Devices:	[____] inches ([____] mm).

[Conform to ANSI A117.1 for positioning requirements for the handicapped.]

FINISH

Paint inside of frame profile with coating to a thickness of [1/16] [_________] inch ([1.5] [_________] mm).

PART 3 EXECUTION

EXAMINATION

Verify wall openings under provisions of Section [01039] [________].

Verify that wall opening sizes and tolerances are acceptable.

INSTALLATION

Install frames in accordance with [NAAMM Section 6] [manufacturer's instructions].

Install assemblies plumb, level and free of warp or twist.

Coordinate with [masonry] [gypsum board] [_________] wall construction for anchor placement.

Install shim space insulation around perimeter of frame assemblies to maintain continuity of thermal barrier.

[Coordinate installation of glass and glazing.]

[Coordinate installation of door hardware and weatherstripping.]

Install [louvers] [________].

Install roll formed steel reinforcement channels between two abutting frames. Anchor to structure and floor.

ERECTION TOLERANCES

Maximum Diagonal Distortion of Installed Door or Frame: [1/16] [1/8] inch ([1.5] [3] [_________] mm) measured with straight edge, corner to corner.

ADJUSTING

Adjust work under provisions of Section [01700] [________].

Shim [hinges] [pivots] with steel plate shims when required.

Adjust hardware for smooth and balanced door movement.

CLEANING

Clean work under provisions of [01700] [________].

Remove temporary protection and clean assemblies just prior to acceptance.

PROTECTION OF FINISHED WORK

Protect finished work under provisions of Section [01500] [________].

Do not permit traffic near finished work without protection to finishes.

SCHEDULES

Opening #	Size (inches)	Elevation	Fire Rated

101	36 x 80	A	3/4 hour

102	30 x 80	D	None

103	72 x 80	B	1-1/2 hour

END OF SECTION