SECTION 08212

STILE AND RAIL WOOD DOORS

PART 1 GENERAL

SECTION INCLUDES

Wood doors, stile and rail design.

[Wood] [and] [glass] panels.

RELATED SECTIONS

Section [______-____________]:	Wood door frames.

Section 08112 - Standard Steel Frames:	Steel door frames.

****** [OR] ******

Section 08115 - Custom Steel Frames: Steel door frames.

Section 08211 - Flush Wood Doors.

Section 08712 - Door Hardware.

Section 08800 - Glazing.

Section 09900 - Painting: Site finishing doors.

REFERENCES

ANSI/HPMA HP - Hardwood and Decorative Plywood.

AWI - Quality Standards of the Architectural Woodwork Institute.

SUBMITTALS

Submit under provisions of Section [01300.] [________.]

Shop Drawings: Illustrate door opening criteria, elevations, sizes, types, swings, [undercuts required,] [special beveling,] identify cutouts for [glazing] [and] [________].

Product Data: Indicate stile and rail core materials and construction; veneer species, type and characteristics; [factory machining criteria,] [factory finishing criteria,] [and] [________].

Samples:	Submit [two] [_______] samples of door construction, [____x____] inch ([____x____] mm) in size cut from [top] [bottom] corner of door.

Samples:	Submit [two] [_______] samples of door veneer, [____x____] inch ([____x____] mm) in size illustrating wood grain, stain color, and sheen.

Manufacturer's Installation Instructions: Indicate

special installation instructions.

QUALITY ASSURANCE

Perform work in accordance with AWI Quality Standard Section 1400, [Premium] [Custom] Grade.

[Finish doors in accordance with AWI Quality Standard Section 1500 [, grades identified in schedule].

Maintain [one copy] [[____] copies] of [each] document on site.

QUALIFICATIONS

Manufacturer: Company specializing in manufacturing the Products specified in this section with minimum [three] [_______] years [documented] experience.

DELIVERY, STORAGE, AND HANDLING

Deliver, store, protect, and handle products to site under provisions of Section [01600.] [________.]

Package, deliver and store doors in accordance with [AWI Section 1300.] [________.]

****** [OR] ******

Accept doors on site in manufacturer's packaging. Inspect for damage.

****** [OR] ******

Protect doors with resilient packaging [sealed with heat shrunk plastic]. Do not store in damp or wet areas; or in areas where sunlight might bleach veneer. Seal top and bottom edges if stored more than one week. Break seal on-site to permit ventilation.

FIELD MEASUREMENTS

Verify that field measurements are as [indicated [on shop drawings].] [instructed by the manufacturer.]

COORDINATION

Coordinate work under provisions of Section [01039.] [________.]

Coordinate the work with door opening construction, door frame and door hardware installation.

WARRANTY

Provide warranty under provisions of Section [01700] [________] to the following term:

Exterior Doors: [Five (5)] [________] years.

Interior Doors: [Two (2)] [________] years.

****** [OR] ******

Life of Installation: Interior [and exterior] doors.

Include coverage for [delamination of veneer,] [warping beyond specified installation tolerances,] [defective materials,] [telegraphing core construction,] [________].

PART 2 PRODUCTS

MANUFACTURERS

[__________________________________] Product [_________].

[__________________________________] Product [_________].

[__________________________________] Product [_________].

Substitutions: Under provisions of Section [01600.] [________.]

DOOR TYPES

Exterior Doors: [1-3/4] [2-1/4] inches ([44] [57] mm) thick; [solid lumber] [veneer and lumber stile and rail] construction; [mortise and tenon] [doweled and glued] joints.

Interior Doors: [1-3/4] [1-3/8] [____] inches ([44] [35] [____] mm) thick; [solid lumber] [veneer and lumber stile and rail] construction; [mortise and tenon] [doweled and glued] joints.

[Transom Panels: [To match door] [_________].]

DOOR FACING

Veneer Facing (Exterior Doors): [AWI [Premium] [Custom] [Economy] quality] species wood, [rotary cut] [plain sliced] [quarter sliced] [rift cut] [_________], with [book] [pair] [end] [________] matched grain, for [paint] [transparent] finish.

Veneer Facing (Interior Doors): [AWI [Premium] [Custom] [Economy] quality] species wood, [rotary cut] [plain sliced] [quarter sliced] [rift cut] [_________], with [book] [pair] [end] [________] matched grain, for [paint] [transparent] finish.

ADHESIVE

Adhesive: Type [I - waterproof] [II - water resistant].

ACCESSORIES

Molding:	Wood, of same species as door facing, [________] shape, [butted] [mitered] corners; prepared for countersink style [tamper proof] screws.

FABRICATION

Fabricate doors in accordance with AWI Quality Standards requirements.

Astragals for Double Doors: [Wood] [Steel] [Aluminum], [____] shaped, overlapping and recessed [at face edge] [at mid-door thickness], specifically for double doors.

Vertical Exposed Edge of Stiles:	[Of same species as veneer facing.] [[Hardwood] [Softwood] for [paint] [transparent] finish.] [Plastic laminate same as door facing.]

Fit door edge trim to edge of stiles after applying veneer facing.

Bond edge banding to cores.

At exterior doors, provide aluminum flashing at the top and bottom rail for full thickness and width of door.

Factory machine doors for finish hardware in accordance with hardware requirements and dimensions. Do not machine for surface hardware.

Factory pre-fit doors for frame opening dimensions identified on shop drawings.

[Cut and configure exterior door edge to receive recessed weather stripping devices. Provide edge clearances in accordance with AWI 1600.]

FINISH

Factory finish doors in accordance with AWI Quality Standard Section 1500 to the following finish designations:

[Finish F3] [_________] Doors: System #3 -transparent, conversion varnish alkyd-urea, [Premium] [Custom] quality, [_________] sheen.

[Finish F4] [_________] Doors: System #4 -transparent vinyl catalyzed, [Premium] [Custom] quality, [_________] sheen.

[Finish F5] [_________] Doors: System #5 -transparent, penetrating oil synthetic, [Premium] [Custom] quality, [_________] sheen.

****** [OR] ******

Factory finish doors in accordance with [approved sample.] [________.]

PART 3 EXECUTION

EXAMINATION

Verify frame opening conditions under provisions of Section [01039.] [________.]

Verify that opening sizes and tolerances are acceptable.

Do not install doors in frame openings that are not plumb or are out-of-tolerance for size or alignment.

INSTALLATION

Install doors in accordance with manufacturer's instructions.

****** [OR] ******

Install doors in accordance with AWI Quality Standards requirements.

Trim door width by cutting equally on both jamb edges.

Trim door height by cutting bottom edges to a maximum of 3/4 inch (19 mm).

Pilot drill screw and bolt holes. [Use threaded through bolts for [half surface hinges.] [________.]

Machine cut for hardware. Core for handsets and cylinders.

Coordinate installation of doors with installation of frames specified in Section [08112] [08114] [________] and hardware specified in Section [08710.] [________.]

Coordinate installation of glass and glazing.

INSTALLATION TOLERANCES

Conform to AWI requirements for fit, clearance, and joint tolerances.

****** [OR] ******

Maximum Diagonal Distortion (Warp): [1/8] [____] inch ([3] [____] mm) measured with straight edge or taught string, corner to corner, over an imaginary 36 x 84 inch

surface area.

Maximum Vertical Distortion (Bow): [1/8] [____] inch ([3] [____] mm) measured with straight edge or taught string, top to bottom, over an imaginary 36 x 84 inch surface area.

Maximum Width Distortion (Cup): [1/8] [____] inch ([3] [____] mm) measured with straight edge or taught string, edge to edge, over an imaginary 36 x 84 inch surface area.

ADJUSTING

Adjust work under provisions of Section [01700.] [________.]

Adjust door for smooth and balanced door movement.

SCHEDULE

END OF SECTION