SECTION 08710

DOOR HARDWARE

PART 1 GENERAL

SECTION INCLUDES

Hardware for [wood] [hollow steel] [aluminum] [__________] doors.

Thresholds.

Weatherstripping, seals and door gaskets.

PRODUCTS FURNISHED BUT NOT INSTALLED UNDER THIS SECTION

Section [______-____________]: Furnish templates for frame preparation.

Section [______-____________]: Furnish templates for door preparation.

Section [______-____________]: Furnish lock cylinders for installation.

PRODUCTS INSTALLED BUT NOT FURNISHED UNDER THIS SECTION

Section [______-____________]: Hardware [and thresholds] supplied for [aluminum entrance doors.] [________.]

RELATED SECTIONS

Section [______-____________]:	Wood door frames.

Section [______-____________]:	Cabinet hardware.

Section 08111 - Standard Steel Doors.

Section 08112 - Standard Steel Frames.

Section 08114 - Custom Steel Doors.

Section 08115 - Custom Steel Frames.

Section 08331 - Overhead Coiling Doors: Lockable coiling doors.

Section 08341 - Overhead Coiling Grilles: Lockable coiling grilles.

Section 08391 - Aluminum Storm Doors and Frames:	Hardware for same [except cylinders].

Section 08410 - Aluminum Entrances and Storefronts: Hardware for same [except cylinders].

Section 08470 - Revolving Entrance Doors: Hardware for same [except cylinders].

Section 08741 - Automatic Door Equipment: Hardware for same [except cylinders].

Section 08920 - Glazed Aluminum Curtain Wall: Hardware for integral doors and frames [except lock cylinders].

Section 08971 - Suspended Glass:	Hardware for integral doors and frames [except lock cylinders].

Section 10441 - Plastic Signs.

Section [______-____________]: Power supply to electric hardware devices.

Section 16721 - Fire Alarm and Smoke Detection Systems: Electrical connection to [activate door closers,] [release magnetic holders,] [and] [________].

ALLOWANCES

Cash Allowance: Include under provisions of Section [01019.] [________.]

Allowance includes [purchase and delivery of door hardware. Installation is included in this section and is part of the Contract Sum/Price.] [purchase, delivery, and installation of door hardware.]

REFERENCES

ANSI A117.1 - Specifications for Making Buildings and Facilities Accessible to and Usable by Physically Handicapped People.

NFPA 80 - Fire Doors and Windows.

AWI - Architectural Woodwork Institute - Quality Standards.

NFPA 101 - Code for Safety to Life from Fire in Buildings and Structures.

NFPA 252 - Fire Tests of Door Assemblies.

UL 10B - Fire Tests of Door Assemblies.

UL 305 - Panic Hardware.

SUBMITTALS

Submit under provisions of Section [01300.] [________.]

Shop Drawings: Indicate locations and mounting heights of each type of hardware, [electrical characteristics and connection requirements,] [and] [________].

Submit manufacturer's parts lists, templates, [and] [________].

Samples:	Submit [1] [____] sample of [hinge,] [latchset,] [________,] illustrating style, color, and finish.

Samples:	[Will be incorporated into the Work.] [Will be returned to supplier.]

Manufacturer's Installation Instructions: Indicate special procedures, perimeter conditions requiring special attention, and [________].

PROJECT RECORD DOCUMENTS

Submit under provisions of Section [01700.] [________.]

Record actual locations of installed cylinders and their [master] [________] key code.

OPERATION AND MAINTENANCE DATA

Submit under provisions of Section [01700.] [________.]

Maintenance Data: Include data on operating hardware, lubrication requirements, and inspection procedures related to preventative maintenance.

QUALITY ASSURANCE

Perform work in accordance with the following requirements:

ANSI A117.1 - Specifications for Making Buildings and Facilities Accessible to and Usable by Physically Handicapped People.

NFPA 101.

ANSI A117.1.

NFPA 80.

NFPA 252.

QUALIFICATIONS

Manufacturer: Company specializing in manufacturing the Products specified in this section with minimum [three] [_______] years [documented] experience.

Hardware Supplier: Company specializing in supplying [commercial] [institutional] [________] door hardware [with [_____] years [documented] experience.] [approved by manufacturer.]

Hardware Supplier Personnel:	Employ [an Architectural Hardware Consultant (AHC)] [a qualified person] to assist in the work of this section.

REGULATORY REQUIREMENTS

Conform to [applicable] [________] code for requirements applicable to fire rated doors and frames.

Products Requiring Electrical Connection: Listed and classified by [Underwriters' Laboratories, Inc.,] [testing firm acceptable to the authority having jurisdiction] as suitable for the purpose specified and indicated.

PRE-INSTALLATION CONFERENCE

Convene [one] [_____] week prior to commencing work of this section, under provisions of Section [01039.] [________.]

DELIVERY, STORAGE, AND HANDLING

Deliver, store, protect and handle products to site under provisions of Section [01600.] [________.]

Package hardware items individually; label and identify each package with door opening code to match hardware schedule.

Deliver keys to [Owner] [________] by security shipment direct from hardware supplier.

COORDINATION

Coordinate work under provisions of Section [01039.] [________.]

Coordinate the work with other directly affected sections involving manufacture or fabrication of internal reinforcement for door hardware.

WARRANTY

Provide [five] [____] year warranty under provisions of Section [01700.] [________.]

Warranty: Include coverage for [door closers] [and] [________].

MAINTENANCE MATERIALS

Provide maintenance materials under provisions of [01700.] [________.]

Provide special wrenches and tools applicable to each different or special hardware component.

Provide maintenance tools and accessories supplied by hardware component manufacturer.

EXTRA MATERIALS

Furnish under provisions of Section [01700.] [________.]

Provide [ten] [_____] extra key lock cylinders for each [master] [_____] keyed group.

PART 2 PRODUCTS

SUPPLIERS

[__________________________________].

[__________________________________].

[__________________________________].

Substitutions: Under provisions of Section [01600.] [________.]

ACCEPTABLE MANUFACTURERS

Hinges: [________], [________], and [________].

Pivots: [________], [________], and [________].

Latch Sets: [________], [________], and [________].

Push/Pulls: [________], [________], and [________].

Cylinder Locks: [________], [________], and [________].

Mortise Locks:	[________], [________], and [________].

Electric Locks: [________], [________], and [________].

Exit Devices: [________], [________], and [________].

Closers: [________], [________], and [________].

Overhead Holders: [________], [________], and [________].

[Manual] [Automatic] Bolts: [________], [________], and

[________].

Gasketing:	[________], [________], and [________].

Sliding Door Hardware: [________], [________], and [________].

Bifolding Door Hardware:	[________], [________], and [________].

Protection Plates: [________], [________], and [________].

Substitutions: Under provisions of Section [01600.] [01630.]

KEYING

Door Locks: [Keyed in like-groups.] [Keyed differently.] [Master keyed.] [Grand master keyed.] [Great grand master keyed.] [________.] [Include [construction keying,] [control keying with removable core cylinders,] [and] [________]. [Key to existing keying system.]

Supply keys in the following quantities:

[____] master keys.

[____] grand master keys.

[____] great grand master keys.

[____] construction keys.

[____] control keys and [_____] extra cylinder cores.

[____] change keys for each [lock] [bitting].

ELECTRICAL CHARACTERISTICS AND COMPONENTS

Electrical Characteristics:

[12] [24] [____] volts, single phase, 60 Hz.

KEY CABINET

Cabinet Construction: Sheet [steel] [aluminum] [________] construction, piano hinged door with [________] type lock [master] [________] keyed to building system; [________] manufactured by [____________].

Cabinet Size: Size for project keys plus [10] [____] percent growth.

[Hooks for [_____] keys.]

Horizontal [metal] [plastic] strips for key hook labelling with clear plastic strip cover over labels.

Finish: [Baked enamel,] [[brushed] [________] finish,] [________] color [as selected].

FINISHES

Finishes: Identified in schedule at end of section.

PART 3 EXECUTION

EXAMINATION

Verify site conditions under provisions of Section [01039.] [________.]

Verify that doors and frames are ready to receive work and dimensions are as [indicated on shop drawings.] [instructed by the manufacturer.]

Verify that electric power is available to power operated devices and of the correct characteristics.

INSTALLATION

Install hardware in accordance with manufacturer's instructions.

Use templates provided by hardware item manufacturer.

Mounting heights for hardware from finished floor to center line of hardware item:

Locksets:	[____] inch ([____] mm).

Push/Pulls:	[____] inch ([____] mm).

Dead Locks:	[____] inch ([____] mm).

Exit Devices:	[____] inch ([____] mm).

FIELD QUALITY CONTROL

Field [inspection and] testing will be performed under provisions of Section [01400.] [________.]

Architectural Hardware Consultant to inspect installation and certify that hardware and installation has been furnished and installed in accordance with manufacturer's instructions [and as specified].

ADJUSTING

Adjust work under provisions of Section [01700.] [________.]

Adjust hardware for smooth operation.

PROTECTION OF FINISHED WORK

Protect finished Work under provisions of Section [01500.] [________.]

Do not permit adjacent work to damage hardware or finish.

SCHEDULES

END OF SECTION