SECTION 09815

HIGH BUILD GLAZED COATINGS

PART	GENERAL

SECTION INCLUDES

Preparation of substrate surfaces.

High build glazed coating.

RELATED SECTIONS

Section [______-____________]: Substrate wall surface.

Section 09900 - Painting.

REFERENCES

ASTM E84 - Surface Burning Characteristics of Building Materials.

FS TT-C-535 - Coating, Epoxy, Two-Component, for Interior Use on Metal, Wood, Wallboard, Painted Surfaces, Concrete and Masonry.

FS TT-C-542 - Coating, Polyurethane, Oil Free, Moisture Curing.

FS TT-C-555 - Coating, Textured (For Interior and Exterior Masonry Surfaces).

SSPC - Steel Structures Painting Council.

UL - Underwriter's Laboratories Inc., Fire Resistance Directory.

SUBMITTALS

Submit under provisions of Section [01300.] [________.]

Product Data: Provide data indicating coating materials [and] [________].

Submit [two] [_______] samples [____x____] inch ([____x____] mm) in size illustrating colors [available] for selection.

Manufacturer's Installation Instructions: Indicate special procedures, perimeter conditions requiring special attention, and [________].

Manufacturer's Certificate: Certify that [Products] [________] meet or exceed [specified requirements.] [________.]

MAINTENANCE DATA

Submit under provisions of Section [01700.] [________.]

Maintenance Data: Include maintenance and cleaning requirements for coatings, repair and patching techniques, and [________].

QUALITY ASSURANCE

Perform surface preparation work on primed or unfinished steel surfaces in accordance with SSPC [________].

Maintain [one copy] [[____] copies] of [each] document on site.

QUALIFICATIONS

Manufacturer: Company specializing in manufacturing the Products specified in this section with minimum [three] [_______] years [documented] experience.

Applicator: Company specializing in performing the work of this section [with minimum [__________] years [documented] experience] [approved by manufacturer].

REGULATORY REQUIREMENTS

Conform to [applicable] [___________] code for flame/smoke rating of [____/____] in accordance with [[UL] [____] requirements.] [ASTM E84.]

MOCKUP

Provide mockup of applied glazed coating under provisions of Section [01400.] [________.]

Provide [________] mockup, [____] feet ([____] m) long by [____] feet ([____] m) wide, illustrating coating, color, surface sheen, and [________].

Locate [where directed.] [________.]

Mockup may [not] remain as part of the Work.

ENVIRONMENTAL REQUIREMENTS

Do not install materials when temperature is below [55] [____] degrees F ([13] [____] degrees C) or above [90] [____] degrees F ([32] [____] degrees C).

Maintain this temperature range, 24 hours before, during, and [72] [____] hours after installation of coating.

Maximum Moisture Content of Surface: [14] [____] percent, negative alkalinity.

Provide lighting level of [80] [____] ft candles ([860] [____] lx) measured mid-height at substrate surface.

Restrict traffic from area where coating is being applied or is curing.

WARRANTY

Provide [five] [____] year warranty under provisions of Section [01700.] [________.]

Warranty: Include coverage for bond to substrate, degradation of chemical resistance and [________].

MAINTENANCE MATERIALS

Provide maintenance materials under provisions of [01700.] [________.]

Provide [1] [____] gallon ([4] [____] l) of each color [and of each type of coating] specified, for Owners maintenance use.

Label each container with manufacturer's name, product number, color number, and room names and numbers where used.

PART	PRODUCTS

MANUFACTURERS

[__________________________________] Product [_________].

[__________________________________] Product [_________].

[__________________________________] Product [_________].

Substitutions: Under provisions of Section [01600.] [________.]

MATERIALS

Coating [Type A]: [FS TT-C-535] two component epoxy, thermosetting type, [100] [90] [____] percent solids, [gloss] [semi-gloss] surface finish.

***** [OR] *****

Coating [Type B]: [FS TT-C-542] single component polyurethane, [gloss] [semi-gloss] surface finish.

***** [OR] *****

Coating [Type C]: Two component polyester epoxy type, [gloss] [semi-gloss] surface finish.

***** [OR] *****

Coating [Type D]: Two component epoxy emulsion type, [gloss] [semi-gloss] surface finish.

***** [OR] *****

Coating [Type E]: Inorganic, vinyl acrylic, moisture evaporating type; [gloss] [semi-gloss] [flat] surface finish.

Conform to the following criteria:

Chemical Group	Type	Result

Acid	[____]	[not affected] [________]

Alkali	[____]	[not affected] [________]

Oxidizing Agent	[____]	[not affected] [________]

Salt Solution	[____]	[not affected] [________]

Solvents	[____]	[not affected] [________]

Maximum Dry Heat Resistance: [____] degrees F ([____] degrees C).

Maximum Wet Heat Resistance: [____] degrees F ([____] degrees C).

Abrasion Resistance: [Excellent.] [Good.] [Fair.]

Scrubability: [Excellent.] [Good.] [Fair.]

Gloss and Color Retention: [Excellent.] [Good.] [Fair.]

ACCESSORIES

Primer [and Filler Base]: [As recommended by coating materials manufacturer for specific substrate surface.] [[________] type, [________] manufactured by [____________].]

Shellac: Pure, white type.

FINISH

Texture and Color: [Solid color] [Mottled] [Speckled] [Contrasting color flakes]; [________] color [as selected].

PART	EXECUTION

EXAMINATION

Verify substrate conditions under provisions of Section [01039.] [________.]

Verify that substrate surfaces are ready to receive work as instructed by the coating manufacturer.

Do not begin work until cementitious substrate has cured [28] [____] days minimum, and measured moisture content is not greater than [16] [____] percent. [Measure concrete surface for negative alkalinity with litmus paper test.]

****** [OR] ******

Do not begin work until wood substrate has dried to a maximum moisture content of [12] [____] percent].

[Verify masonry joints are struck flush.]

PREPARATION

Seal [indelible markings] [________] on substrate with shellac.

Clean surfaces of loose foreign matter.

Remove finish hardware, fixture covers, and accessories and store.

[Strip existing paint or coatings from surface.]

[Clean existing painted or sealed surfaces with mixture of trisodium phosphate and water to remove surface grease or foreign films.]

Prepare metal surfaces in accordance with SSPC SP [____].

Mask and protect adjacent surfaces and materials not receiving coating from over spray; repair damage.

PRIMER AND SURFACE SEALING

Patch [wood] [concrete] [________] substrate with filler to produce smooth, even surface.

Apply masonry filler to [concrete and] masonry substrate wall surface in accordance with manufacturer's instructions; to a minimum thickness of [30] [40] [____] mils ([0.8] [1] [____] mm).

Apply primer to [all] [________] surfaces.

APPLICATION

Apply coating in accordance with manufacturer's instructions.

Apply color base coat and [clear] [color] glaze overcoat to a total minimum cured thickness of [15] [____] mils ([0.4] [____] mm).

CLEANING

Clean work under provisions of [01700.] [________.]

Clean surfaces immediately of overspray, splatter, excess material, and [________].

After coating has cured, clean and replace finishing hardware, fixtures, and fittings previously removed.

PROTECTION OF FINISHED WORK

Protect finished Work under provisions of Section [01500.] [________.]

Protect elements surrounding the work of this Section from damage or disfiguration.

SCHEDULE

Corridor 108: Type B; gloss wainscot, 48 inches high, gloss; "Putrid Yellow" color.

Lab 202: Type A; semi-gloss, "Warm Green" color.

END OF SECTION