SECTION 10171

SOLID PHENOLIC TOILET COMPARTMENTS

PART	GENERAL

SECTION INCLUDES

Solid plastic toilet compartments, [floor mounted.] [head rail braced.] [ceiling hung.]

[Urinal] [Vestibule] screens; wall mounted with floor to ceiling [pilaster] [tube] brace.

[Shower cubicles.]

PRODUCTS INSTALLED BUT NOT FURNISHED UNDER THIS SECTION

Section [______-____________]: Placement of concealed supports.

RELATED SECTIONS

Section [______-____________]: [Framing and plates within walls] [Framing above ceiling] for partition panel support.

Section 10800 - Toilet and Bath Accessories.

REFERENCES

ANSI A117.1 - Safety Standards for the Handicapped.

ASTM A167 - Stainless and Heat-Resisting Chromium-Nickel Steel Plate, Sheet, and Strip.

NEMA LD-3 - High Pressure Decorative Laminates.

SUBMITTALS

Submit under provisions of Section [01300.] [________.]

Shop Drawings: Indicate partition plan, elevation views, dimensions, details of [wall,] [floor,] [and] [ceiling] supports, door swings.

Product Data: Provide data on panel construction, hardware, and accessories.

Samples: Submit [two] [_______] samples of partition panels, [____x____] inch ([____x____] mm) in size illustrating panel finish, color, and sheen.

Manufacturer's Installation Instructions: Indicate special procedures, perimeter conditions requiring special attention, and [________].

REGULATORY REQUIREMENTS

Conform to [ANSI A117.1] [___________] code for access for the handicapped.

FIELD MEASUREMENTS

Verify that field measurements are as [indicated [on shop drawings].] [instructed by the manufacturer.]

COORDINATION

Coordinate work under provisions of Section [01039.] [________.]

Coordinate the work with placement of support framing and anchors in [wall] [and] [ceiling].

PART	PRODUCTS

ACCEPTABLE MANUFACTURERS

[__________________________________] Product [_________].

[__________________________________] Product [_________].

[__________________________________] Product [_________].

Substitutions: Under provisions of Section [01600.] [________.]

MATERIALS

Solid Phenolic Panel: NEMA LD-3 solid phenolic core with melamine laminate veneer material.

ACCESSORIES

Pilaster Shoe: Formed [chromed steel with [polished] [satin] finish,] [ASTM A167 type 304 stainless steel with [No. 4] [____] finish,] [3] [____] inch ([175] [____] mm) high, with adjustable screw jack.

Head Rails: Hollow [stainless steel] [aluminum] tube, [1 x 1-5/8] [____] inch ([25 x 41] [____] mm) size, with [anti-grip strips and] cast socket wall brackets.

Attachments, Screws, and Bolts: Stainless steel; [tamper proof type,] heavy duty extruded aluminum brackets.

Through Bolts and Nuts: [Stainless steel] [________] with [tamper proof heads] [________].

Hardware: [Chrome plated non-ferrous cast metal:] [Stainless steel:]

Pivot hinges, gravity type, adjustable for door close positioning.

Nylon bearings.

Thumb turn door latch [with exterior emergency access feature].

Door strike and keeper with rubber bumper.

Coat hook with rubber bumper.

[Door pull for outswinging doors.]

FABRICATION

Fabricate partitions by forming solid phenolic with finished faces and edges. Finish edges convex.

Bevel corners and edges of cut-outs.

Doors and Panels:

Thickness: [1] [____] inch ([25] [____] mm)

Door Width: [24] [____] inch ([610] [____] mm)

Door Width for Handicapped Use: [36] [____] inch ([915] [______] mm) [, out-swinging].

Height: [58] [____] inch (1 473] [____] mm)

Thickness of Pilasters: [1-1/4] [____] inch ([32] [____] mm).

FINISHING

Plastic Laminate, Single Color: [________] color [as selected].

****** [OR] ******

Plastic Laminate, Two Colors: [________] color [as selected] for [doors] [________], [________] color [as selected] for [panels,] [pilasters,] [and] [________].

Stainless Steel Surfaces: [No. 4] [____] finish.

Exposed Steel Surfaces: [[Polished] [Satin] chrome plated] [________].

Aluminum: Anodized to [________] color [as selected].

Non-ferrous Surfaces: [Polished] [Satin] chrome plated.

PART	EXECUTION

EXAMINATION

Verify site conditions under provisions of Section [01039.] [________.]

Verify correct spacing of and between plumbing fixtures.

Verify correct location of built-in framing, anchorage, and bracing.

INSTALLATION

Install partitions secure, rigid, plumb, and level in accordance with manufacturer's instructions.

Maintain [3/8 to 1/2] [________] inch ([9 to 13] [________] mm) space between wall and panels and between wall and end pilasters.

Attached panel brackets securely to walls using anchor devices.

Attach panels and pilasters to brackets with [tamper proof] through bolts and nuts. [Locate head rail joints at pilaster center lines.]

Anchor urinal screen panels to walls with [two] [____] panel brackets and vertical upright consisting of [pilaster] [tubular head rail stock and sockets] anchored to floor and ceiling.

Provide adjustment for floor variations with screw jack through steel saddles integral with pilaster. Conceal floor fastenings with pilaster shoes.

Support pilasters from built-in framing using [two] [____] adjustable hanging studs providing vertical leveling. Conceal ceiling fastenings with pilaster shoe.

Equip each door with two hinges, one door latch, [one] [____] coat hook and bumper [; outswinging door with pull].

Install door strike and keeper with door bumper on each pilaster in alignment with door latch.

Field touch-up of scratches or damaged finish will not be permitted.

Replace damaged or scratched materials with new materials.

ERECTION TOLERANCES

Maximum Variation From True Position: [1/4] [____] inch ([6] [____] mm).

Maximum Variation From Plumb: [1/8] [____] inch ([3] [____] mm).

ADJUSTING

Adjust work under provisions of Section [01700.] [________.]

Adjust and align hardware to uniform clearance at vertical edge of doors, not exceeding 3/16 inch (5 mm).

Adjust hinges to position doors in [partial opening] [full closed] position when unlatched. [Return out swinging doors to closed position.]

Adjust adjacent components for consistency of line or plane.

SCHEDULES

Toilet Room 204: Three toilet stalls of floor mounted, head rail braced type; two urinal screens with pilaster bracing; two contrasting colors as selected.

Staff Washroom: One toilet stall of ceiling mounted type; single color as selected.

END OF SECTION