SECTION 11164

DOCK SEALS AND SHELTERS

PART 1 GENERAL

SECTION INCLUDES

Compression door seals.

Telescopic shelters with support framing.

PRODUCTS FURNISHED BUT NOT INSTALLED UNDER THIS SECTION

Section [______-____________]: Placement of seal and shelter frame into [________] wall construction.

RELATED SECTIONS

Section [______-____________]:	Anchor bolts.

Section [______-____________]:	Framed wall openings.

Section 11161 - Dock Levelers.

Section 11165 - Dock Bumpers.

SUBMITTALS

Submit under provisions of Section [01300.] [________.]

Shop Drawings: Indicate framed wall opening, dimensions and tolerances, adjacent construction and fittings required for anchorages, and anchor points.

Samples:	Submit [two] [_______] cuts of [seal] [shelter] covering material, [____x____] inch ([____x____] mm) in size illustrating color and finish.

Manufacturer's Installation Instructions: Indicate special requirements and [________].

OPERATION AND MAINTENANCE DATA

Submit under provisions of Section [01700.] [________.]

Operation Data: Provide operating instructions, identify unit limitations.

Maintenance Data: Provide unit maintenance information, lubrication cycles, spare parts manual.

FIELD MEASUREMENTS

Verify that field measurements are as [indicated [on shop drawings].] [instructed by the manufacturer.]

PART 2 PRODUCTS

MANUFACTURERS

[__________________________________] Product [_________].

[__________________________________] Product [_________].

[__________________________________] Product [_________].

Substitutions: Under provisions of Section [01600.] [________.]

COMPONENTS

Door Seal (Compressible construction):

Nominal Cross Section Dimensions: [____x____] inch ([____x____] mm).

Cushion:	Closed cell foam for full depth of seal; [straight] [tapered] jambs.

Covering Material: [Vinyl] [Neoprene] [Hypalon] [________] impregnated waterproof [nylon] [________] fabric; [with supplementary high abrasion resistant wear layer,] to remain flexible to [-65] [____] degrees F ([-54] [____] degrees C).

Covering Weight:	[22] [28] [40] [____] oz/sq ft ([6.7] [8.5] [12.2] [____] gm/sq m).

Covering Color: [Gray] [Green] [Black] [________] color [with [5] [____] inch ([125] [____] mm) wide yellow stripe continuous].

Header: [Fixed] [Movable] air vented construction.

Seams: [Molded without mechanical stitching] [Mechanically stitched]; [double] [triple] ply at exposed face.

Bottom Door Seal: [Same construction as above.] [________________.]

[Seal] [Shelter] Operating Range: [____] inches ([____] mm) beyond wall surface.

****** [OR] ******

Stationary Dock Shelter:

Frame Construction (Top and Sides): [Treated wood] [________].

Side [and Top] Covering Material: [Vinyl] [Neoprene] [Hypalon] [________] impregnated waterproof [nylon] [________] fabric; [with supplementary high abrasion resistant wear layer,] to remain flexible to [-65] [____] degrees F ([-54] [____] degrees C).

[Top Covering Material: Translucent waterproof [nylon] [________] fabric; to remain flexible to [-65] [____] degrees F ([-54] [____] degrees C).]

Covering Weight:	[22] [28] [40] [____] oz/sq ft ([6.7] [8.5] [12.2] [____] gm/sq m).

Covering Color: [Gray] [Green] [Black] [________] color [with [5] [____] inch ([125] [____] mm) wide yellow stripe continuous].

Seams: [Molded without mechanical stitching] [Mechanically stitched]; [double] [triple] ply at exposed face.

****** [OR] ******

Retractable Dock Shelter:

Frame Construction: [Galvanized] steel tubular frame construction; spring loaded scissor action maintained at extended position.

Frame Extension:	[____] inch ([____] mm) extended position from compressed stop.

Side [and Top] Covering Material: [Vinyl] [Neoprene] [Hypalon] [________] impregnated waterproof [nylon] [________] fabric; [with supplementary high abrasion resistant wear layer,] to remain flexible to [-65] [____] degrees F ([-54] [____] degrees C).

[Top Covering Material: Translucent waterproof [nylon] [________] fabric; to remain flexible to [-65] [____] degrees F ([-54] [____] degrees C).]

Covering Weight:	[22] [28] [40] [____] oz/sq ft ([6.7] [8.5] [12.2] [____] gm/sq m).

Covering Color: [Gray] [Green] [Black] [________] color [with [5] [____] inch ([125] [____] mm) wide yellow stripe continuous].

Seams: [Molded without mechanical stitching] [Mechanically stitched]; [double] [triple] ply at exposed face.

[Seal] [Shelter] Operating Range: [____] inches ([____] mm) beyond wall surface.

Fasteners: [Galvanized] [________] permitting site adjustment and alignment.

PART 3 EXECUTION

EXAMINATION

Verify existing conditions under provisions of Section [01039.] [________.]

Verify that rough-in wall opening and anchors are acceptable, correctly sized, and aligned to tolerances.

PREPARATION

Provide frame and integral anchors for placement by Section [________].

ERECTION

Erect [seal] [and] [shelter] components in accordance with manufacturer's instructions.

Set plumb and level.

Attach anchors and fittings to prepared wall construction and opening frame.

ADJUSTING

Adjust work under provisions of Section [01700.] [________.]

Adjust installed unit for smooth [and balanced] operation.

SCHEDULES

Main Loading Dock: 24 inch extension, retracting, two blue and two green vinyl covering.

Garbage Unloading Dock: 4 x 12 inch cross section dimensions, bright yellow neoprene/nylon covering.

END OF SECTION