SECTION 11172

WASTE COMPACTORS

PART 1 GENERAL

SECTION INCLUDES

Packaged waste compactor unit [and discharge container].

PRODUCTS FURNISHED BUT NOT INSTALLED UNDER THIS SECTION

Section [_____-__________]: Placement of rough-in unit frame and anchors.

RELATED SECTIONS

Section [_____-__________]: Placement of anchors bolts and inserts.

Section 09900 - Painting: Field painting of exposed steel frame.

Section [______-____________]: [Conveying device] [Garbage chute] with discharge to compactor unit.

Section [______-____________]: Domestic water supply to compactor unit.

Section [______-____________]:	Floor [funnel] drain.

Section [______-____________]: Conduit and electrical power to compactor unit controls.

REFERENCES

ANSI Z245.1 - Safety Requirements for Refuse Collection and Compaction Equipment.

ANSI/NEMA MG1 - Motors and Generators.

National Solid Wastes Management Association (NSWMA) -Commercial / Industrial Compactors Ratings.

SUBMITTALS

Submit under provisions of Section [01300.] [________.]

Shop Drawings: Indicate machine location, rough-in and anchor placement dimensions and tolerances, clearances required and [________].

Product Data: Provide unit capacities, physical dimensions, utility requirements and locations, point loads.

Test Reports: Indicate NSWMA ratings accompanied with certified test results.

Manufacturer's Installation Instructions: Indicate special installation requirements and [________].

Manufacturer's Certificate: Certify that [Products] [________] meet or exceed [specified requirements] [___________________].

OPERATION AND MAINTENANCE DATA

Submit under provisions of Section [01700.] [________.]

Operation Data: Include description of system operation, adjusting and testing required.

Maintenance Data: Identify system maintenance requirements, servicing cycles, lubrication types required and [local] spare part sources.

QUALITY ASSURANCE

Equipment Rating: In accordance with ANSI Z245.1 and NSWMA certification requirements.

Maintain [one copy] [[____] copies] of [each] document on site.

QUALIFICATIONS

Manufacturer: Company specializing in manufacturing the Products specified in this section with minimum [three] [_______] years [documented] experience.

REGULATORY REQUIREMENTS

Conform to [applicable] [___________] code for operating unit.

Provide certificate of compliance from [authority having jurisdiction] [________________] indicating approval of unit.

DELIVERY, STORAGE, AND HANDLING

Deliver, store, protect and handle products to site under provisions of Section [01600.] [________.]

Accept unit on site. Inspect for damage.

FIELD MEASUREMENTS

Verify that field measurements are as [indicated [on shop drawings].] [instructed by the manufacturer.]

SEQUENCING

Sequence work under the provisions of Section [01010.]

[________.]

Sequence work to leave building openings of sufficient size to permit transport of unit to final position.

COORDINATION

Coordinate work under provisions of Section [01039.] [________.]

Coordinate the work with installation of [garbage chute discharge] [________].

WARRANTY

Provide [five] [____] year warranty under provisions of Section [01700.] [________.]

Warranty: Include coverage for [motor] [and] [________].

PART 2 PRODUCTS

MANUFACTURERS

[__________________________________] Product [_________].

[__________________________________] Product [_________].

[__________________________________] Product [_________].

Substitutions: Under provisions of Section [01600.] [________.]

COMPONENTS

Compactor Operational Criteria:

Service Location: [Interior] [Exterior].

Type: [Top] [Rear] loading, [horizontal] [vertical] operating.

Control Mode: [Fully automatic] [Manual start] [Manual dump] [________].

Refuse Source:	[Chute] [By hand] [________].

Chamber Capacity Per Cycle: [____] cu ft ([____] cu m).

Cycle Time: [____] seconds.

Duty Cycle: [____] cycles per hour.

Volume Reduction: [____] percent.

Compactor Functional Criteria:

Clear Entry Opening: [___x___] inch ([___x___] mm).

Ram Face Pressure - Normal: [___] psi ([___] KPa).

Ram Face Pressure - Peak: [___] psi ([___] KPa).

Compaction Force - Normal:	[___] psi ([___] KPa).

Compaction Force - Peak: [___] psi ([___] KPa).

Compactor Features:

Construction: [Stainless] Steel, welded.

Motor: [ANSI/NEMA MG1,] [____] hp ([____] W), [____] volt, [1] [3] phase.

Control Panel: On/Off [key] switch, emergency STOP button, cycle selector switch for [single] [continuous] cycle operation.

Cycling:	Governed by electric eye connected to signal light to indicate discharge [bag] [container] is full.

Compacted Discharge: [Rear] [Front end] loading.

Odor Suppressing Features: [Disinfectant] [and deodorant] [________] spray.

Hopper Sprinkler: [________].

Conveyer For Multiple Bag Storage:	[________].

Discharge Container:

Volume Capacity: [____] cu ft ([____] cu m).

Weight Capacity: [____] lbs ([____] Kg).

Type: Plastic [single] [double] ply disposable bags.

****** [OR] ******

Discharge Container:

Volume Capacity: [____] cu ft ([____] cu m).

Weight Capacity: [____] lbs ([____] Kg).

Type: [Manufacturer's standard of fabricated steel, enamel finish] [________].

Transport Mechanism:	[[Front] [and] [rear] latch points.] [Steel wheels, fixed and caster.]

Discharge Conveyer: [________].

Anchors and Fasteners:	[Galvanized] [Stainless] steel.

SHOP FINISHING

Trash [Inlet] [and] [Outlet]: [Galvanized] [________].

Unit Frame and Accessories: [Zinc chromate] [________] primer; two [baked] enamel finish coats to [________] color [as selected].

PART 3 EXECUTION

EXAMINATION

Verify compactor frame anchors under provisions of Section [01039.] [________.]

Verify that anchors are correctly positioned.

PREPARATION

Provide [rough-in frame and] anchors for placement by Section [03100.] [________.]

INSTALLATION

Install unit [and inlet hopper] in accordance with manufacturer's instructions.

Install Work in accordance with standards required by authority having jurisdiction.

Anchor unit securely in place.

Touch-up minor damaged surfaces caused during installation. Replace damaged components as directed by Architect/Engineer.

INTERFACE WITH OTHER PRODUCTS

Coordinate installation with [garbage chute discharge] [________].

ADJUSTING

Adjust work under provisions of Section [01700.] [________.]

Adjust unit mechanism to achieve specified requirements.

DEMONSTRATION

Provide systems demonstration under provisions of Section [01650.] [________.]

Demonstrate and instruct [Owner] [________] on unit operation. Describe unit limitations.

END OF SECTION