SECTION 15440

PLUMBING FIXTURES

PART 1 GENERAL

SECTION INCLUDES

Water closets.

Urinals.

Lavatories.

Sinks.

Service sinks.

Electric water coolers.

Drinking fountains.

Showers.

Bathtubs.

Wash fountains.

Eyewash fountains.

Emergency showers.

PRODUCTS FURNISHED BUT NOT INSTALLED UNDER THIS SECTION

Section [_____-__________]: Placement of [terrazzo service sinks] [mop hangers] [shower curtains] [Shower bases] [reinforced glass fiber tubs and showers] [_____________].

PRODUCTS INSTALLED BUT NOT FURNISHED UNDER THIS SECTION

Section 01010 - Summary of Work:	Owner furnished fixtures including [__________________].

Section 10800 - Toilet and Bath Accessories:	Supply of [integral lavatory counter tops] [marble bath tubs] [_______________] for placement by this Section.

Section 11400 - Food Services Equipment:	Supply of [kitchen fixtures] [_______________] for placement by this Section.

Section 11600 - Laboratory Equipment: Supply of [laboratory fixtures] [_______________] for placement by this Section.

RELATED SECTIONS

Section 06410 - Custom Casework: Preparation of counters for sinks.

Section 06410 - Custom Casework: Lavatory tops.

Section 07900 - Joint Sealers: Seal fixtures to walls and floors.

Section 11400 - Food Services Equipment.

Section 11600 - Laboratory Equipment.

Section 15140 - Supports and Anchors.

Section 15410 - Plumbing Piping.

Section 15430 - Plumbing Specialties.

Section 15450 - Plumbing Equipment.

ALLOWANCES

Cash Allowance: Include under provisions of Section [01019.] [________.]

Allowance includes purchase and delivery of owner selected fixtures. Installation is included in this section and is part of the Contract Sum/Price.

REFERENCES

ANSI/ASME A112.6.1 - Supports for Off-the-Floor Plumbing Fixtures for Public Use.

ASME A112.18.1 - Finished and Rough Brass Plumbing Fixture Fittings.

ANSI/ASME A112.19.1 - Enameled Cast Iron Plumbing Fixtures.

ANSI/ASME A112.19.2 - Vitreous China Plumbing Fixtures.

ANSI/ASME A112.19.3 - Stainless Steel Plumbing Fixtures (Designed for Residential Use).

ANSI/ASME A112.19.4 - Porcelain Enameled Formed Steel Plumbing Fixtures.

ANSI/ASME A112.19.5 - Trim for Water-Closet Bowls, Tanks, and Urinals (Dimensional Standards).

IAPMO/ANSI Z124.1 - Plastic Bathtub Units.

IAPMO/ANSI Z124.2 - Plastic Shower Receptors and Shower Stalls.

ANSI Z358.1 - Emergency Eyewash and Shower Equipment.

ANSI/ARI 1010 - Drinking-Fountains and Self-Contained, Mechanically-Refrigerated Drinking-Water Coolers.

SUBMITTALS

Submit under provisions of Section [01300.] [________.]

Product Data: Provide catalogue illustrations of fixtures, sizes, [rough-in dimensions,] utility sizes, trim, and finishes.

Manufacturer's Installation Instructions.

OPERATION AND MAINTENANCE DATA

Submit under provisions of Section [01700.] [________.]

Maintenance Data: Include fixture trim exploded view and replacement parts lists.

MOCKUP

Provide mockup of typical bathroom group under provisions of Section [01400.] [________.]

Mockup may [not] remain as part of the Work.

DELIVERY, STORAGE, AND HANDLING

Deliver, store, protect and handle products to site under provisions of Section [01600.] [________.]

Accept fixtures on site in factory packaging. Inspect for damage.

Protect installed fixtures from damage by securing areas and by leaving factory packaging in place to protect fixtures and prevent use.

FIELD MEASUREMENTS

Verify that field measurements are as [indicated [on shop drawings].] [instructed by the manufacturer.]

Confirm that millwork is constructed with adequate provision for the installation of countertop lavatories and sinks.

WARRANTY

Provide [five] [____] year warranty under provisions of Section [01700.] [________.]

Warranty: Include coverage of [electric water cooler compressor.] [____________.]

EXTRA MATERIALS

Furnish under provisions of Section [01700.] [________.]

Provide [two] [____] of [faucet washers] [flush valve service kits] [_______________].

PART 2 PRODUCTS

WATER CLOSET (WC-1)

Bowl

Manufacturer: [_________________________] Model [________].

Other acceptable manufacturers offering equivalent products.

[_________________________] Model [________].

[_________________________] Model [________].

[_________________________] Model [________].

ANSI/ASME A112.19.2; [floor mounted, siphon jet] [[wall hung,] [siphon jet] [blow out]] vitreous china closet bowl, with elongated rim, 1-1/2 inch (38 mm) [top] [back] spud, china bolt caps.

Flush Valve

Manufacturer: [_________________________] Model [________].

Other acceptable manufacturers offering equivalent products.

[_________________________] Model [________].

[_________________________] Model [________].

[_________________________] Model [________].

ASME A112.18.1; exposed chrome plated, diaphragm type with oscillating handle, escutcheon, seat bumper, integral screwdriver stop and vacuum breaker [; maximum [3] [___] gpm ([12] [___] L) flush volume].

****** [OR] ******

ASME A112.18.1; concealed rough brass, diaphragm type with exposed chrome plated [push button] [oscillating handle] and escutcheon, screw driver stop and vacuum breaker [; maximum [3] [___] gpm ([12] [___] L) flush volume].

Seat

Manufacturer: [_________________________] Model [________].

Other acceptable manufacturers offering equivalent products.

[_________________________] Model [________].

[_________________________] Model [________].

[_________________________] Model [________].

Solid [black] [white] plastic, open front, extended back, [self-sustaining hinge,] brass bolts, [without] cover.

Wall Mounted Carrier

Manufacturer: [_________________________] Model [________].

Other acceptable manufacturers offering equivalent products.

[_________________________] Model [________].

[_________________________] Model [________].

[_________________________] Model [________].

ANSI/ASME A112.6.1; [adjustable] [non-adjustable] cast iron frame, integral drain hub and vent, adjustable spud, lugs for floor and wall attachment, threaded fixture studs with nuts and washers.

WATER CLOSET (WC-2)

Bowl

Manufacturer: [_________________________] Model [________].

Other acceptable manufacturers offering equivalent products.

[_________________________] Model [________].

[_________________________] Model [________].

[_________________________] Model [________].

ANSI/ASME A112.19.2; wall hung, vitreous china, reverse trap, whirlpool action close-coupled closet combination with regular rim, insulated vitreous china closet tank with fittings and lever flushing valve, chrome plated bolt caps.

****** [OR] ******

ANSI/ASME A112.19.2; floor mounted, siphon jet, vitreous china, [18 inches (450 mm) high] close-coupled closet combination with elongated rim, insulated vitreous china closet tank with fittings and lever flushing valve, bolt caps.

****** [OR] ******

ANSI/ASME A112.19.2; floor mounted, vitreous china reverse trap, close-coupled closet combination with regular rim, insulated vitreous china closet tank with fittings and lever flushing valve, bolt caps.

Seat

Manufacturer: [_________________________] Model [________].

Other acceptable manufacturers offering equivalent products.

[_________________________] Model [________].

[_________________________] Model [________].

[_________________________] Model [________].

Solid [black] [white] plastic, [open] [closed] front and cover, brass bolts.

****** [OR] ******

Solid [black] [white] plastic, open front, extended back, less cover, complete with self-sustaining hinge.

Wall Mounted Carrier

Manufacturer: [_________________________] Model [________].

Other acceptable manufacturers offering equivalent products.

[_________________________] Model [________].

[_________________________] Model [________].

[_________________________] Model [________].

ANSI/ASME A112.6.1; [adjustable] [non-adjustable] cast iron frame, integral drain hub and vent, adjustable spud, lugs for floor and wall attachment, threaded fixture studs with nuts and washers.

URINAL (UR-1)

Urinal

Manufacturer: [_________________________] Model [________].

Other acceptable manufacturers offering equivalent products.

[_________________________] Model [________].

[_________________________] Model [________].

[_________________________] Model [________].

ANSI/ASME A112.19.2; vitreous china, wall hung [washout] [blowout] [siphon jet] urinal with shields, integral trap, [removable stainless steel strainer,] [3/4] [1] inch ([19] [25] mm) [top] [back] spud, steel supporting hanger.

Flush Valve

Manufacturer: [_________________________] Model [________].

Other acceptable manufacturers offering equivalent products.

[_________________________] Model [________].

[_________________________] Model [________].

[_________________________] Model [________].

ASME A112.18.1; exposed chrome plated, diaphragm type with [oscillating handle,] [push plate,] escutcheon, integral screwdriver stop [,vacuum breaker] [; maximum [3] [___] gpm ([12] [___] L) flush volume].

****** [OR] ******

ASME A112.18.1; concealed rough brass, diaphragm type with exposed chrome plated [push button] [oscillating handle] and escutcheon, wheel handle stop and vacuum breaker [; maximum [3] [___] gpm ([12] [___] L) flush volume].

****** [OR] ******

ASME A112.18.1; exposed chrome plated, porous felt type for 1/2 inch (13 mm) supply with [oscillating handle,] [push button,] screwdriver stop [and vacuum breaker].

Wall Mounted Carrier

Manufacturer: [_________________________] Model [________].

Other acceptable manufacturers offering equivalent products.

[_________________________] Model [________].

[_________________________] Model [________].

[_________________________] Model [________].

ANSI/ASME A112.6.1; cast iron and steel frame with tubular legs, lugs for floor and wall attachment, threaded fixture studs for fixture hanger, bearing studs.

URINAL (UR-2)

Urinal

Manufacturer: [_________________________] Model [________].

Other acceptable manufacturers offering equivalent products.

[_________________________] Model [________].

[_________________________] Model [________].

[_________________________] Model [________].

ANSI/ASME A112.19.2; vitreous china slope front stall urinal with integral flushing rim, removable stainless steel strainer 3/4 inch (19 mm) top spud.

Flush Valve

Manufacturer: [_________________________] Model [________].

Other acceptable manufacturers offering equivalent products.

[_________________________] Model [________].

[_________________________] Model [________].

[_________________________] Model [________].

ASME A112.18.1; exposed chrome plated, diaphragm type with [oscillating handle,] [push plate,]escutcheon, integral screwdriver stop [,vacuum breaker] [; maximum [3] [___] gpm ([12] [___] L) flush volume].

****** [OR] ******

ASME A112.18.1; concealed rough brass, diaphragm type with exposed chrome plated [push button] [oscillating handle] and escutcheon, wheel handle stop and vacuum breaker [; maximum [3] [___] gpm ([12] [___] L) flush volume].

Flush Tank

Manufacturer: [_________________________] Model [________].

Other acceptable manufacturers offering equivalent products.

[_________________________] Model [________].

[_________________________] Model [________].

[_________________________] Model [________].

ANSI/ASME A112.19.5; vitreous china insulated tank with concealed cover, [bottom] [over rim] supply, siphon valve.

LAVATORY

Basin

Manufacturer: [_________________________] Model [________].

Other acceptable manufacturers offering equivalent products.

[_________________________] Model [________].

[_________________________] Model [________].

[_________________________] Model [________].

ANSI/ASME A112.19.2; vitreous china wall-hung lavatory [_____ x_____] inch ([_____ x _____] mm) minimum, with 4 inch (100 mm) high back, drillings on [4] [8] inch ([100] [200] mm) centers, rectangular basin with splash lip, front overflow, and soap depression.

****** [OR] ******

ANSI/ASME A112.19.1; porcelain enamelled cast iron wall-hung lavatory [_____ x_____] inch ([_____ x _____] mm) minimum, with 4 inch (100 mm) high back, drillings on [4] [8] inch ([100] [200] mm) centers, rectangular basin with splash lip, front overflow, and soap depression.

****** [OR] ******

ANSI/ASME A112.19.4; porcelain on steel self-rimming counter top lavatory, [_____ x _____] inches ([_____ x _____] mm) with drillings on [4] [8] inch ([100] [200] mm) centers, front overflow, [soap depression,] seal of putty, caulking, or concealed vinyl gasket.

****** [OR] ******

ANSI/ASME A112.19.2; vitreous china self-rimming counter top lavatory, [_____ x _____] inches ([_____ x _____] mm) with drillings on [4] [8] inch ([100] [200] mm) centers, front overflow, [soap depression,] seal of putty, caulking, or concealed vinyl gasket.

Trim

Manufacturer: [_________________________] Model [________].

Other acceptable manufacturers offering equivalent products.

[_________________________] Model [________].

[_________________________] Model [________].

[_________________________] Model [________].

ASME A112.18.1; chrome plated [combination] supply fitting with [pop-up waste,] [chain and plug,] [open grid strainer,] water economy aerator, [indexed handles,] [single lever handle,] chrome plated 17 gage (1.3 mm) brass P-trap [with clean-out plug] and arm with escutcheon.

****** [OR] ******

ASME A112.18.1; chrome plated metered mixing faucet with [aerator] [spray] and cover plate, open grid strainer, chrome plated 17 gage (1.3 mm) brass P-trap [with clean- out plug] and arm with escutcheon.

Wall Mounted Carrier

Manufacturer: [_________________________] Model [________].

Other acceptable manufacturers offering equivalent products.

[_________________________] Model [________].

[_________________________] Model [________].

[_________________________] Model [________].

ANSI/ASME A112.6.1; cast iron and steel frame with tubular legs, lugs for floor and wall attachment, [threaded studs for fixture hanger,] [concealed arm supports,] bearing plate and studs.

SINK

Bowl

Manufacturer: [_________________________] Model [________].

Other acceptable manufacturers offering equivalent products.

[_________________________] Model [________].

[_________________________] Model [________].

[_________________________] Model [________].

ANSI/ASME A112.19.3; single compartment [_____x_____x_____] inch ([_____x_____x_____] mm) outside dimensions, [20] [_____] gage ([0.9] [_____] mm) thick, Type [302] [304] [316] stainless steel, self-rimming with undercoating, 3-1/2 inch (90 mm) crumb cup and [chromed brass] [stainless steel] drain, ledge back drilled for trim.

****** [OR] ******

ANSI/ASME A112.19.3; double compartment [_____x_____x_____] inch ([_____x_____x_____] mm) outside dimensions [20] [___] gage ([0.9] [___] thick, Type [302] [304] [316] stainless steel, self-rimming with undercoating, 3-1/2 inch (90 mm) crumb cups, and [chromed brass] [stainless steel] drain, ledge back drilled for trim.

****** [OR] ******

[ANSI/ASME A112.19.4; steel,] [ANSI A112.19.1; cast iron,] porcelain enamelled [single] [double] compartment, [_____x_____x_____] inch ([_____x_____x_____] mm) outside dimensions, self-rimming and undercoated, with 3-1/2 inch (90 mm) diameter crumb cup and [chromed brass] [stainless steel] drain, ledge back drilled for trim.

Trim

Manufacturer: [_________________________] Model [________].

Other acceptable manufacturers offering equivalent products.

[_________________________] Model [________].

[_________________________] Model [________].

[_________________________] Model [________].

ASME A112.18.1; chrome plated brass supply with swing spout, water economy aerator, [indexed lever handles] [single lever handle] [and retractable spray]; chrome plated 17 gage (1.3 mm) brass P-trap [with clean-out plug] and arm with escutcheon.

BATHTUB [AND SHOWER]

Bathtub

Manufacturer: [_________________________] Model [________].

Other acceptable manufacturers offering equivalent products.

[_________________________] Model [________].

[_________________________] Model [________].

[_________________________] Model [________].

ANSI/ASME A112.19.4; [porcelain on steel] [enamelled cast iron] bathtub [with slip resistant surface,] contoured front apron, [60] [_____] inches ([1500] [_____] mm) long, [_________] color [as selected].

****** [OR] ******

IAPMO/ANSI Z124.1; molded glass fiber reinforced polyester, [with slip-resistant bottom surface,] contoured shape, [60] [_____] inches long x [30] [_____] inches wide([1 525] [_____] mm long x [760] [_____] mm wide) [_________] color [as selected].

Trim

Manufacturer: [_________________________] Model [________].

Other acceptable manufacturers offering equivalent products.

[_________________________] Model [________].

[_________________________] Model [________].

[_________________________] Model [________].

ASME A112.18.1; concealed over rim supply with spout and indexed handles, lever operated pop-up waste and overflow.

****** [OR] ******

ANSI A112.18.1; concealed shower and over rim supply with diverter spout, indexed handles, bent shower arm with [flow control and] [adjustable spray] ball joint showerhead and escutcheon, lever operated pop-up waste and overflow.

****** [OR] ******

ANSI A112.18.1; concealed shower and over rim supply with diverter spout, [pressure balanced] [thermostatic] mixing valve, bent shower arm with [flow control and] [adjustable spray] ball joint showerhead and escutcheon, lever operated pop-up waste and overflow.

SHOWER

Cabinet

Manufacturer: [_________________________] Model [________].

Other acceptable manufacturers offering equivalent products.

[_________________________] Model [________].

[_________________________] Model [________].

[_________________________] Model [________].

ANSI A112.19.4; porcelain enamelled steel, [32 x 32 x 75] [___x___x___] inch ([800 x 800 x 1900] [___x___x___] mm) high, with [stone texture] receptor, soap dish, removable chrome plated strainer, tail piece, [_________] color [as selected].

****** [OR] ******

ANSI Z124.2 reinforced glass fiber, [32 x 32 x 75] [___x___x___] inch ([800 x 800 x 1900] [___x___x___] mm) high, with [stone texture] receptor, soap dish, [integral seat,] removable chrome plated strainer, tail piece, [_________] color [as selected].

Trim

Manufacturer: [_________________________] Model [________].

Other acceptable manufacturers offering equivalent products.

[_________________________] Model [________].

[_________________________] Model [________].

[_________________________] Model [________].

ASME A112.18.1; concealed shower supply with indexed handles, bent shower arm with [flow control and] [adjustable spray] ball joint shower head and escutcheon.

****** [OR] ******

ASME A112.18.1; concealed straight way pattern valve with indexed cross handle.

****** [OR] ******

ASME A112.18.1; concealed rough brass metering valve with closed fluid metering system adjustable from 5 to 120 seconds, chrome plated push button and escutcheon, wheel handle stop.

****** [OR] ******

ASME A112.18.1; concealed shower supply with [pressure balanced] [thermostatic] mixing valves, bent shower arm with [flow control and] [adjustable spray] ball joint shower head and escutcheon.

Shower Head

Manufacturer: [_________________________] Model [________].

Other acceptable manufacturers offering equivalent products.

[_________________________] Model [________].

[_________________________] Model [________].

[_________________________] Model [________].

ASME A112.18.1; chrome plated vandal-proof institutional head with integral wall bracket, built-in 2-1/2 gal/min (0.2 L/sec) flow control.

DRINKING FOUNTAIN

Fountain

Manufacturer: [_________________________] Model [________].

Other acceptable manufacturers offering equivalent products.

[_________________________] Model [________].

[_________________________] Model [________].

[_________________________] Model [________].

Molded [white] [____________________] reinforced glass fiber with underside vandal proof cowling, hooded elevated anti-squirt bubbler with stream guard, automatic stream regulator, [cross] [lever] handle, mounting bracket, screwdriver stop.

****** [OR] ******

[White] [____________________] [reinforced glass fiber,] [vitreous china,] [semi-recessed,] [fully-recessed,] with elevated anti-squirt bubbler with stream guard, automatic stream regulator, [cross] [lever] handle,access cover plate, mounting bracket, screwdriver stop.

ELECTRIC WATER COOLER

Fountain

Manufacturer: [_________________________] Model [________].

Other acceptable manufacturers offering equivalent products.

[_________________________] Model [________].

[_________________________] Model [________].

[_________________________] Model [________].

ANSI/ARI 1010; [surface] [semi-recessed] [recessed] [handicapped] mounted electric water cooler with stainless steel top, [vinyl on steel] [stainless steel] [__________] body, elevated anti-squirt bubbler with stream guard, automatic stream regulator, mounting bracket, refrigerated with integral air cooled condenser.

Capacity: [_____] gpm ([_____] L/s) of 50 degree F (10 degree C) water with inlet at 80 degree F (27 degree C) and room temperature of 90 degree F (32 degree C).

Electrical: Maximum [_____] hp ([_____] kW) compressor, [6] [____] foot ([2] [____] m) cord and plug for connection to electric wiring system [including grounding connector].

WASH FOUNTAINS

Bowl

Manufacturer: [_________________________] Model [________].

Other acceptable manufacturers offering equivalent products.

[_________________________] Model [________].

[_________________________] Model [________].

[_________________________] Model [________].

[Circular] [Semi-circular], [36] [54] [____] inch ([900] [1450] [____] mm) diameter, [precast stone] [enamelled steel] [stainless steel].

Accessories

Manufacturer: [_________________________] Model [________].

Other acceptable manufacturers offering equivalent products.

[_________________________] Model [________].

[_________________________] Model [________].

[_________________________] Model [________].

Foot controlled self-closing valve, spray head, liquid soap dispenser, [manual] [thermostatic] mixing valve, supporting tube, spud and strainer, operating mechanism, foot levers and rail, combination stop, strainer and check valves.

SERVICE SINK (SS-1)

Bowl

Manufacturer: [_________________________] Model

[________].

Other acceptable manufacturers offering equivalent products.

[_________________________] Model [________].

[_________________________] Model [________].

[_________________________] Model [________].

ANSI/ASME A112.19.1; 22 x 18 x 12 inch (560 x 460 x 300 mm) deep, porcelain enamelled (inside only) cast iron roll-rim sink, with 12 inch (300 mm) high back, concealed hanger, chrome plated strainer, cast iron P-trap with adjustable floor flange.

****** [OR] ******

[36] [24] x 24 x 10 inch ([900] [600] x 600 x 250 mm) high [white] [_____] molded stone, floor mounted, with one inch (25 mm) wide shoulders, stainless steel strainer.

Trim

Manufacturer: [_________________________] Model [________].

Other acceptable manufacturers offering equivalent products.

[_________________________] Model [________].

[_________________________] Model [________].

[_________________________] Model [________].

ASME A112.18.1 exposed wall type supply with [cross] [lever] handles, spout wall brace, vacuum breaker, hose end spout, strainers, eccentric adjustable inlets, integral screwdriver stops with covering caps and adjustable threaded wall flanges; 5 feet (1.5 m) of 1/2 inch (13 mm) diameter plain end reinforced [plastic] [rubber] hose, hose clamp, mop hanger.

Accessories

5 feet (1.5 m) of 1/2 inch (13 mm) diameter plain end reinforced [plastic] [rubber] hose.

Hose clamp hanger.

Mop hanger.

EMERGENCY EYE [AND FACE] WASH

Manufacturer:

[_________________________] Model [________].

Other acceptable manufacturers offering equivalent products.

[_________________________] Model [________].

[_________________________] Model [________].

[_________________________] Model [________].

ANSI Z358.1; [wall-mounted,] [free standing,] self-cleaning, non-clogging eye [and face] wash with quick opening, full-flow valves, [stainless steel] [ABS] eye [and face] wash receptor, twin eye wash heads [and face spray ring,] [stainless steel dust cover,] [copper alloy] [PVC] control valve and fittings.

EMERGENCY SHOWER (EW-2)

Manufacturer:

[_________________________] Model [________].

Other acceptable manufacturers offering equivalent products.

[_________________________] Model [________].

[_________________________] Model [________].

[_________________________] Model [________].

ANSI Z358.1; [wall-mounted,] [free standing,] self-cleaning, non-clogging 8 inch (200 mm) diameter [stainless steel] [copper alloy] [plastic] deluge shower head with elbow, one inch (25 mm) full flow valve with pull chain and 8 inch (200 mm) diameter ring, one inch (25 mm) interconnecting fittings.

PART 3 EXECUTION

EXAMINATION

Verify that walls and floor finishes are prepared and ready for installation of fixtures.

Verify that electric power is available and of the correct characteristics.

PREPARATION

Rough-in fixture piping connections in accordance with minimum sizes indicated in fixture rough-in schedule for particular fixtures.

INSTALLATION

Install in accordance with manufacturer's instructions.

Install each fixture with trap, easily removable for servicing and cleaning.

Provide chrome plated rigid or flexible supplies to fixtures with [loose key] [screwdriver] [__________] stops, reducers, and escutcheons.

Install components level and plumb.

Install and secure fixtures in place with [wall supports] [wall carriers] and bolts.

Seal fixtures to wall and floor surfaces with sealant as specified in Section 07900, color to match fixture.

Solidly attach water closets to floor with lag screws. Lead flashing is not intended hold fixture in place.

INTERFACE WITH OTHER PRODUCTS

Review millwork shop drawings. Confirm location and size of fixtures and openings before rough-in and installation.

ADJUSTING

Adjust work under provisions of Section [01700.] [________.]

Adjust stops or valves for intended water flow rate to fixtures without splashing, noise, or overflow.

CLEANING

Clean work under provisions of [01700.] [________.]

At completion clean plumbing fixtures and equipment.

PROTECTION OF FINISHED WORK

Protect finished Work under provisions of Section [01500.] [________.]

Do not permit use of fixtures.

FIXTURE HEIGHTS

Install fixtures to heights above finished floor as indicated.

Water-Closet

Standard [15] [___] inches ([380] [___] mm) to top of bowl rim.

Handicapped [18] [___] inches ([455] [___] mm) to top of seat.

Urinal

Standard [22] [___] inches ([560] [___] mm) to top of bowl rim.

Handicapped [19] [___] inches ([485] [___] mm) to top of bowl rim.

Lavatory

Standard [31] [___] inches ([785] [___] mm) to top of basin rim.

Handicapped [32] [___] inches ([810] [___] mm) to top of basin rim.

Drinking Fountain

Standard [30] [40] [___] inches [760] [1015] [___] mm to top of basin rim.

Handicapped [36] [___] inches ([915] [___] mm) to top of basin rim.

Water Closet Flush Valves

Standard [11] [___] inches ([280] [___] mm) min. above bowl rim.

Recessed [10] [___] inches ([255] [___] mm) min. above bowl rim.

Shower Heads

Adult [male] [69.5] [___] inches ([1765] [___] mm) to bottom of head.

Adult [female] [64.5] [___] inches ([1640] [___] mm) to bottom of head.

Child [58.5] [___] inches ([1490] [___] mm) to bottom of head.

Emergency Eye [And Face] Wash

Standard [38] [___] inches ([965] [___] mm) to receptor rim.

Emergency Shower

Standard [84] [___] inches ([2130] [___] mm) to bottom of head.

FIXTURE ROUGH-IN SCHEDULE

Hot Water Cold Water	Waste_______Vent

Lavatory:	1/2 inch	1/2 inch	1-1/2 inch	1-1/4 inch

(13 mm)	(13 mm)	(38 mm)	(32 mm)

Service Sink:	1/2 inch	1/2 inch	2 inch	1-1/2 inch

(13 mm)	(13 mm)	(50 mm)	(38 mm)

Service Sink:	1/2 inch	1/2 inch	3 inch	1-1/2 inch

(13 mm)	(13 mm)	(75 mm)	(38 mm)

Sink:	1/2 inch	1/2 inch	1-1/2 inch	1-1/4 inch

(13 mm)	(13 mm)	(38 mm)	(32 mm)

Drinking	1/2 inch	1-1/4 inch	1-1/4 inch

Fountain:	(13 mm)	(32 mm)	(32 mm)

Water Closet	1 inch	4 inch	2 inch

(Flush Valve):	(25 mm)	(100 mm)	(50 mm)

Water Closet	1/2 inch	4 inch	2 inch

(Tank Type):	(13 mm)	(100 mm)	(50 mm)

Urinal	3/4 inch	2 inch	1-1/2 inch

(Flush Valve):	(19 mm)	(50 mm)	(38 mm)

Urinal	1/2 inch	2 inch	1-1/2 inch

(Tank Type):	(13 mm)	(50 mm)	(38 mm)

END OF SECTION