SECTION 16180

EQUIPMENT WIRING SYSTEMS

PART 1	GENERAL

SECTION INCLUDES

Electrical connections to equipment specified under other sections.

RELATED SECTIONS

Section [01010 - Summary of Work] [01011 - Summary of Project]: Owner-furnished equipment.

Section 08331 - Overhead Coiling Doors.

Section 11400 - Food Services Equipment.

Section 11600 - Laboratory Equipment.

Section 14215 - Electric Elevators - Passenger.

Section 15450 - Plumbing Equipment.

Section 15784 - Unit Air Conditioners.

Section 16111 - Conduit.

Section 16123 - Building Wire and Cable.

Section 16130 - Boxes.

REFERENCES

NEMA WD 1 - General Purpose Wiring Devices.

NEMA WD 6 - Wiring Device Configurations.

ANSI/NFPA 70 - National Electrical Code.

SUBMITTALS

Submit under provisions of Section [01300.] [_____.]

Product Data: Provide wiring device manufacturer's catalog information showing dimensions, configurations, and construction.

Manufacturer's Instructions:	Indicate application conditions and limitations of use stipulated by Product testing agency specified under Regulatory Requirements. Include instructions for storage, handling, protection, examination, preparation, installation, and starting of Product.

REGULATORY REQUIREMENTS

Conform to requirements of ANSI/NFPA 70.

Furnish products listed and classified by [Underwriters Laboratories, Inc.] [testing firm acceptable to authority having jurisdiction] as suitable for purpose specified and shown.

COORDINATION

Coordinate work under provisions of Section [01039.] [______.]

Obtain and review shop drawings, product data, and manufacturer's instructions for equipment furnished under other sections.

Determine connection locations and requirements.

Sequence rough-in of electrical connections to coordinate with installation schedule for equipment.

Sequence electrical connections to coordinate with start-up schedule for equipment.

PART 2	PRODUCTS

CORDS AND CAPS

Manufacturers:

[______________________________] Model [___________.]

[______________________________] Model [___________.]

[______________________________] Model [___________.]

Substitutions: Under provisions of Section [01600.] [_______.]

Attachment Plug Construction: Conform to NEMA WD 1.

Configuration: NEMA WD 6; match receptacle configuration at outlet provided for equipment.

Cord Construction: ANSI/NFPA 70, Type [SO] [SJO] [____] multiconductor flexible cord with identified equipment grounding conductor, suitable for use in damp locations.

Size: Suitable for connected load of equipment, length of cord, and rating of branch circuit overcurrent protection.

PART 3	EXECUTION

EXAMINATION

Verify conditions under provisions of Section [01039.] [_____.]

Verify that equipment is ready for electrical connection, wiring, and energization.

ELECTRICAL CONNECTIONS

Make electrical connections in accordance with equipment manufacturer's instructions.

Make conduit connections to equipment using flexible conduit. Use liquidtight flexible conduit with watertight connectors in damp or wet locations.

Make wiring connections using wire and cable with insulation suitable for temperatures encountered in heat producing equipment.

Provide receptacle outlet where connection with attachment plug is indicated. Provide cord and cap where field-supplied attachment plug is indicated.

Provide suitable strain-relief clamps and fittings for cord connections at outlet boxes and equipment connection boxes.

Install disconnect switches, controllers, control stations, and control devices as indicated.

Modify equipment control wiring with terminal block jumpers as indicated.

Provide interconnecting conduit and wiring between devices and equipment where indicated.

Coolers and Freezers: Cut and seal conduit openings in freezer and cooler walls, floor, and ceilings.

EQUIPMENT CONNECTION SCHEDULE

Air Conditioning Unit AC-1:

Furnished:	Section 15781.

Installed:	Section 15781.

Electrical Connection: Flexible conduit; provide field-installed disconnect switch.

Voltage: 480 volts, 3 phase, 60 Hz.

Load rating: 19 kW + 7.5 hp.

FLA: 31.6 amperes.

WSA: 38.3 amperes.

Branch Circuit: 80 ampere fuse, maximum.

Location: Roof, above room 453.

Air Conditioning Unit AC-2:

Furnished:	Section 01010.

Installed:	Section 15784.

Electrical Connection:	Cord and plug (NEMA 6-20R).

Voltage: 208 volts, 1 phase, 60 Hz.

Load rating: N/A.

FLA: 12.6 amperes.

WSA: 15.3 amperes.

Branch Circuit: 20 ampere fuse, maximum.

Location: Room 208.

Door Operator 3:

Furnished:	Section 08331.

Installed:	Section 08331.

Electrical Connection: Flexible conduit; provide field-installed disconnect switch.

Voltage: 480 volts, 3 phase, 60 Hz.

Load rating: 5 hp.

FLA: N/A.

WSA: N/A.

Branch Circuit: N/A.

Location: Door 3.

END OF SECTION