SECTION 16510

INTERIOR LUMINAIRES

PART 1 GENERAL

SECTION INCLUDES

Interior luminaires and accessories.

Emergency lighting units.

Exit signs.

Ballasts.

Fluorescent dimming ballasts and controls.

Fluorescent lamp emergency power supply.

Lamps.

Luminaire accessories.

RELATED SECTIONS

Section [15930] [________] - [Air Terminal Units] [_____] - [____________________________]: Air distribution accessories for air handling luminaires.

Section 16130 - Boxes.

Section 16520 - Luminous Ceilings.

REFERENCES

ANSI C78.379 - Electric Lamps - Incandescent and High-Intensity Discharge Reflector Lamps - Classification of Beam Patterns.

ANSI C82.1 - Ballasts for Fluorescent Lamps - Specifications.

ANSI C82.4 - Ballasts for High-Intensity Discharge and Low Pressure Sodium Lamps (Multiple Supply Type).

ANSI/NFPA 70 - National Electrical Code.

ANSI/NFPA 101 - Life Safety Code.

NEMA WD 6 - Wiring Devices-Dimensional Requirements.

SUBMITTALS

Submit under provisions of Section [01300] [________].

Shop Drawings: Indicate dimensions and components for each luminaire that is not a standard product of the manufacturer.

Product Data: Provide dimensions, ratings, and performance data.

Manufacturer's Instructions:	Indicate application conditions and limitations of use stipulated by product testing agency specified under Regulatory Requirements.

Manufacturer's Instructions:	Include instructions for storage, handling, protection, examination, preparation, and installation of product.

PROJECT RECORD DOCUMENTS

Submit under provisions of Section [01700] [_________].

Accurately record actual locations of each luminaire.

OPERATION AND MAINTENANCE DATA

Submit under provisions of Section [01700] [________].

Maintenance Data: Include replacement parts list.

QUALIFICATIONS

Manufacturer: Company specializing in manufacturing products specified in this Section with minimum [three] [________] years [documented] experience.

REGULATORY REQUIREMENTS

Conform to requirements of ANSI/NFPA 70.

Conform to requirements of [NFPA 101] [________________].

Furnish products listed and classified by [Underwriters Laboratories, Inc.] [testing firm acceptable to authority having jurisdiction] as suitable for purpose specified and shown.

EXTRA MATERIALS

Furnish under provisions of Section [01700] [________].

Provide [two] [_______] of each plastic lens.

Provide [one] [______] replacement lamp for each lamp installed.

Provide [two] [______] of each ballast type.

Provide [______] of [________________________________.]

PART 2 PRODUCTS

LUMINAIRES

Furnish products as specified [in schedule] [on Drawings].

Substitutions: Under provisions of Section [01600] [____].

Install ballasts, lamps, and specified accessories at factory.

****** [OR] ******

Manufacturers:

[_________________________________] Model [________].

[_________________________________] Model [________].

[_________________________________] Model [________].

Substitutions: Under provisions of Section [01600] [____].

Description:	[Troffer] [Downlight] [________________________________] type luminaire with [ballast] [,lamps] [and] [________________] installed by luminaire manufacturer.

Size: [________________________________].

Material: [Sheet steel housing] [_____________________].

Enclosure: [Prismatic acrylic lens, pattern 12] [Clear glass] [________________________________]. [Provide gasketing between enclosure and frame and between frame and luminaire housing.]

Photometric Control Elements: [Anodized specular aluminum reflector] [___________________________________].

Photometric Performance:	[Minimum coefficient of utilization 0.65 at room cavity ratio of 2 with ceiling- wall-floor reflectance of 70-50-20 percent] [____].

Installation Conditions:	[Wet Location]	[Damp Location] [Enclosed and Gasketed] [____].

Mounting: [Ceiling surface] [Recessed in grid ceiling] [Pendant] [Wall mounting] [___________________________________].

Ballast:	[Manufacturer's standard, matched to lamp characteristics, rated [120] [277] volts.] [_______________________________________________________].

Lamp: [One] [_______] each, [__________________________________________].

Accessories:

[________________________________________].

INCANDESCENT EMERGENCY LIGHTING UNITS

Manufacturers:

[_________________________________] Model [________].

[_________________________________] Model [________].

[_________________________________] Model [________].

Substitutions: Under provisions of Section [01600] [____].

Description: Self-contained emergency lighting unit.

Battery:	[6] [12] volt, [nickel-cadmium] [lead calcium] [____] type, with 1.5 hour capacity.

Battery Charger:	Dual-rate type, with sufficient capacity to recharge discharged battery to full charge within twelve hours.

Lamps: [12] [______] watt minimum, [sealed beam type in nickel or chrome plated steel housing] [____].

Remote Lamps: [Match lamps on unit] [____].

Housing:	[Steel with [gray] [bronze] hammer tone finish [and vinyl wood grain front panel]] [White plastic] [____].

Indicators: Provide lamps to indicate AC ON and RECHARGING. [Provide voltmeter].

Provide TEST switch to transfer unit from external power supply to integral battery supply.

Electrical Connection: [6 foot (2 M) cord with plug cap, NEMA WD 6, Type 5-15 configuration] [Conduit connection].

Input Voltage:	[120] [277] volts.

EXIT SIGNS

Manufacturers:

[_________________________________] Model [________].

[_________________________________] Model [________].

[_________________________________] Model [________].

Substitutions: Under provisions of Section [01600] [____].

Description:	Exit sign fixture [suitable for use as emergency lighting unit].

Housing: [Extruded aluminum] [Sheet steel] [__________________].

Face: [Translucent [glass] [plastic] face with [red] [green] [________] letters on [white] [_________] background] [[Aluminum] [Steel] stencil face with [red] [green] letters].

Directional Arrows: [As indicated] [Universal type for field adjustment].

Mounting: [As indicated] [Wall] [Ceiling] [Pendant] [Universal, for field selection].

Battery:	[6] [12] volt, [nickel-cadmium] [lead calcium] [____] type, with 1.5 hour capacity.

Battery Charger:	Dual-rate type, with sufficient capacity to recharge discharged battery to full charge within twelve hours.

Lamps:	[Manufacturers standard] [________________________________].

Input Voltage: [120] [277] volts.

Accessories: [_______________________________________].

BALLASTS

Fluorescent Ballast:

[_________________________________] Model [________].

[_________________________________] Model [________].

[_________________________________] Model [________].

Substitutions: Under provisions of Section [01600] [____].

Description:	[ANSI C82.1, high power factor type electromagnetic ballast] [____].

Provide ballast suitable for lamps specified.

Voltage:	[[120] [277] [____] volts] [Match luminaire voltage].

Source Quality Control: Certify ballast design and construction by Certified Ballast Manufacturers, Inc.

High Intensity Discharge (HID) Ballast:

[_________________________________] Model [________].

[_________________________________] Model [________].

[_________________________________] Model [________].

Substitutions: Under provisions of Section [01600] [____].

Description:	ANSI C82.4, [mercury vapor] [metal halide] [low pressure sodium] [high pressure sodium] lamp ballast.

Provide ballast suitable for lamp specified.

Voltage:	[[120] [277] volts] [Match luminaire voltage].

FLUORESCENT DIMMING BALLASTS AND CONTROLS

Control Unit: [Rotary] [Linear slide] type, rated [500]

[1000] [1500] [_______] watts at [120] [277] volts.

[_________________________________] Model [________].

[_________________________________] Model [________].

[_________________________________] Model [________].

Substitutions: Under provisions of Section [01600] [____].

Dimming Ballast:

[____________________________________________].

[____________________________________________].

[____________________________________________].

Furnish dimming ballasts in specified luminaires.

Use ballast selected by dimming system manufacturer as suitable for operation with control unit.

Lamps: [Suitable for lamp type and quantity specified for luminaire] [_____________________________________.]

FLUORESCENT LAMP EMERGENCY POWER SUPPLY

Manufacturers:

[_________________________________] Model [________].

[_________________________________] Model [________].

[_________________________________] Model [________].

Substitutions: Under provisions of Section [01600] [____].

Description:	Emergency battery power supply suitable for installation in ballast compartment of fluorescent luminaire.

Lamp Ratings: [One F40CW lamp providing 600 lumens, minimum] [_______________________________________________].

Battery:	Sealed [lead calcium] [________________________] type, rated for [10] [____] year life.

Include TEST switch and AC ON indicator light, installed to be operable and visible from the outside of an assembled luminaire.

LAMPS

Incandescent Lamp Manufacturers:

[___________________________________].

[___________________________________].

[___________________________________].

Substitutions: Under provisions of Section [01600] [______________].

Fluorescent Lamp Manufacturers:

[___________________________________].

[___________________________________].

[___________________________________].

Substitutions: Under provisions of Section [01600]

[______________].

High Intensity Discharge (HID) Lamp Manufacturers:

[___________________________________].

[___________________________________].

[___________________________________].

Substitutions: Under provisions of Section [01600] [______________].

Provide lamp type specified for luminaire.

Reflector Lamp Beam Patterns: ANSI C78.379.

ACCESSORIES

[_______________________________________________]:

[_________________________________] Model [________].

[_________________________________] Model [________].

[_________________________________] Model [________].

Substitutions: Under provisions of Section [01600] [______________].

Description: [_______________________________________].

PART 3 EXECUTION

EXAMINATION

Examine substrate [and supporting grids] for luminaires.

Examine each luminaire to determine suitability for lamps specified.

INSTALLATION

Install in accordance with manufacturers instructions.

Install suspended luminaires [and] [exit signs] using pendants supported from swivel hangers. Provide pendant length required to suspend luminaire at indicated height.

Support luminaires larger than 2 x 4 foot (600 x 1 200 mm) size independent of ceiling framing.

Locate recessed ceiling luminaires as indicated on reflected ceiling plan.

Install surface mounted luminaires [and] [exit signs] plumb and adjust to align with building lines and with each other. Secure to prohibit movement.

Exposed Grid Ceilings: [Support surface mounted luminaires on grid ceiling directly from building structure] [Provide auxiliary members spanning ceiling Ts to support surface mounted luminaires] [Fasten surface mounted luminaires to

ceiling T using bolts, screws, rivets, or suitable clips].

Install recessed luminaires to permit removal from below.

Install recessed luminaires using accessories and firestopping materials to meet regulatory requirements for fire rating.

Install clips to secure recessed grid-supported luminaires in place.

Install wall mounted luminaires [, emergency lighting units] [and] [exit signs] at height [as indicated on Drawings] [as scheduled].

Install accessories furnished with each luminaire.

Connect luminaires [, emergency lighting units] [and] [exit signs] to branch circuit outlets provided under Section 16130 [using flexible conduit] [as indicated].

Make wiring connections to branch circuit using building wire with insulation suitable for temperature conditions within luminaire.

Bond products and metal accessories to branch circuit equipment grounding conductor.

Install specified lamps in each luminaire [, emergency lighting unit] [and] [exit sign].

INTERFACE WITH OTHER PRODUCTS

Interface with air handling accessories furnished and installed under Section [15930] [________].

FIELD QUALITY CONTROL

Operate each luminaire after installation and connection. Inspect for proper connection and operation.

ADJUSTING

Adjust Work under provisions of Section [01700] [________].

Aim and adjust luminaires [as indicated on Drawings] [as directed].

Adjust exit sign directional arrows as indicated.

Relamp luminaires [that have failed lamps] at Substantial Completion.

CLEANING

Clean Work under provisions of Section [01700] [________].

Clean electrical parts to remove conductive and deleterious materials.

Remove dirt and debris from enclosure.

Clean photometric control surfaces as recommended by manufacturer.

Clean finishes and touch up damage.

DEMONSTRATION

Provide systems demonstration under provisions of Section [01650] [________].

Provide [minimum of [two] [_______] hours] demonstration of luminaire operation.

SCHEDULE

Type A Interior Luminaire:

ABC Company Model XYZ.

Isocandela Corporation Catalog No. 123A456.

Clunk Luminaire Company Type XY-45.

Description: Fluorescent troffer.

Material: Painted steel.

Mounting: Recessed grid ceiling.

Ballast: Manufacturer's standard, rated 120 volts.

Lamp: Four F40CW.

Type B Interior Luminaire:

Church Downlight Company Model 80867.

Pratt Lighting, Inc. Catalog 703-684-030.

Watson Bright, Ltd. Canadienne Series.

Description: Surface downlight.

Size: 10 inches round.

Material: Extruded aluminum housing.

Enclosure:	Open.

Photometric Control:	Anodized specular aluminum reflector.

Installation Conditions: Dry Location.

Mounting: Ceiling surface mounting.

Ballast: Manufacturer's standard, matched to lamp characteristics, rated 277 volts.

Lamp: 150 watts, metal halide type coated lamp.

END OF SECTION