SECTION 16530

SITE LIGHTING

PART 1 GENERAL

SECTION INCLUDES

Exterior luminaires and accessories.

Poles.

RELATED SECTIONS

Section 03300 - Cast-in-Place Concrete: Foundations for poles.

REFERENCES

ANSI C78.379 - Electric Lamps - Incandescent and High-Intensity Discharge Reflector Lamps - Classification of Beam Patterns.

ANSI C82.1 - Ballasts for Fluorescent Lamps- Specifications.

ANSI C82.4 - Ballasts for High-Intensity-Discharge and Low-Pressure Sodium Lamps (Multiple-Supply Type).

ANSI O5.1 - Specifications and Dimensions for Wood Poles.

ANSI/NFPA 70 - National Electrical Code.

ANSI/IES RP-8 - Recommended Practice for Roadway Lighting.

ANSI/IES RP-20 - Lighting for Parking Facilities.

SYSTEM DESCRIPTION

Roadway lighting of [____________________________].

Parking area lighting of [_______________________].

DESIGN REQUIREMENTS

Design and layout lighting system in conformance with IES recommended procedures.

Roadway:	ANSI/IES RP-8, [freeway] [expressway] [major] [collector] [local] [alley] [sidewalk] [pedestrian walkway] [isolated interchange] [isolated intersection] [bikeway].

****** [OR] ******

Roadway:	ANSI/IES RP-8, classification as indicated on Drawings.

Parking Lot:	ANSI/IES RP-20, [low] [medium] [high] activity level.

[__________________________________________________].

PERFORMANCE REQUIREMENTS

Roadway:	[Provide illumination levels and uniformity indicated on Drawings] [__________________].

Parking Area: [Provide illumination levels and uniformity indicated on Drawings] [__________________].

SUBMITTALS

Submit under provisions of Section [01300] [_____].

Shop Drawings: Indicate dimensions and components for each luminaire which is not a standard product of the manufacturer.

Product Data: Provide dimensions, ratings, and performance data.

Design Data: Include lighting calculations.

Test Reports: Indicate measured illumination levels.

Manufacturer's Instructions:	Indicate application conditions and limitations of use stipulated by product testing agency specified under "Regulatory Requirements".

Manufacturer's Instructions:	Include instructions for storage, handling, protection, examination, preparation, installation, and starting of product.

PROJECT RECORD DOCUMENTS

Submit under provisions of Section [01700] [_____].

Accurately record actual locations of each luminaire.

OPERATION AND MAINTENANCE DATA

Submit under provisions of Section [01700] [_____].

Maintenance Data: Include instructions for maintaining luminaires.

QUALIFICATIONS

Manufacturer: Company specializing in manufacturing products specified in this Section with minimum [three] [_____] years [documented] experience.

REGULATORY REQUIREMENTS

Conform to requirements of ANSI/NFPA 70.

Furnish products listed and classified by [Underwriters Laboratories, Inc.] [testing firm acceptable to authority having jurisdiction] as suitable for purpose specified and shown.

DELIVERY, STORAGE, AND HANDLING

Deliver, store, protect, and handle products to site under provisions of Section [01600] [_____].

Accept products on site. Inspect for damage.

Protect poles from finish damage by handling carefully.

Store and handle solid wood poles in accordance with ANSI O5.1.

COORDINATION

Furnish bolt templates and pole mounting accessories to installer of pole foundations.

EXTRA MATERIALS

Furnish under provisions of Section [01700] [_____].

Provide [two] [_____] of each lamp type and wattage installed.

PART 2 PRODUCTS

LUMINAIRES

Furnish products as specified [in schedule] [on Drawings].

Substitutions: Under provisions of Section [01600] [_____].

****** [OR] ******

Manufacturers:

[_________________________] Model [__________].

[_________________________] Model [__________].

[_________________________] Model [__________].

Substitutions: Under provisions of Section [01600] [___].

Description:	[Roadway] [Area flood] [__________] type luminaire.

Size: [_______________].

Material: [Extruded aluminum housing with cast aluminum bracket] [______________________________].

Enclosure: [Clear glass] [________________]. [Provide gasketing between enclosure and frame and luminaire body.]

Photometric Control:	[Anodized specular aluminum reflector] [_____________________________].

Photometric Performance: ANSI/IES RP-8.

Vertical Light Distribution: [Short] [Medium] [Long].

Lateral Light Distribution: [Type I] [Type I, four way] [Type II] [Type II, four way] [Type III] [Type IV] [Type V].

Control Above Maximum Candlepower: [Cutoff] [Semicutoff] [Noncutoff].

Installation Conditions:	[Wet location] [Outdoor use only] [Damp location] [Enclosed and gasketed] [_____________].

Mounting: [Provide pole mount bracket] [Wall mounting].

Ballast:	[Manufacturer's standard, matched to lamp characteristics, rated [120] [208] [277] [480] volts] [_____________].

Lamp: [One] [_____] each, rated [____] watts, [mercury vapor] [metal halide] [high pressure sodium] [low pressure sodium] [__________] type [coated] [clear] lamp.

****** [OR] ******

Lamp: [One] [_____] each, [____________________].

Accessories:

Provide photocell.

[______________________________].

Pole: [25 (8 m) foot tapered round aluminum pole with natural finish] [______________________________].

BALLASTS

Fluorescent Ballast:

[_________________________] Model [__________].

[_________________________] Model [__________].

[_________________________] Model [__________].

Substitutions: Under provisions of Section [01600] [___].

Description:	[ANSI C82.1, high power factor type electromagnetic ballast] [___].

Provide ballast suitable for lamps specified.

Voltage:	[[120] [277] [___] volts] [Match luminaire voltage].

Source Quality Control: Certify ballast design and construction by Certified Ballast Manufacturers, Inc.

High Intensity Discharge (HID) Ballast:

[_________________________] Model [__________].

[_________________________] Model [__________].

[_________________________] Model [__________].

Substitutions: Under provisions of Section [01600] [_____].

Description:	ANSI C82.4, [mercury vapor] [metal halide] [low pressure sodium] [high pressure sodium] lamp ballast.

Provide ballast suitable for lamp specified.

Voltage:	[[120] [208] [277] [480] volts] [Match luminaire voltage].

LAMPS

Incandescent Lamp Manufacturers:

[_________________________].

[_________________________].

[_________________________].

Substitutions: Under provisions of Section [01600] [_____].

Fluorescent Lamp Manufacturers:

[_________________________].

[_________________________].

[_________________________]

Substitutions: Under provisions of Section [01600] [_____].

High Intensity Discharge (HID) Lamp Manufacturers:

[_________________________].

[_________________________].

[_________________________].

Substitutions: Under provisions of Section [01600] [_____].

Provide lamp type specified for luminaire.

Reflector Lamp Beam Patterns: ANSI C78.379.

POLES

Manufacturers:

[_________________________] Model [__________].

[_________________________] Model [__________].

[_________________________] Model [__________].

Substitutions: Under provisions of Section [01600] [____].

Material and Finish: [__________________].

Section Shape and Dimensions: [Round] [Tapered round]

[Square] [___].

Height: [[25] [___] feet ([8] [___] m)] [As indicated on Drawings] [As scheduled].

Base: [[Breakaway,] [Nonbreakaway,][transformer type] [___________________________]] [Direct embedded type].

Accessories:

Handhole.

[__________________________________].

Loading Capacity Ratings:

Luminaire Weight: [___] pounds ([___] kg).

Luminaire and Bracket Effective Projected Area: [___] square feet ([___] square meters).

Steady Wind:	[_____] miles per hour ([_____] kph), minimum.

PART 3 EXECUTION

EXAMINATION

Examine excavation [and concrete foundation] for lighting poles.

Examine each luminaire to determine suitability for lamps specified.

INSTALLATION

Install in accordance with manufacturers' instructions.

Install lighting poles at locations indicated.

Install poles plumb.	[Provide [shims] [double nuts] to adjust plumb. Grout around each base.]

Install lamps in each luminaire.

Bond luminaires [,metal accessories] [and] [metal poles] to branch circuit equipment grounding conductor. [Provide supplementary grounding electrode at each pole.]

FIELD QUALITY CONTROL

Operate each luminaire after installation and connection. Inspect for improper connections and operation.

Measure illumination levels [to verify conformance with performance requirements].

Take measurements during night sky, without moon or with heavy overcast clouds effectively obscuring moon.

ADJUSTING

Adjust work under provisions of Section [01700] [_____].

Aim and adjust luminaires to provide illumination levels and distribution [indicated on Drawings] [as directed].

Relamp luminaires [which have failed lamps] at Date of Substantial Completion.

CLEANING

Clean work under provisions of Section [01700] [_____].

Clean electrical parts to remove conductive and deleterious materials.

Remove dirt and debris from enclosure.

Clean photometric control surfaces as recommended by manufacturer.

Clean finishes and touch up damage.

SCHEDULE

Type A Exterior Luminaire:

ABC Company Model XYZ.

Isocandela Corporation Catalog No. 123A456, with No. 5443 pole.

Clunk Luminaire Company Type XY-45.

Description: Roadway type luminaire.

Material: Aluminum housing.

Photometric Performance:	ANSI/IES RP-8, short vertical and Type III lateral distribution, with cutoff above maximum candlepower.

Installation Conditions:	Pole height greater than 25 feet.

Mounting: Provide pole mount bracket.

Ballast: Manufacturer's standard, rated 208 volts.

Lamp: 250 watts, high pressure sodium, clear.

Provide photocell.

Pole: 35 foot round aluminum pole with bronze anodized finish.

Type B Exterior Luminaire:

Church Brass Company Model 80867.

Johnson Lighting, Inc. Catalog No. 703-684-0300.

Watson, Ltd. Canadienne Series.

Description: Area flood type luminaire.

Size: 18 inches square by 5 inches deep.

Material: Extruded aluminum housing with cast aluminum trim.

Enclosure:	Clear glass, fully gasketed.

Photometric Control:	Anodized specular aluminum reflector.

Installation Conditions: Wet Location.

Mounting: Wall mounting.

Ballast: Manufacturer's standard, matched to lamp characteristics, rated 208 volts.

Lamp: 150 watts, metal halide type coated lamp.

END OF SECTION