SECTION 16535

EMERGENCY LIGHTING EQUIPMENT

PART 1 GENERAL

WORK INCLUDED

Emergency lighting units.

Emergency exit signs.

Emergency fluorescent lamp power supplies.

REFERENCES

FS W-L-305 - Light Set, General Illumination (Emergency or Auxiliary)

NFPA 101 - Code for Safety to Life from Fire in Buildings and Structures

NEMA WD1 - General-Purpose Wiring Devices.

REGULATORY REQUIREMENTS

Conform to [[local] [__________] building code] [NFPA 101] for installation requirements.

SUBMITTALS

Submit product data under provisions of Section [01300.] [01340.]

Provide product data on emergency lighting units, exit signs, and emergency fluorescent lamp power supply units.

PART 2 PRODUCTS

ACCEPTABLE MANUFACTURERS - INCANDESCENT EMERGENCY LIGHTING UNITS

[________________________________________.]

[________________________________________.]

[________________________________________.]

Substitutions: Under provisions of Section [01600.] [01630.]

INCANDESCENT EMERGENCY LIGHTING UNITS

Emergency Lighting Unit: [FS W-L-305; Type I, Class I, Style [D] [_____].] [Self-contained unit with rechargeable

storage batteries, charger, and lamps.]

Battery: [6] [12] volt, [nickel-cadmium] [lead calcium] [_____] type, with 1.5 hour capacity to supply the connected lamp load.

Charger: Dual-rate charger, capable of maintaining the battery in a full-charge state during normal conditions, and capable of recharging discharged battery to full charged within 12 hours.

Lamps: [12] [_____] Watt minimum, [sealed beam type in nickel or chrome plated steel housing.]

Remote Lamps: [Match lamps on unit.] [_______________.]

Unit Housing: Steel with [gray] [bronze] hammer tone finish [and vinyl wood grain front panel].] [White plastic.] [________________________________________.]

Indicators: Provide lamps to indicate AC ON and RECHARGING. [Provide voltmeter.]

Provide switch to transfer unit from normal supply to battery supply.

Accessories: [___________________________________.]

Electrical Connection: [6 foot (2 m) cord with NEMA WD 1, Type 5-15P cap.] [Knockout for conduit connection.]

Unit Voltage: [120] [277] volts, AC.

ACCEPTABLE MANUFACTURERS - SELF-CONTAINED EMERGENCY POWER EXIT SIGNS

[________________________________________.]

[________________________________________.]

[________________________________________.]

Substitutions: Under provisions of Section [01600.] [01630.]

SELF-CONTAINED EMERGENCY POWER EXIT SIGNS

Type: Exit signs with integral battery-operated emergency power supply, including power failure relay, test switch, AC ON pilot light, battery, and fully-automatic two-rate charger.

Battery: Sealed lead acid or lead calcium cell, requiring no maintenance or replacement for [10] [_____] years under normal conditions.

ACCEPTABLE MANUFACTURERS - EMERGENCY FLUORESCENT LAMP POWER SUPPLY

[________________________________________.]

[________________________________________.]

[________________________________________.]

Substitutions: Under provisions of Section [01600.] [01630.]

EMERGENCY FLUORESCENT LAMP POWER SUPPLY

Unit: Self-contained, with automatic transfer to battery supply on power failure, including test switch, AC ON pilot light, fully-automatic two-rate charger, battery, and power supply capable of operating a F40CW lamp with a minimum output of 600 lumens.

Battery: Sealed lead acid or lead calcium cell, requiring no maintenance or replacement for [10] [_____] years under normal conditions.

PART 3 EXECUTION

INSTALLATION

Install units plumb and level.

Aim directional lampheads as directed.

END OF SECTION