SECTION 16722

INTRUSION DETECTION AND SECURITY ACCESS SYSTEM

PART 1 GENERAL

SECTION INCLUDES

Intrusion detection devices.

Alarm control panel.

Signaling devices.

Security access devices.

Access control panel.

RELATED WORK

Section 08712 - Door Hardware.

Section 16120 - Wire and Cable.

REFERENCES

NFPA 72G - Notification Appliances for Protective Signaling Systems.

NFPA 72H - Guide for Test Procedures for Protective Signaling Systems.

SYSTEM DESCRIPTION

Intrusion Detection System: Protect building and selected areas from intrusion during SECURE hours as follows:

Exterior Windows: [________________________________.]

Exterior Doors: [__________________________________.]

[________________]: [______________________________.]

Security Access System: Control access to [building] [and] [selected areas] using [encoded cards.] [coded keypads.]

Selected Exterior Doors: Control access [into] [and] [out of] building.

Selected Building Areas: Control access [into] [and] [out of] [______________________________.]

QUALITY ASSURANCE

Manufacturer: Company specializing in [intrusion detection] [and] [security access] systems with [three] [_____] years experience.

Installer: Company specializing in [Intrusion detection] [and] [security access] systems with [three] [_____] years experience.

SUBMITTALS

Submit under provisions of Section [01300.] [_____.]

Shop Drawings: Indicate layout, wiring diagrams, and dimensions.

Product Data: Provide data sheets for each item of equipment, equipment ratings, and for finishes.

Manufacturer's Installation Instructions: Indicate installation instructions.

Manufacturer's Certificate: Certify that system meets or exceeds [specified requirements.] [____________________.]

Manufacturer's Field Reports: Submit under provisions of Section [01400.] [_____.]

Manufacturer's Field Reports: Indicate that system is operational.

RECORD DRAWINGS

Submit under the provisions of Section [01700.] [_____.]

Accurately indicate actual location of detection and signaling devices, and end-of-line devices.

OPERATION AND MAINTENANCE DATA

Submit under provisions of Section [01700.] [_____.]

Operation Data: Include operating instructions.

Maintenance Data: Include maintenance and repair procedures.

PART 2 PRODUCTS

MANUFACTURERS

[_____________________________________________.]

[_____________________________________________.]

[_____________________________________________.]

Substitutions: Under provisions of Section [01600.] [_____.]

ALARM CONTROL PANEL

Control Panel: Modular construction with [flush] [surface] wall-mounted enclosure.

Power Supply: Adequate to serve control panel modules, [remote detectors,] [remote annunciators,] [relays,] and alarm signaling devices. [Include battery-operated emergency power supply with capacity for operating system in standby mode for [24] [___] hours.]

System Supervision: Provide electrically-supervised system, with supervised alarm initiating and alarm signaling circuits. Occurrence of single ground or open condition in a circuit places circuit in ALARM mode. Component or power supply failure places system in ALARM mode. Occurrence of single ground or open condition on alarm initiating circuit does not disable that circuit from transmitting in ALARM.

Detection Circuits: Supervised zone module with alarm and trouble indication.

Signal Circuits: Supervised [zone coded] signal module, sufficient for signal devices connected to system.

Remote Station Signal Transmitter: Electrically supervised, capable of transmitting alarm and trouble signals over telephone lines to remote station receiver.

Remote Station Signal Receiver: Electrically supervised, capable of receiving signals from remote station transmitter over telephone lines with up to [4000] [____] ohms loop resistance, and visually annunciating alarm signals [by zone] and common trouble signal. Include circuit for remote audible alarm and trouble signal, accessory alarm and trouble relays with SPDT contacts, and separate manual alarm and trouble SILENCE functions.

Auxiliary Relays: Provide sufficient SPDT auxiliary relay contacts [for each detection zone] to provide accessory functions specified.

Alarm Sequence of Operation: Actuation of intrusion detecting device causes system to enter ALARM, which includes the following operations:

Sound and display local alarm signaling devices with non-coded signal.

Transmit [non-coded] [zone-coded] signal to [municipal connection.] [remote station equipment.]

Indicate location of actuated device on control panel[.] [and on remote annunciator panel.]

[__________________________________________________.]

Alarm Reset: Key-accessible RESET function resets alarm system out of ALARM if alarm initiating circuits have cleared.

Lamp Test: Manual LAMP TEST function causes alarm indication at each zone at control panel[.] [and at annunciator panel.]

INITIATING DEVICES

Magnetic Switch: [______________________________________.] [Manufacturer and model: [_____________________________.]]

Proximity Switch: [_____________________________________.] [Manufacturer and model: [_____________________________.]]

Motion Detector: [______________________________________.] [Manufacturer and model: [_____________________________.]]

Photoelectric Detector: [_______________________________.] [Manufacturer and model: [_____________________________.]]

Pressure Mats: [________________________________________.] [Manufacturer and model: [_____________________________.]]

Foil Screen: [__________________________________________.] [Manufacturer and model: [_____________________________.]]

Floor Trap: [___________________________________________.] [Manufacturer and model: [_____________________________.]]

Vibration Detector: [___________________________________.] [Manufacturer and model: [_____________________________.]]

Audio Detector: [_______________________________________.] [Manufacturer and model: [_____________________________.]]

SIGNAL DEVICES

Alarm Bells: NFPA 72G; Electric [vibrating,] [single stroke,] [8] [10] [___] inch ([200] [250] [___] mm) with bell operating mechanism behind dome. Sound Rating: [81] [___] dB at 10 ft (3 m).

Remote annunciator: Provide [supervised] remote annunciator including audible and visual indication of intrusion [by zone], and audible and visual indication of system trouble. Install in [flush] [surface] wall-mounted enclosure. [Manufacturer and model: [_________________.]]

SECURITY ACCESS SYSTEM

Security Access Control Panel: [_______________________.] [Manufacturer and model: [_____________________________.]]

Encoded Card Reader: [__________________________________.] [Manufacturer and model: [_____________________________.]]

Encoded Card Controller: [______________________________.] [Manufacturer and model: [_____________________________.]]

Key Pad Unit: [_________________________________________.] [Manufacturer and model: [_____________________________.]]

Electric Strike: [______________________________________.] [Manufacturer and model: [_____________________________.]]

Electric Lock: [________________________________________.] [Manufacturer and model: [_____________________________.]]

PART 3 EXECUTION

INSTALLATION

Install system in accordance with manufacturer's instructions.

Install wiring for detection and signal circuit conductors in [conduit.] [cable.] Use [16] [14] AWG minimum size conductors.

Make conduit and wiring connections to door hardware devices furnished and installed under Section 08712.

FIELD QUALITY CONTROL

Field [inspection and] testing will be performed under provisions of Section [01400.] [_____.]

Test in accordance with NFPA 72H.

MANUFACTURER'S FIELD SERVICES

Provide manufacturer's field services under provisions of Section [01400.] [_____.]

Include services of technician to supervise installation, adjustments, final connections, and system testing.

END OF SECTION