SECTION 02516

ASPHALTIC BLOCK PAVERS

PART 1 GENERAL

SECTION INCLUDES

Asphaltic [block] [plank] pavers and adhesive.

RELATED SECTIONS

Section [______-____________]:	Stabilized base.

Section 02510 - Asphaltic Concrete Paving: Asphalt substrate [and extruded asphalt curbs].

Section 02514 - Portland Cement Concrete Paving:	Concrete substrate.

Section [02526 - Precast Concrete Parking Curbs] [______-____________]: [Concrete] [Timber] [________] parking curbs.

Section 05800 - Expansion Control.

Section [______-____________]:	Floor drains.

UNIT PRICE - MEASUREMENT AND PAYMENT

Asphalt [Block] [Plank] Pavers:

Basis of Measurement: By the square [foot] [________] ([meter] [________]).

Basis of Payment: Includes preparation of substrate, priming, placing pavers, finishing.

SUBMITTALS

Submit under provisions of Section [01300.] [________.]

Product Data: Provide characteristics of paver unit, dimensions, and special shapes.

Samples:	Submit [two] [_______] samples of each paver size, illustrating style, size, color range and surface texture of units being provided.

Manufacturer's Installation Instructions: Indicate substrate requirements, installation methods, and [________].

MAINTENANCE DATA

Submit under provisions of Section [01700.] [________.]

Maintenance Data: Provide data for Owner's continuing maintenance of the paver surface, replacement of paver units, and surface wax maintenance requirements.

EXTRA MATERIALS

Furnish under provisions of Section [01700.] [________.]

Provide [10] [____] of each paver size.

PART 2 PRODUCTS

MANUFACTURERS

[__________________________________] Product [_________].

[__________________________________] Product [_________].

[__________________________________] Product [_________].

Substitutions: Under provisions of Section [01600.] [________.]

MATERIALS

Pavers: Fibrous asphaltic [block] [plank]; [____x____x____] inches ([____x____x____] mm) size; [natural] [exposed aggregate] [sand blasted] finish of [________] color.

Adhesive: [Neoprene modified] asphaltic type, recommended by paver manufacturer.

[Primer] [Surface Conditioner]: [________________].

Joint Filler: Portland cement and clean sand.

Surface Wax: [________________].

PART 3 EXECUTION

EXAMINATION

Verify substrate conditions under provisions of Section [01039.] [________.]

Verify that substrate is level, smooth, capable of supporting pavers and imposed loads, and ready to receive work of this Section.

Verify gradients and elevations of substrate are correct.

PREPARATION

Apply [primer] [surface conditioner] to surface of substrate in accordance with manufacturer's instructions.

INSTALLATION

Apply adhesive and pavers in accordance with manufacturer's instructions.

Place paver units in [herring bone] [ashlar] [running bond] [________] pattern, from straight reference edge.

Place half units or special shaped units at edges and interruptions. Maintain tight joints.

Machine roll units to level surface.

Sweep a dry mixture of one part Portland cement and three parts sand into paver joints.

Fog spray surfaces with water to ensure wetting of joint filler.

Sweep excess filler from surface of pavers.

Apply surface wax.

END OF SECTION