SECTION 06200

FINISH CARPENTRY

PART	GENERAL

SECTION INCLUDES

Finish carpentry items, other than shop prefabricated casework.

Hardware and attachment accessories.

PRODUCTS FURNISHED BUT NOT INSTALLED UNDER THIS SECTION

Section [______-____________]: Installation of recessed wood blocking and [__________.]

Section [______-____________]: Installation of [attachment accessories.] [_________.]

PRODUCTS INSTALLED BUT NOT FURNISHED UNDER THIS SECTION

Section [______-____________]: Supply of [hardware] [attachment accessories] [and] [__________] to this section.

Section [______-____________]: [Boxes] [Trim] for recessed [components.] [__________.]

RELATED SECTIONS

Section [______-____________]: [Stone] [Cast plastic] [__________] window stools.

Section 06114 - Wood Blocking and Curbing: Grounds and support framing.

Section 06410 - Custom Casework: Shop fabricated custom cabinet work.

Section 06423 - Wood Veneer Faced Paneling: Shop fabricated custom paneling.

Section 08211 - Flush Wood Doors.

Section 08212 - Stile and Rail Wood Doors.

Section 08610 - Wood Windows.

Section 08800 - Glazing: [Glass and glazing of [wood partitions screens] [________].] [Glass shelves.] [________.]

Section 09900 - Painting: Painting and finishing of finish carpentry items.

Section 12370 - Residential Casework: Shop fabricated cabinet work.

REFERENCES

ANSI A135.4 - Basic Hardboard.

ANSI A208.1 - Mat Formed Wood Particleboard.

ASTM E84 - Test Method for Surface Burning Characteristics of Building Materials.

AWI - Quality Standards.

AWPA (American Wood Preservers Association) C2 - Lumber, Timbers, Bridge Ties and Mine Ties - Preservative Treatment by Pressure Processes.

AWPA (American Wood Preservers Association) C20 - Structural Lumber Fire Retardant Treatment by Pressure Process.

BHMA A156.9 - Cabinet Hardware.

FS MMM-A-130 - Adhesive, Contact.

HPMA (Hardwood Plywood Manufacturer's Association) HP - American Standard for Hardwood and Decorative Plywood.

NEMA (National Electric Manufacturers Association) LD3 - High Pressure Decorative Laminates.

NHLA (National Hardwood Lumber Association).

NWWDA (National Wood Window and Door Association) I.S.4 - Water Repellant Preservative Treatment for Millwork.

PS 1 - Construction and Industrial Plywood.

PS 20 - American Softwood Lumber Standard.

SUBMITTALS

Submit under provisions of Section [01300.] [________.]

Shop Drawings: Indicate materials, component profiles, fastening methods, jointing details, accessories, and [________], to a minimum scale of [1-1/2 inch to 1 ft] [________] ([1:8] [_____]).

Product Data: Provide data on fire retardant treatment materials and application instructions.

Provide instructions for [attachment hardware,] [finish hardware,] [and] [________].

Samples: Submit [two] [____] samples of finish plywood, [____x____] inch ([____x____] mm) in size illustrating wood grain and specified finish.

Submit [two] [_____] samples of wood trim [____] inch ([____] mm) long.

QUALITY ASSURANCE

Perform work in accordance with [AWI [Premium] [Custom] [Economy] quality.] [NHLA.]

QUALIFICATIONS

Fabricator: Company specializing in fabricating the products specified in this section with minimum [three] [_______] years [documented] experience.

REGULATORY REQUIREMENTS

Conform to [applicable] [________] code for [fire retardant] [________] requirements.

DELIVERY, STORAGE, AND HANDLING

Deliver, store, protect and handle products to site under provisions of Section [01600.] [________.]

Protect work from moisture damage.

FIELD MEASUREMENTS

Verify that field measurements are as [indicated [on shop drawings]] [instructed by the manufacturer].

COORDINATION

Coordinate work under provisions of Section [01039.] [________.]

Coordinate the work with [plumbing] [and] [electrical] rough-in, installation of associated and adjacent components, [and] [________].

PART	PRODUCTS

FABRICATORS

[__________________________________].

[__________________________________].

[__________________________________].

Substitutions: Under provisions of Section [01600.] [________.]

LUMBER MATERIALS

Softwood Lumber: [PS 20;] Graded in accordance with AWI [Economy] [Custom] [Premium]; [________] species, [________] sawn, maximum moisture content of [6] [____] percent; with [vertical] [mixed] [flat] grain [, of quality suitable for transparent finish].

Hardwood Lumber: Graded in accordance with AWI [Economy] [Custom] [Premium]; [________] species, [________] sawn, maximum moisture content of [6] [8] [11] percent; with [vertical] [mixed] [flat] [plain sawn] [__________] grain [, of quality suitable for transparent finish].

SHEET MATERIALS

Softwood Plywood: [PS 1 Grade [C-D] [____];] Graded in accordance with AWI [Economy] [Custom] [Premium]; [veneer] [lumber] [particleboard] core; [________] face species, [________] cut.

****** [OR] ******

Hardwood Plywood: [HPMA HP Grade [____] Type [____];] Graded in accordance with AWI [Economy] [Custom] [Premium]; [veneer] [lumber] [particleboard] core, type of glue recommended for application; [________] face species, [________] cut.

Prefinished Paneling: [________] face species, [________] cut, [________] grain, [V-cut vertical joint scoring]; [3/16] [1/4] [____] inch ([4] [6] [____] mm) thick; [________] manufactured by [____________].

Wood Particleboard: [ANSI A208.1 Type [1] [2];] AWI standard, composed of wood chips, [medium] [________] density, made with [high waterproof resin binders] [water resistant adhesive]; of grade to suit application; sanded faces.

Hardboard: [ANSI A135.4;] Pressed wood fiber with resin binder, [standard] [tempered] grade, [1/4] [____] inch ([6] [____] mm) thick, smooth [one] [two] sides.

Pegboard: Pressed wood fiber with resin binder, [standard] [tempered] grade; [1/8 inch (3 mm) thick with 3/16 inch (4 mm) diameter holes at 1 inch (25 mm) on center.] [1/4 inch (6 mm) thick with 9/32 inch (7 mm) diameter holes at 1 inch (25 mm) on center.]

PLASTIC LAMINATE MATERIALS

Plastic Laminate: AWI, [[0.040] [____] inch ([1] [____] mm) Post Forming] [[0.050] [____] inch ([1.3] [____] mm) General Purpose] [________] quality; [________] color, [________] pattern, and [gloss] [matte] [textured] [furniture] [________] surface texture [as selected]; [________] manufactured by [____________].

****** [OR] ******

Plastic Laminate: NEMA LD 3, [PF 42 Post Forming] [GP - [50] [33] General Purpose] [________] type; [________] color, [________] pattern, and [gloss] [matte] [textured] [furniture] [________] surface texture [as selected].

****** [OR] ******

Low Pressure Laminate: [Melamine] [________]; [________] color, [________] pattern, and [gloss] [matte] [textured] [furniture] [________] surface texture [as selected].

****** [OR] ******

Solid Laminate: [________] color, [________] pattern, and [gloss] [matte] [textured] [furniture] [________] surface texture [as selected].

Laminate Backing Sheet: [0.020] [____] inch ([0.5] [____] mm) Backing Sheet grade, undecorated plastic laminate; [________] manufactured by [____________].

***** [OR] *****

Laminate Backing Sheet: NEMA LD-3 BK20 backing grade, undecorated plastic laminate.

ADHESIVE

Adhesive: [FS MMM-A-130 contact adhesive.] [Type recommended by [AWI] [laminate manufacturer] to suit application.] [________.]

****** [OR] ******

Adhesive: [Urea-formaldehyde resin] [Contact cement] [Resorcinol formaldehyde] [Polyvinyl acetate] [Casein] [________]; [________] manufactured by [____________].

FASTENERS

Fasteners: Of size and type to suit application; [________] finish in concealed locations and [________] finish in exposed locations.

Concealed Joint Fasteners: Threaded steel.

ACCESSORIES

Lumber for Shimming, Blocking, and [________]: Softwood lumber of [________] species.

Plastic Edge Trim: Extruded [convex] [flat] shaped; [smooth] [ridged] finish; self locking serrated tongue; of width to match component thickness; [________] color [as selected].

****** [OR] ******

Aluminum Edge Trim: Extruded [convex] [flat] shape; [smooth] [ridged] surface finish; self locking serrated tongue; of width to match component thickness; [natural mill] [clear anodized] [bronze anodized] [________] finish.

Glass: Type [A] [____], as specified in Section 08800.

****** [OR] ******

[Float] [Patterned] Glass: [Clear] [[________] pattern], [________] quality; [____] inch ([____] mm) thick [minimum].

****** [OR] ******

Safety Glass: [Clear] [________]; [heat strengthened] [fully tempered] [laminated] [________]; [____] inch ([____] mm) thick [minimum].

****** [OR] ******

Wire Glass: [Clear] [________], polished [both sides] [one side]; [square] [diagonal] [________] mesh of woven stainless steel wire of [1/2] [____] inch ([12] [____] mm) grid size; [1/4] [____] inch ([6] [____] mm) thick.

Primer: [Alkyd primer sealer] [________] type.

Wood Filler: [Solvent] [Oil] base, tinted to match surface finish color.

WOOD TREATMENT PROCESSES

Fire retardant (FR-S Type): Chemically treated and pressure impregnated; capable of providing a maximum flame spread/smoke development rating of [____] / [____] in accordance with ASTM E84; [________] manufactured by [____________].

Wood Preservative by Pressure Treatment (PT Type): [AWPA Treatment C2] using [water borne] [_____________] preservative with [0.25] [_____] percent retainage.

Wood Repellant Preservative Treatment by Dipping Method: NWWDA I.S.4, with [0.25] [_____] percent retainage.

Wood Preservative (Surface Application): [Clear] [colored], [_____________] type, [________] manufactured by [____________].

SHOP TREATMENT OF WOOD MATERIALS

Shop [pressure treat] [dip] [brush apply] treatment to wood materials requiring [UL fire rating] [preservatives] to [concealed wood blocking.] [________.]

Provide UL approved identification on fire retardant treated material.

Deliver fire retardant treated materials cut to required sizes. Minimize field cutting.

[Redry] [Kiln dry] wood after pressure treatment to maximum [____] percent moisture content.

HARDWARE

Hardware: BHMA A156.9 as follows:

Hinges: [________] style, [________] finish.

Pulls: [________] style, [________] finish.

Latches: [________] style, [________] finish.

Shelf Standards: [________] style, [________] finish.

Shelf Brackets: [________] style, [________] finish.

Drawer Slides: [________] style, [________] finish.

****** [OR] ******

Hinges: [________] style, [________] finish; [________] manufactured by [____________].

Pulls: [________] style, [________] finish; [________] manufactured by [____________].

Latches: [________] style, [________] finish; [________] manufactured by [____________].

Shelf Standards: [________] style, [________] finish; [________] manufactured by [____________].

Shelf Brackets: [________] style, [________] finish; [________] manufactured by [____________].

Drawer Slides: [________] style, [________] finish; [________] manufactured by [____________].

FABRICATION

Fabricate to [AWI [Economy] [Custom] [Premium] standards.] [________].

Shop assemble work for delivery to site, permitting passage through building openings.

Fit exposed sheet material edges with [3/8 inch (9.5 mm) matching hardwood] [matching veneer] [plastic] [aluminum] edging. Use one piece for full length only.

Cap exposed plastic laminate finish edges with [material of same finish and pattern] [plastic trim] [aluminum trim] [________].

Shop prepare and identify components for [book match] [________] grain matching during site erection.

When necessary to cut and fit on site, provide materials with ample allowance for cutting. Provide trim for scribing and site cutting.

Apply plastic laminate finish in full uninterrupted sheets consistent with manufactured sizes. Fit corners and joints hairline; secure with concealed fasteners. [Slightly bevel arises]. [Locate counter butt joints minimum [2] [____] feet ([600] [____] mm) from sink cut-outs.]

Apply laminate backing sheet to reverse side of plastic laminate finished surfaces.

SHOP FINISHING

Sand work smooth and set exposed nails [and screws].

Apply wood filler in exposed nail [and screw] indentations.

[On items to receive transparent finishes, use wood filler which matches surrounding surfaces and of types recommended for applied finishes.]

Finish work in accordance with AWI - Section 1500 System [#1] [#2] [#3] [#4] [#5] [#6] [#7] [#8] [#9] [#10] [#11] [#12] [#13].

****** [OR] ******

Seal [, stain] and varnish exposed to view surfaces. Brush apply only.

Seal [, stain] and varnish semi-exposed to view surfaces. Brush apply only.

[Prime paint] [Seal] surfaces in contact with cementitious materials.

PART	EXECUTION

EXAMINATION

Verify adequacy of backing and support framing.

Verify mechanical, electrical, and building items affecting work of this section are placed and ready to receive this work.

INSTALLATION

Install work in accordance with AWI [Economy] [Custom] [Premium] Quality Standard.

Set and secure materials and components in place, plumb and level.

Carefully scribe work abutting other components, with maximum gaps of [1/32] [____] inch ([1] [____] mm). Do not use additional overlay trim to conceal larger gaps.

Install [components] [trim] [________] with [[nails] [screws] [bolts with blind fasteners] at [____] inch ([____] mm) on center.] [wall adhesive by gun application.] [________.]

[Install prefinished paneling with [full bed contact adhesive applied to substrate.] [[nails] [screws] [wall adhesive by the bead method] at [____] inch ([____] mm) on center.]

Install hardware [supplied by Section [________].] [in accordance with manufacturer's instructions.]

SITE APPLIED WOOD TREATMENT

Apply preservative treatment in accordance with manufacturer's instructions.

Brush apply [one] [two] coats of preservative treatment on wood in contact with [cementitious materials] [roofing and related metal flashings] [and] [_________]. [Treat site-sawn cuts.]

Allow preservative to dry prior to erecting members.

PREPARATION FOR SITE FINISHING

Set exposed fasteners. [Apply wood filler in exposed fastener indentations.] Sand work smooth.

****** [OR] ******

Site Finishing: Refer to Section [09900.] [________.]

Before installation, prime paint surfaces of items or assemblies to be in contact with cementitious materials.

ERECTION TOLERANCES

Maximum Variation from True Position: [1/16] [____] inch ([1.5] [____] mm).

Maximum Offset from True Alignment with Abutting Materials: [1/32] [____] inch ([0.7] [____] mm).

SCHEDULE

Exterior:

Enclosing Structural Members: Softwood lumber; "PT" preservative treat.

Brackets, Finials, and Pediments: Prepare for paint finish.

Enclosing Soffit Spaces: As detailed.

Handrails: Redwood; prepare for stained and sealed finish.

Bench Seats and Backs: "PT" preservative treat.

Soffits and Facias: Prepare for paint finish.

Window Casings and Moldings: Softwood; prepare for paint finish.

Interior:

Door, Glazed Light, and Pocket Door Frames: White birch; prepare for paint finish.

Window Sills: Clear fir; prepare for transparent finish.

Suspended Wood Ceiling System: "FR-S" treated.

Glazed Screen Partition System: Clear fir; prepare for transparent finish.

On-site Constructed Stairs, Balustrades, and Handrails: Clear fir; prepare for stained finish.

Moldings, Bases, Casings, and Miscellaneous Trim: Clear white pine; prepare for paint finish.

Valance Work: Clear fir; prepare for paint finish.

Loose Shelving: Birch plywood; prepare for paint finish.

False Box Beams: Knotty Tight Knot Cedar; unfinished.

END OF SECTION