SECTION 15181

CONDENSATE DRAIN PIPING

PART 1 GENERAL

1.1	SUMMARY

A.	Includes But Not Limited To

1.	Furnish and install condensate drain piping as described in Contract Documents.

B.	Related Sections

1.	Section 15051 - General Mechanical Requirements

PART 2 PRODUCTS

2.1	MATERIALS

A.	Condensate Drains

1.	Type M copper or Schedule 40 PVC for condensate drains from roof top units.

2.	3 inch deep seal, water trap with vacuum breaker adjacent to cooling coil connection.

2.2	MANUFACTURED UNITS

A.	Condensate Pump

1.	Rated at 225 gph at 15 feet total head. Complete with one gallon polystyrene tank with pump and automatic float control. 1/5 HP, 120 volt, one phase, 60 Hertz.

2.	Condensate piping shall be Type M copper, no plastic tubing allowed.

3.	Approved Manufacturers -

a.	Little Giant No. VCL45S

b.	Beckett No. CU551UL

PART 3 EXECUTION

3.1	INSTALLATION

A.	Condensate Drains

1.	Support piping and protect from damage.

2.	Coordinate installation of piping with pipe supports detailed on architectural drawings.

3.	Maintain minimum slope as required per code.

END OF SECTION