SECTION 15826

FIRE DAMPERS

PART 1 GENERAL

1.1	SUMMARY

A.	Includes But Not Limited To

1.	Furnish and install fire described in Contract Documents.

B.	Related Sections

1.	Section 15051 - General Mechanical Requirements

1.2	QUALITY ASSURANCE

A.	Requirements of Regulatory Agencies

1.	Dampers shall conform to NFPA and SMACNA requirements and bear UL label.

2.	Dampers shall be approved by fire authorities having jurisdiction where so required.

3.	Wall fire dampers shall conform to UL 555 'Fire Damper Test Standard'

1.3	MAINTENANCE

A.	Extra Materials - Leave one fusible links of each rating type used on Project with Owner.

PART 2 PRODUCTS

2.1	MANUFACTURED UNITS

A.	Fire Dampers

1.	Walls (Type 1) -

a.	Type 'B', blades out of airstream

b.	Include integral sleeve

c.	165 deg F link unless otherwise indicated on Drawings

b.	Approved Manufacturers And Models -

1)	Air Balance Inc - Model 119BLX

2)	Greenheck - Model FD150XB

3)	Potorff - Model VFD-10 ISB, D-ISB

4)	Ruskin - Model IBD20B

5)	Safe Air Inc - Model 150B Sleeved

6)	Equals by Cesco or Prefco as approved by Architect before bidding. See Section 01600.

PART 3 EXECUTION

3.1	INSTALLATION

A.	Install fire dampers in ducts where ducts penetrate fire rated walls and floors.

END OF SECTION