STANDARD	1 Aug 1998	15853

UPDATES -

SECTION 15853

ROOF-MOUNTED AIR INLETS AND OUTLETS

PART 1 GENERAL

1.1	SUMMARY

A.	Includes But Not Limited To

1.	Furnish and install roof vents as described in Contract Documents.

B.	Related Sections

1.	Section 15051 - General Mechanical Requirements	15051

PART 2 PRODUCTS

2.1	MANUFACTURED UNITS

A.	Roof Vents

1.	Penthouse type of extruded aluminum complete with roof curb to fit slope of roof and 1/2 inch mesh 16 gauge aluminum bird screen.

2.	Finish as specified by Architect.

3.	Approved Models And Manufacturers -	Approved Products

a.	Tiered Type - Model TRE extruded aluminum ventilator by Loren Cook Company, Springfield, Missouri

b.	Louvered Penthouse -

1)	Model GLAB by Carnes Company, Verona, WI

2)	Model WRH by Greenheck Fan Corporation, Schofield, WI

3)	Model MPH by Jenn-Air Industries Inc, Indianapolis, IN

PART 3 EXECUTION - Not Used	Installation

END OF SECTION