# Project Quiznos #7680 1102 N. Hwy 190 Suite A. HVAC Calculations

Fri Apr 1 08:43:41 CST 2005

There is no calculation for North & Shaded Glass
There is no calculation for NorthEast and NorthWest Glass
The Btuh Gain for 138 SqFt of East and West Double Pane Glass = 13110
There is no calculation for SouthEast and SouthWest Glass
There is no calculation for South Glass
There is no calculation for SkyLights
The Btuh Gain for 40 SqFt of Windows in Doors = 528

The Btuh Gain for 588 SqFt of Mason Above Grade R-5 Wall Number 1 = 1822.8
The Btuh Gain for 437 SqFt of Wood R-11 & 1/2" Gypsum Wall Number 2 = 1136.2
There is no calculation for Wall Number 3
There is no calculation for Wall Number 4

The Btuh Gain for 1400 SqFt of Roof Only 5.25" - 6.5" R-19; Ceiling Number 1 = 7280

There is no calculation for Ceiling Number 2

There is no calculation for Floor Number 1
There is no calculation for Floor Number 2

The Btuh Gain for 38 People = 380

There is no calculation for Motor HP

There is no calculation for Ducts Out of Conditioned Spaces

The Btuh Gain for 1400 SqFt of Area Lighting in a Retail Store = 5600

There is no calculation for Coffee Machines
There is no calculation for Electric Food Warmers
There is no calculation for Gas Food Warmers
There is no calculation for Electric Fry Kettle
There is no calculation for Gas Fry Kettle
There is no calculation for Electric Griddle
There is no calculation for Gas Griddle
There is no calculation for Hair Dryer Helmets
There is no calculation for 4-Slice Toaster
38444 watts are being calculated for BTUh

There is no calculation for Outside Fresh Air #1
There is no calculation for Outside Fresh Air #2
There is no calculation for Outside Fresh Air #3
The Cafeteria or Fast Food Outside Fresh Air #4 = 640 cfm
The Btuh Gain for Outside Fresh Air #4 = 19200
The Kitchen Outside Fresh Air #5 = 90 cfm
The Btuh Gain for Outside Fresh Air #5 = 2700
There is no calculation for Outside Fresh Air #6

The Total Outside Fresh Air CFM = 730
This is in accordance with International Mechanical Code 2003

The Total BTUh Gain = 182466.6

The Total Tons of HVAC needed = 15.20555