| UNIT 3: INSTALLATION - LESSSON 6: STARTING THE SYSTEM Starting the System When starting the KX-TAW848 for the first time the System Initialization Procedure MUST be performed. The System Initialization Procedure clears all system programming that may be entered into memory, and loads the default settings. Once executed, other system programs can be changed to meet the needs of the users of the system. This procedure should only be executed when first installing the system. Once the system is initialized, this procedure should NOT be executed unless the programmer wants to clear all programming changes and return them to their default settings. To execute the System Initialization, follow these steps: Set the Power Switch to the “OFF” position and confirm the SD Card is installed. Set the System Clear Switch to the "SYSTEM INITIALIZE" position. Connect the AC and DC power cords and plug them into the system and an AC outlet accordingly Turn the Power Switch ON Press the reset button. (The run indicator will flash.) Slide the System Clear Switch to the “NORMAL” position while the power indicator is flashing (within approximately 10 seconds). The system is now initialized and ready for programming changes. (Depending on the configuration, initialization takes about 1 to 3 minutes. If successfully executed, the RUN indicator will stop flashing and be kept lit.) If trouble occurs during startup, please review section 4 of the Installation Manual.