| UNIT 2: HARDWARE & CONFIGURATION - LESSON 1: OPTIONAL SERVICE CARDS Slot Type B
MODEL # | DESCRIPTION | MAX # PER SYSTEM | SLOT TYPE
KX-TAW84874 | 8-Port Single Line Extension Card (SLC8) | 2 | Type B
| Provides for the connection of 8 single line devices. Includes 8 DTMF receivers. A maximum of 2 cards can be installed per system.
MODEL # | DESCRIPTION | MAX # PER SYSTEM | SLOT TYPE
KX-TAW84876 | 8-Port Proprietary Extension Card (PLC8) | 2 | Type B
| Provides for connection of KX-T7700 series telephones, KX-T7885 and KX-TD7895 wireless telephones, DSS consoles, and KX-TVS Voice Processing Systems. Each KX-TAW84875 adds 8 ports to the Main Unit. A maximum of 2 cards can be installed per system.
Option Slot
MODEL # | DESCRIPTION | MAX # PER SYSTEM | SLOT TYPE
KX-TAW84861 | 4-Port Doorphone Card (DPH4) | 1 | Option Slot 8 or 9 only
| Supports up to 4 KX-T30865 doorphones. Also equipped with 4 dry contacts for connection to electric door strikes or other compatible equipment. A maximum of 1 card can be installed per system.
MODEL # | DESCRIPTION | MAX # PER SYSTEM | SLOT TYPE
KX-TAW84866 | 8-Channel Echo Canceller Card (ECHO8) | 1 | Option
| Provides echo cancellation for conference calls for up to 16 ports. Required for conferences of six or more parties. A maximum of 1 card can be installed per system.
MODEL # | DESCRIPTION | MAX # PER SYSTEM | SLOT TYPE
KX-TAW84868 | Extension Caller ID Card (EXT-CID) | 1 | Option
| Required to pass Caller ID to single line devices. Supports up to 8 single line devices. A maximum of 1 card can be installed per system. Requires at least one KX-TAW84893 to be installed.
MODEL # | DESCRIPTION | MAX # PER SYSTEM | SLOT TYPE
KX-TAW84891 | 2-Channel Message Card (MSG2) | 2 | Option
| Provides 2 ports for outgoing DISA, queuing and Timed Reminder (wake up) messages. A maximum of 32 messages can be recorded with a total record time of 8 minutes. The maximum recording time of each message is one minute. A maximum of 2 cards can be installed per system. Each card can play two messages simultaneously. Adding a card increases the number of messages that can be played simultaneously, but does not increase the total recording time or the number of messages that can be recorded.