| UNIT 6: MULTI-CELL WIRELESS - LESSON 3: INSTALLATION & PROGRAMMING Registering Portable Stations The next step is to register the Portable Stations. The registration process establishes the initial communication between the Portable Station and the Cell Station. Registering a Portable Station is a two-step process. First, the registration process must be started by entering system programming, and then registering each Portable Station individually. It is suggested that you have all the Portable Stations that are to be registered at the same time you are programming using your Personal Computer. The programming location should also be in an area that has a Cell Station signal strength 8 or greater. Click here to see an example of how to use the Maintenance Console to register the Portable Stations The next step is to register each individual Portable Station. This process varies slightly between the KX-TD7680 and KX-TD7690. Register a KX-TD7680 To register a KX-TD7680, turn the KX-TD7680 on by holding the PWR button down for 5 seconds. After a few seconds the display will show: Press the button below the F3 indication. The display will show: Hold the F3 button down until the display indicates “EXECUTING”. After a few seconds the display will indicate “REGISTERED”. This Portable Station is now registered as an extension on this KX-TAW848. The display will indicate the date, time, and extension number as well as SCO indications above the three F-buttons. Register a KX-TD7690 To register a KX-TD7690, turn the KX-TD7690 on by holding the PWR button down for 5 seconds. After a few seconds press the MENU button. Then using the Navigation button, highlight PS PROGRAM and press the SEL button. Then use the Navigation button to highlight SYSTEM SETTING and press SEL. Highlight REGISTRATION and press SEL, then SYSTEM1 and SEL. The display will flash EXECUTING for a few seconds and then REGISTERED. This Portable Station is now registered as an extension on this KX-TAW848. The display will indicate the date, time, and extension number as well as MENU, KEY and FCO indications. Up to 28 Portable Stations can be registered on a KX-TAW848. Each Portable Station must be registered individually. Click here to see an example of how to use the Maintenance Console to configure a second Portable Station Now register the second Portable Station accordingly. Continue this process until all required Portable Stations are registered. Each Portable Station can be registered on up to 4 systems. The systems can be any of the Panasonic Telephone Systems supporting the Multi-Cell Wireless feature. These systems include the KX-TAW848, KX-TDA50, KX-TDA100 and KX-TDA200. For example, perhaps you have a KX-TAW848 installed in both your office and your residence. You could register the Portable Station on both systems and use the same Portable Station when at work or home.