| UNIT 6: MULTI-CELL WIRELESS - LESSON 3: INSTALLATION & PROGRAMMING Programming Portable Stations The Portable Station Menu includes three submenus, which are used to customize the Portable Stations used on the system. The first submenu is the Extension Settings Menu which contains 8 tabs used to navigate the various programming fields. In a typical installation only a few fields will need to be modified, however some applications may require greater flexibility and require more complex programming. One field that should always be customized is the Extension Name. Each Portable Station can have a name (20 characters) assigned to it. The name appears as a reference on all programming screens and is displayed on proprietary display telephones when intercom calls are made or received. Click here to see an example of the Wireless Extension Settings Menu The FWD/DND screen allows the system programmer to set the DND and FWD features for the PS user. The Flexible Key screen allows the flexible CO buttons to be customized to allow one-touch access to a certain feature. A maximum of 12 flexible CO buttons can be customized for each PS. Available options include: Not Stored, Loop CO, Single CO, Group CO, DSS, One-touch, G-DN, Message Waiting, FWD/DND (Both), FWD/DND (External), FWD/DND (Internal), Group FWD (Both), Group FWD (External), Group FWD (Internal), Account, Conference, Terminate, EFA, Call Park, Log-in/Log-out, Hurry-up, Wrap-up, Time Service, TRS Level Change, Time Service - Automatic / Manual, Two-way Record, Two-way Transfer, LCS, Voice Mail Transfer