SECTION 01025

MEASUREMENT AND PAYMENT

PART	GENERAL

SECTION INCLUDES

Measurement and payment criteria applicable to [portions of] the Work performed under a unit price payment method.

Defect assessment and non-payment for rejected work.

AUTHORITY

Measurement methods delineated in the individual specification sections are intended to complement the criteria of this section. [In the event of conflict, the requirements of the individual specification section shall govern.]

Take all measurements and compute quantities. The [Architect/Engineer] [Owner] will verify measurements and quantities.

****** [OR] ******

The [Architect/Engineer] [Owner] will take all measurements and compute quantities accordingly.

Assist by providing necessary equipment, workers, and survey personnel as required.

UNIT QUANTITIES SPECIFIED

Quantities and measurements indicated in the [Bid Form] [individual specification sections] [________] are for bidding and contract purposes only. Quantities and measurements supplied or placed in the Work and verified by the [Architect/Engineer] [Owner] shall determine payment.

If the actual Work requires more or fewer quantities than those quantities indicated, provide the required quantities at the unit sum/prices contracted.

MEASUREMENT OF QUANTITIES

Measurement Devices:

Weigh Scales: Inspected, tested and certified by the applicable [state] [________] Weights and Measures department within the past [year.] [________.]

Platform Scales: Of sufficient size and capacity to accommodate the conveying vehicle.

Metering Devices: Inspected, tested and certified by the applicable [State] [________] department within the past [year.] [________.]

Measurement by Weight: Concrete reinforcing steel, rolled or formed steel or other metal shapes will be measured by handbook weights. Welded assemblies will be measured by handbook or scale weight.

Measurement by Volume: Measured by cubic dimension using mean length, width and height or thickness.

Measurement by Area: Measured by square dimension using mean length and width or radius.

Linear Measurement: Measured by linear dimension, at the item centerline or mean chord.

Stipulated Sum/Price Measurement: Items measured by weight, volume, area, or linear means or combination, as appropriate, as a completed item or unit of the Work.

PAYMENT

Payment Includes: Full compensation for all required labor, Products, tools, equipment, plant, transportation, services and incidentals; erection, application or installation of an item of the Work; overhead and profit.

Final payment for Work governed by unit prices will be made on the basis of the actual measurements and quantities accepted by the Architect/Engineer multiplied by the unit sum/price for Work which is incorporated in or made necessary by the Work.

DEFECT ASSESSMENT

Replace the Work, or portions of the Work, not conforming to specified requirements.

If, in the opinion of the [Architect/Engineer] [Owner] [________], it is not practical to remove and replace the Work, the [Architect/Engineer] [Owner] [________] will direct one of the following remedies:

The defective Work may remain, but the unit sum/price will be [adjusted to a new sum/price] [reduced [50] [____] percent] at the discretion of the [Architect/Engineer.] [Owner.]

The defective Work will be partially repaired to the instructions of the [Architect/Engineer] [Owner] [________], and the unit sum/price will be [adjusted to a new sum/price] [reduced [50] [____] percent] at the discretion of the [Architect/Engineer.] [Owner.] [________.]

The individual specification sections may modify these options or may identify a specific formula or percentage sum/price reduction.

[The authority of the [Architect/Engineer] [Owner] [________] to assess the defect and identify payment adjustment, is final.]

NON-PAYMENT FOR REJECTED PRODUCTS

Payment will not be made for any of the following:

Products wasted or disposed of in a manner that is not acceptable.

Products determined as unacceptable before or after placement.

Products not completely unloaded from the transporting vehicle.

Products placed beyond the lines and levels of the required Work.

Products remaining on hand after completion of the Work.

Loading, hauling and disposing of rejected Products.

PART	PRODUCTS

Not Used

PART	EXECUTION

Not Used

END OF SECTION