SECTION 01560

TEMPORARY CONTROLS

PART 1 GENERAL

SECTION INCLUDES

Water Control.

Dust Control.

Erosion and Sediment Control.

Noise Control.

Pest Control.

Pollution Control.

Rodent Control.

RELATED SECTIONS

Section [01010 - Summary of Work] [01011 - Summary of Project]: [Contractor use of premises] [Owner occupancy] [Maintenance of operations].

Section [01039 - Coordination and Meetings] [01041 -Project Coordination]: Project coordination.

Section 01500 - Construction Facilities and Temporary Controls: [Temporary water control] [Construction cleaning] [Traffic regulation].

WATER CONTROL

Grade site to drain.	Maintain excavations free of water. Provide, operate, and maintain pumping equipment.

Protect site from puddling or running water.	[Provide water barriers as required to protect site from [soil erosion] [____________________].]

DUST CONTROL

Execute Work by methods to minimize raising dust from construction operations.

Provide positive means to prevent air-borne dust from dispersing into atmosphere.

EROSION AND SEDIMENT CONTROL

Plan and execute construction by methods to control surface drainage from cuts and fills, from borrow and waste disposal areas. Prevent erosion and sedimentation.

Minimize amount of bare soil exposed at one time.

Provide temporary measures such as berms, dikes, and drains, to prevent water flow.

Construct fill and waste areas by selective placement to avoid erosive surface silts or clays.

Periodically inspect earthwork to detect evidence of erosion and sedimentation; promptly apply corrective measures.

NOISE CONTROL

PEST CONTROL

POLLUTION CONTROL

Provide methods, means, and facilities to prevent contamination of soil, water, and atmosphere from discharge of noxious, toxic substances, and pollutants produced by construction operations.

RODENT CONTROL

PART 2 PRODUCTS

Not Used

PART 3 EXECUTION

Not Used

END OF SECTION