SECTION 02060

BUILDING DEMOLITION

PART 1 GENERAL

SECTION INCLUDES

Demolition of designated structures [and removal of materials from site].

Demolition and removal of foundations [and slabs-on-grade].

Disconnecting and [capping] [removal] of identified utilities.

[Filling] [Removal] of underground tanks and piping.

Refer to items [as scheduled at end of section] [as indicated].

RELATED SECTIONS

Section 01019 - Contract Considerations:	Requirements applicable to unit prices for the work of this Section.

****** [OR] ******

Section 01025 - Measurement and Payment:	Requirements applicable to unit prices for the work of this section.

Section [01039 - Coordination and Meetings] [01120 -Alteration Project Procedures]: Re-installation of

removed [components.] [materials.]

Section 01500 - Construction Facilities and Temporary Controls: [Barriers, fences and landscape protection.] [Dust control.]

Section 01600 - Material and Equipment.

Section 01700 - Contract Closeout: Project record documents.

Section 02072 - Minor Demolition for Remodelling.

Section 02110 - Site Clearing: Clearing outside periphery of structures.

Section [02205 - Soil Materials] [02207 - Aggregate Materials]: Backfill materials.

UNIT PRICE - MEASUREMENT AND PAYMENT

Demolished Materials:

Basis of Measurement: By the [cubic [yard] [foot] (cubic meter)] [truck load].

Basis of Payment: Includes demolition, loading, removal from site.

To Remove Relics, Antiques, and Similar Objects Remaining the Property of the Owner:

Basis of Measurement: By the [unit] [weight] [________].

Basis of Payment: Includes removal, loading, and transporting to [designated location] [________].

To Remove and Store Materials and Equipment for Re-installation:

Basis of Measurement: By the [unit] [weight] [________].

Basis of Payment: Includes removal, loading, and transporting to [designated location] [________].

SUBMITTALS

Submit under provisions of Section [01300.] [________.]

Shop Drawings: Indicate [demolition] [and] [removal sequence and location of salvageable items]; location and construction of [barricades] [, fences] [and] [temporary work].

PROJECT RECORD DOCUMENTS

Submit under provisions of Section [01700.] [________.]

Accurately record actual locations of capped utilities, subsurface obstructions, and [________________].

QUALIFICATIONS

Demolition Firm:	Company specializing in performing the Work of this Section with minimum [________] years [documented] experience.

REGULATORY REQUIREMENTS

Conform to [applicable] [________] code for demolition of structures, safety of adjacent structures, dust control [, runoff control] [, disposal] and [________].

Obtain required permits from authorities.

Notify affected utility companies before starting work and comply with their requirements.

Do not close or obstruct [roadways] [sidewalks] [hydrants] without permits.

Conform to applicable regulatory procedures when discovering hazardous or contaminated materials.

Test soils around buried tanks for contamination.

SEQUENCING

Sequence work under the provisions of Section [01010.] [________.]

Sequence activities to demolish the Work in the following [order] [stages]:

[________________].

[________________].

[________________].

SCHEDULING

Schedule work under the provisions of Section [01300.] [01310.] [01311.] [________.]

Schedule Work to [precede] [coincide with] [site excavation work] [new construction] [________________].

Describe demolition removal procedures and schedule.

[Perform work between the hours of [____] and [____].]

PART 2 PRODUCTS

FILL MATERIALS

Fill Material: Type [____] fill, specified in Section [02205] [02207] [________].

PART 3 EXECUTION

PREPARATION

Provide, erect, and maintain temporary barriers and security devices [at locations indicated].

Protect existing [landscaping materials] [, appurtenances] [, structures] and [________________] which are not to be demolished.

Prevent movement or settlement of adjacent structures. Provide bracing and shoring.

Mark location of utilities.

DEMOLITION REQUIREMENTS

Conduct demolition to minimize interference with adjacent [structures.] [occupancies.] [________.]

Cease operations immediately if adjacent structures appear to be in danger. Notify [authority having jurisdiction] [Architect/Engineer]. Do not resume operations until directed.

Conduct operations with minimum interference to public or private accesses. Maintain [protected] egress and access at all times.

Obtain written permission from adjacent property owners when demolition equipment will traverse, infringe upon or limit access to their property.

Sprinkle Work with water to minimize dust. Provide hoses and water connections for this purpose.

DEMOLITION

Disconnect [remove] and cap [and identify] designated utilities within demolition areas.

Remove foundation walls and footings to a minimum of [two] [____] feet (600 [____] mm) below finished grade [beyond area of new construction] [within area of new construction].

Remove concrete slabs on grade.

****** [OR] ******

Break up concrete slabs on grade to permit natural moisture drainage.

Empty buried tanks located within demolition area. [Remove buried tanks, components, and piping from site] [Fill tanks with sand or fine gravel and cover with fill, remove piping].

Remove materials to be re-installed or retained in manner to prevent damage. Store and protect in accordance with requirements of Section [01600.] [________.]

Backfill [areas excavated] [open pits and holes] caused as a result of demolition [, in accordance with Section [02223] [________]].

Rough grade and compact areas affected by demolition to [maintain site grades and contours] [________________].

Remove demolished materials from site.

Do not burn or bury materials on site. Leave site in clean condition.

[Remove temporary work.]

SCHEDULES

Relics, antiques, and similar objects remain the property of Owner. Obtain direction regarding method of removal. Items [may] include:

[________________________________________________].

[________________________________________________].

[________________________________________________].

Items to be removed, stored, and protected for re-installation:

[________________________________________________].

[________________________________________________].

[________________________________________________].

Items to be removed and be retained by Owner; deliver to [location designated by Architect/Engineer] [________].

[________________________________________________].

[________________________________________________].

[________________________________________________].

Items to be removed and kept by the Owner:

[________________________________________________].

[________________________________________________].

[________________________________________________].

Items to be protected:

[________________________________________________].

[________________________________________________].

[________________________________________________].

END OF SECTION