SECTION 11600

LABORATORY EQUIPMENT

PART 1 GENERAL

SECTION INCLUDES

Laboratory equipment.

[Connection to utilities.]

[Service fittings and outlets.]

PRODUCTS FURNISHED BUT NOT INSTALLED UNDER THIS SECTION

Section [______-____________]: Templates for placement of [weigh scale] [________] equipment anchors.

Section [_____-__________]: Placement of [rough-in frames] [anchors] [concealed [above ceiling] [wall] structural attachments] [and] [________].

Section [______-____________]: Placement of counter top [and reagent shelf] plumbing service fittings.

Section [______-____________]: Placement of counter top [and reagent shelf] electrical service outlets.

PRODUCTS INSTALLED BUT NOT FURNISHED UNDER THIS SECTION

Section 01010 - Summary of Work:	Owner furnished laboratory furnishings for installation by this section.

Section [_____-__________]: Supply of laboratory equipment service fittings for placement by this section.

RELATED SECTIONS

Section [_____-__________]: Placement of anchors bolts and inserts.

Section 03300 - Cast-in-Place Concrete: Concrete equipment pads and bases for [________] equipment.

Section [______-____________]: Base finish to [________] equipment.

Section 09900 - Painting: Field painting of exposed metal frame.

Section 12301 - Metal Casework.

Section 15410 - Plumbing Piping:	Domestic water supply to [________] equipment.

Section 15410 - Plumbing Piping:	Natural gas supply to [________] equipment.

Section 15520 - Steam and Steam Condensate Piping: Steam supply to [________] equipment.

Section 15410 - Plumbing Piping:	Compressed air supply to [________] equipment.

Section 15430 - Plumbing Specialties: Floor [funnel] drain.

Section 15440 - Plumbing Fixtures: Sinks for [________] equipment.

Section 16180 - Equipment Wiring Systems: [Conduit and] electrical power to [________] equipment.

Section 16721 - Fire Alarm and Smoke Detection Systems: Fire and smoke detection devices to be installed in [________] laboratory equipment.

ALLOWANCES

Cash Allowance: Include under provisions of Section [01019.] [________.]

Allowance includes purchase and delivery of [particular] scheduled laboratory equipment. Installation is included

in this section and is part of the Contract Sum/Price.

****** [OR] ******

Allowance includes purchase, delivery, and installation of [particular] scheduled laboratory equipment.

REFERENCES

[________].

SUBMITTALS

Submit under provisions of Section [01300.] [________.]

Shop Drawings: Indicate equipment locations, large scale plans, elevations, cross sections, rough-in and anchor placement dimensions and tolerances, clearances required and [________].

Product Data: Provide equipment dimensions and construction, equipment capacities, physical dimensions, utility and service requirements and locations, point loads and [________].

Samples:	Submit [two] [_______] samples of exposed finish surfaces, [____x____] inch ([____x____] mm) in size illustrating color and finish.

Manufacturer's Installation Instructions: Indicate special installation requirements and [________].

Manufacturer's Certificate: Certify that [Products] [________] meet or exceed [specified requirements] [___________________].

PROJECT RECORD DOCUMENTS

Submit under provisions of Section [01700.] [________.]

Record actual locations of concealed utility connections and [________].

OPERATION AND MAINTENANCE DATA

Submit under provisions of Section [01700.] [________.]

Operation Data: Include description of equipment operation, adjusting and testing required.

Maintenance Data: Identify system maintenance requirements, servicing cycles, lubrication types required and [local] spare part sources.

QUALIFICATIONS

Manufacturer: Company specializing in manufacturing the Products specified in this section with minimum [three]

[_______] years [documented] experience.

REGULATORY REQUIREMENTS

Conform to [applicable] [___________] code for [________] equipment.

Conform to [UL] [NFPA] [________] requirements for fabrication and installation of [________] equipment.

Provide certificate of compliance from [authority having jurisdiction] [________________] indicating approval of

PRE-INSTALLATION CONFERENCE

Convene [one] [_____] week prior to commencing work of this section, under provisions of Section [01039.] [________.]

DELIVERY, STORAGE, AND HANDLING

Deliver, store, protect and handle products to site under provisions of Section [01600.] [________.]

Accept [________] equipment on site.	Inspect on arrival for damage.

Leave building openings of sufficient size to permit transport of unit to final position.

FIELD MEASUREMENTS

Verify that field measurements are as [indicated [on shop drawings].] [instructed by the manufacturer.]

COORDINATION

Coordinate work under provisions of Section [01039.] [________.]

Coordinate equipment installation with size, location and installation of service utilities.

WARRANTY

Provide [five] [____] year warranty under provisions of Section [01700.] [________.]

Warranty: Include coverage for [refrigeration equipment contained with [________] equipment.] [________.]

PART 2 PRODUCTS

COMPONENTS

Equipment:	Scheduled at end of section.

Rough-in: Frames, anchors, supports, accessories and closure trim; appropriate to scheduled equipment.

SHOP FINISHING

Concealed Frame of [________] Equipment:	[Galvanized] [Baked primer] [________].

[________] Equipment and Accessories: [Zinc chromate] [________] primer; two [baked] enamel finish coats to [________] color [as selected].

SOURCE QUALITY CONTROL AND TESTS

Provide testing of [________] under provisions of Section [01400.] [________.]

Provide shop [inspection] [and] [testing] for [________] equipment items.

PART 3 EXECUTION

EXAMINATION

Verify equipment rough-in under provisions of Section [01039.] [________.]

Verify that rough-in frames, anchors and supports are accurately placed.

PREPARATION

Provide [rough-in frame and] anchors for placement by Section [03100.] [________.]

INSTALLATION

Install in accordance with manufacturer's instructions.

Install in accordance with standards required by authority having jurisdiction.

Anchor equipment securely in place.

Sequence installation to ensure utility connections are achieved in an orderly and expeditious manner.

Touch-up minor damaged surfaces caused during installation. Replace damaged components as directed by Architect/Engineer.

INTERFACE WITH OTHER PRODUCTS

Coordinate installation of [________] with [________].

MANUFACTURER'S FIELD SERVICES

Prepare and start equipment under provisions of Section [01400.] [________.]

ADJUSTING

Adjust work under provisions of Section [01700.] [________.]

Adjust operating equipment to efficient operation.

DEMONSTRATION

Provide systems demonstration under provisions of Section [01650.] [________.]

Demonstrate equipment operation and [________].

SCHEDULES

FUME HOOD

Manufacturers:

[_____________________________] Model [________].

[_____________________________] Model [________].

[_____________________________] Model [________].

Features: Stainless steel cabinet interior, baked enamel cabinet exterior, stone work top surface, sliding framed glass sash, 75 CFM exhaust through open sash, adjustable cement-asbestos baffles, 100 w incandescent lamp in vapor tight light fixture.

Working Surface of Fume Hood: Capable of supporting 75 psi live load.

[________] EQUIPMENT

Manufacturers:

[_____________________________] Model [________].

[_____________________________] Model [________].

[_____________________________] Model [________].

Features: [________].

Working Surface of [________] Equipment:	Capable of supporting [[____] lbs ([____] Kg) static load.] [[____] psi ([____] KPa) live load.]

END OF SECTION